Spoke2#term len 0
Spoke2#sh run
Building configuration...

Current configuration : 1744 bytes
!
upgrade fpd auto
version 12.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname Spoke2
!
boot-start-marker
boot-end-marker
!
logging message-counter syslog
!
no aaa new-model
ip source-route
ip cef
!
!
!
!
no ip domain lookup
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
archive
 log config
  hidekeys
! 
!
crypto isakmp policy 10
 authentication pre-share
crypto isakmp key cisco address 0.0.0.0 0.0.0.0
!
!
crypto ipsec transform-set TRA esp-aes esp-sha-hmac 
!
crypto ipsec profile PRO
 set transform-set TRA 
!
!
!
!
!
!
!
!
interface Tunnel0
 bandwidth 8000
 ip address 172.16.1.102 255.255.255.0
 no ip redirects
 ip nhrp map multicast 10.0.0.1
 ip nhrp map 172.16.1.1 10.0.0.1
 ip nhrp network-id 1
 ip nhrp nhs 172.16.1.1
 ipv6 address 2001:DB8::102/64
 ipv6 eigrp 101
 ipv6 nhrp map 2001:DB8::1/128 10.0.0.1
 ipv6 nhrp map multicast 10.0.0.1
 ipv6 nhrp network-id 101
 ipv6 nhrp nhs 2001:DB8::1
 tunnel source FastEthernet0/0
 tunnel mode gre multipoint
 tunnel protection ipsec profile PRO
!
interface FastEthernet0/0
 ip address 10.0.0.102 255.255.255.0
 duplex auto
 speed auto
!
interface FastEthernet0/1
 ip address 192.168.102.1 255.255.255.0
 duplex auto
 speed auto
 ipv6 address 2001:DB8:102::/64 eui-64
 ipv6 eigrp 101
!
router eigrp 1
 passive-interface FastEthernet0/0
 network 0.0.0.0
 no auto-summary
!
ip forward-protocol nd
no ip http server
no ip http secure-server
!
!
!
logging alarm informational
ipv6 router eigrp 101
 no shutdown
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
!
gatekeeper
 shutdown
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 login
!
end

Spoke2#sh ip rute
              ^
% Invalid input detected at '^' marker.

Spoke2#sh ip route
Codes: C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area 
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route

Gateway of last resort is not set

     172.16.0.0/24 is subnetted, 1 subnets
C       172.16.1.0 is directly connected, Tunnel0
     10.0.0.0/24 is subnetted, 1 subnets
C       10.0.0.0 is directly connected, FastEthernet0/0
D    192.168.0.0/24 [90/1602560] via 172.16.1.1, 00:02:33, Tunnel0
C    192.168.102.0/24 is directly connected, FastEthernet0/1
D    192.168.101.0/24 [90/2882560] via 172.16.1.101, 00:02:19, Tunnel0
Spoke2#sh ipv6 route
IPv6 Routing Table - Default - 7 entries
Codes: C - Connected, L - Local, S - Static, U - Per-user Static route
       B - BGP, M - MIPv6, R - RIP, I1 - ISIS L1
       I2 - ISIS L2, IA - ISIS interarea, IS - ISIS summary, D - EIGRP
       EX - EIGRP external
       O - OSPF Intra, OI - OSPF Inter, OE1 - OSPF ext 1, OE2 - OSPF ext 2
       ON1 - OSPF NSSA ext 1, ON2 - OSPF NSSA ext 2
C   2001:DB8::/64 [0/0]
     via Tunnel0, directly connected
L   2001:DB8::102/128 [0/0]
     via Tunnel0, receive
D   2001:DB8:100::/64 [90/1602560]
     via FE80::C800:3FF:FE2E:8, Tunnel0
D   2001:DB8:101::/64 [90/2882560]
     via FE80::C801:3FF:FE2E:8, Tunnel0
C   2001:DB8:102::/64 [0/0]
     via FastEthernet0/1, directly connected
L   2001:DB8:102:0:C802:3FF:FE2E:6/128 [0/0]
     via FastEthernet0/1, receive
L   FF00::/8 [0/0]
     via Null0, receive