RT1

NWBB_T12-60-RT1#sh ip route
Codes: C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route

Gateway of last resort is 0.0.0.0 to network 0.0.0.0

     192.168.10.0/28 is subnetted, 1 subnets
C       192.168.10.32 is directly connected, Vlan190
     172.20.0.0/16 is variably subnetted, 5 subnets, 2 masks
C       172.20.20.12/30 is directly connected, Tunnel0
D       172.20.20.8/30 [90/310044416] via 172.20.20.13, 01:26:23, Tunnel0
D       172.20.20.0/30 [90/310044416] via 172.20.20.13, 01:26:23, Tunnel0
D       172.20.21.0/24 [90/297246976] via 172.20.20.13, 01:26:23, Tunnel0
D       172.20.20.16/30 [90/540446976] via 192.168.10.35, 01:26:13, Vlan190
     195.219.82.0/29 is subnetted, 1 subnets
D       195.219.82.96 [90/297247232] via 172.20.20.13, 01:26:23, Tunnel0
     24.0.0.0/29 is subnetted, 1 subnets
R       24.142.114.0 [120/2] via 192.168.10.39, 00:00:23, Vlan190
     10.0.0.0/8 is variably subnetted, 2 subnets, 2 masks
C       10.10.9.0/24 is directly connected, Vlan12
R       10.8.13.1/32 [120/2] via 192.168.10.39, 00:00:25, Vlan190
     192.168.0.0/29 is subnetted, 1 subnets
D       192.168.0.16 [90/297249536] via 172.20.20.13, 01:26:24, Tunnel0
     209.239.70.0/28 is subnetted, 1 subnets
C       209.239.70.16 is directly connected, FastEthernet0/0
S*   0.0.0.0/0 is directly connected, FastEthernet0/0

NWBB_T12-60-RT1#sh ip route static
S*   0.0.0.0/0 is directly connected, FastEthernet0/0

NWBB_T12-60-RT1#sh ip eigrp int
IP-EIGRP interfaces for process 65000

                        Xmit Queue   Mean   Pacing Time   Multicast    Pending
Interface        Peers  Un/Reliable  SRTT   Un/Reliable   Flow Timer   Routes
Vl12               1        0/0         1       0/1           50           0
Tu0                1        0/0       194      71/2702    3630        0
Vl190              1        0/0         1       0/1           50           0

NWBB_T12-60-RT1#sh ip eigrp top
IP-EIGRP Topology Table for AS(65000)/ID(209.239.70.19)

Codes: P - Passive, A - Active, U - Update, Q - Query, R - Reply,
       r - reply Status, s - sia Status

P 10.10.9.0/24, 1 successors, FD is 256025600
        via Connected, Vlan12
P 10.8.13.1/32, 1 successors, FD is 281600
        via Redistributed (281600/0)
P 195.219.82.96/29, 1 successors, FD is 297247232
        via 172.20.20.13 (297247232/28416), Tunnel0
P 192.168.10.32/28, 1 successors, FD is 28160
        via Connected, Vlan190
P 192.168.0.16/29, 1 successors, FD is 297249536
        via 172.20.20.13 (297249536/30720), Tunnel0
P 172.20.20.12/30, 1 successors, FD is 297244416
        via Connected, Tunnel0
P 172.20.20.8/30, 1 successors, FD is 310044416
        via 172.20.20.13 (310044416/297244416), Tunnel0
P 172.20.20.0/30, 1 successors, FD is 310044416
        via 172.20.20.13 (310044416/297244416), Tunnel0
P 172.20.21.0/24, 1 successors, FD is 297246976
        via 172.20.20.13 (297246976/28160), Tunnel0
P 172.20.20.16/30, 1 successors, FD is 540446976
        via 192.168.10.35 (540446976/540444416), Vlan190, serno 662
        via 172.20.20.13 (553244416/540444416), Tunnel0
        via 10.10.9.3 (796444416/540444416), Vlan12
P 24.142.114.0/29, 1 successors, FD is 281600
        via Redistributed (281600/0)
NWBB_T12-60-RT1#

                 RT2

NWBB_T12-60-RT2#sh ip route
Codes: C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route

Gateway of last resort is 0.0.0.0 to network 0.0.0.0

     192.168.10.0/28 is subnetted, 1 subnets
C       192.168.10.32 is directly connected, Vlan190
     172.20.0.0/16 is variably subnetted, 5 subnets, 2 masks
D       172.20.20.12/30 [90/297246976] via 192.168.10.34, 01:32:34, Vlan190
D       172.20.20.8/30 [90/310046976] via 192.168.10.34, 01:32:34, Vlan190
D       172.20.20.0/30 [90/310046976] via 192.168.10.34, 01:32:34, Vlan190
D       172.20.21.0/24 [90/297249536] via 192.168.10.34, 01:32:34, Vlan190
C       172.20.20.16/30 is directly connected, Tunnel0
     195.219.82.0/29 is subnetted, 1 subnets
D       195.219.82.96 [90/297249792] via 192.168.10.34, 01:32:34, Vlan190
     24.0.0.0/29 is subnetted, 1 subnets
R       24.142.114.0 [120/2] via 192.168.10.39, 00:00:23, Vlan190
     10.0.0.0/8 is variably subnetted, 2 subnets, 2 masks
C       10.10.9.0/24 is directly connected, Vlan12
R       10.8.13.1/32 [120/2] via 192.168.10.39, 00:00:24, Vlan190
     192.168.0.0/29 is subnetted, 1 subnets
D       192.168.0.16 [90/297252096] via 192.168.10.34, 01:32:36, Vlan190
     209.239.70.0/28 is subnetted, 1 subnets
C       209.239.70.16 is directly connected, FastEthernet0/0
S*   0.0.0.0/0 is directly connected, FastEthernet0/0

NWBB_T12-60-RT2#sh ip route static
S*   0.0.0.0/0 is directly connected, FastEthernet0/0

NWBB_T12-60-RT2#sh ip eigrp int
IP-EIGRP interfaces for process 65000

                        Xmit Queue   Mean   Pacing Time   Multicast    Pending
Interface        Peers  Un/Reliable  SRTT   Un/Reliable   Flow Timer   Routes
Vl12               1        0/0         1       0/1           50           0
Tu0                1        0/0       259      71/2702    3914         0
Vl190              1        0/0        59       0/1          236           0

NWBB_T12-60-RT2#sh ip eigrp top
IP-EIGRP Topology Table for AS(65000)/ID(209.239.70.20)

Codes: P - Passive, A - Active, U - Update, Q - Query, R - Reply,
       r - reply Status, s - sia Status

P 10.10.9.0/24, 1 successors, FD is 256025600
        via Connected, Vlan12
P 10.8.13.1/32, 1 successors, FD is 281600
        via Redistributed (281600/0)
P 195.219.82.96/29, 1 successors, FD is 297249792
        via 192.168.10.34 (297249792/297247232), Vlan190
        via 172.20.20.17 (540447232/28416), Tunnel0
        via 10.10.9.2 (553247232/297247232), Vlan12
P 192.168.10.32/28, 1 successors, FD is 28160
        via Connected, Vlan190
P 192.168.0.16/29, 1 successors, FD is 297252096
        via 192.168.10.34 (297252096/297249536), Vlan190
        via 172.20.20.17 (540449536/30720), Tunnel0
        via 10.10.9.2 (553249536/297249536), Vlan12
P 172.20.20.12/30, 1 successors, FD is 297246976
        via 192.168.10.34 (297246976/297244416), Vlan190
        via 172.20.20.17 (553244416/297244416), Tunnel0
        via 10.10.9.2 (553244416/297244416), Vlan12
P 172.20.20.8/30, 1 successors, FD is 310046976
        via 192.168.10.34 (310046976/310044416), Vlan190
        via 172.20.20.17 (553244416/297244416), Tunnel0
        via 10.10.9.2 (566044416/310044416), Vlan12
P 172.20.20.0/30, 1 successors, FD is 310046976
        via 192.168.10.34 (310046976/310044416), Vlan190
        via 172.20.20.17 (553244416/297244416), Tunnel0
        via 10.10.9.2 (566044416/310044416), Vlan12
P 172.20.21.0/24, 1 successors, FD is 297249536
        via 192.168.10.34 (297249536/297246976), Vlan190
        via 172.20.20.17 (540446976/28160), Tunnel0
        via 10.10.9.2 (553246976/297246976), Vlan12
P 172.20.20.16/30, 1 successors, FD is 540444416
        via Connected, Tunnel0
P 24.142.114.0/29, 1 successors, FD is 281600
        via Redistributed (281600/0)
NWBB_T12-60-RT2#

                Hub

newwave_vpn#sh ip route
Codes: C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route

Gateway of last resort is 172.20.21.2 to network 0.0.0.0

     192.168.10.0/28 is subnetted, 1 subnets
D       192.168.10.32 [90/297246976] via 172.20.20.14, 01:36:20, Tunnel2
     172.20.0.0/16 is variably subnetted, 5 subnets, 2 masks
C       172.20.20.12/30 is directly connected, Tunnel2
C       172.20.20.8/30 is directly connected, Tunnel1
C       172.20.20.0/30 is directly connected, Tunnel0
C       172.20.21.0/24 is directly connected, FastEthernet0/0
C       172.20.20.16/30 is directly connected, Tunnel3
     195.219.82.0/24 is variably subnetted, 4 subnets, 2 masks
C       195.219.82.108/30 is directly connected, FastEthernet0/1.2
D       195.219.82.96/29 [90/28416] via 172.20.21.2, 01:36:20, FastEthernet0/0
C       195.219.82.120/30 is directly connected, FastEthernet0/1.7
C       195.219.82.112/30 is directly connected, FastEthernet0/1.4
     24.0.0.0/29 is subnetted, 1 subnets
D EX    24.142.114.0 [170/297270016] via 172.20.20.14, 00:09:40, Tunnel2
     10.0.0.0/8 is variably subnetted, 5 subnets, 2 masks
S       10.1.9.0/24 [1/0] via 172.20.20.2
D       10.10.9.0/24 [90/553244416] via 172.20.20.14, 01:36:22, Tunnel2
D EX    10.8.13.1/32 [170/297270016] via 172.20.20.14, 00:09:40, Tunnel2
S       10.8.12.0/24 [95/0] via 172.20.20.2
S       10.8.13.0/24 [95/0] via 172.20.20.14
     217.10.164.0/32 is subnetted, 2 subnets
S       217.10.164.35 is directly connected, FastEthernet0/1.4
S       217.10.164.34 is directly connected, FastEthernet0/1.2
     78.0.0.0/23 is subnetted, 1 subnets
S       78.40.64.0 [95/0] via 172.20.20.2
     192.168.0.0/24 is variably subnetted, 2 subnets, 2 masks
S       192.168.0.32/28 [1/0] via 172.20.20.2
D       192.168.0.16/29 [90/30720] via 172.20.21.2, 01:36:22, FastEthernet0/0
     209.239.70.0/32 is subnetted, 2 subnets
S       209.239.70.19 is directly connected, FastEthernet0/1.7
S       209.239.70.20 is directly connected, FastEthernet0/1.4
     192.168.3.0/30 is subnetted, 1 subnets
C       192.168.3.0 is directly connected, FastEthernet0/1.6
S*   0.0.0.0/0 [1/0] via 172.20.21.2

newwave_vpn#sh ip route static
     10.0.0.0/8 is variably subnetted, 5 subnets, 2 masks
S       10.1.9.0/24 [1/0] via 172.20.20.2
S       10.8.12.0/24 [95/0] via 172.20.20.2
S       10.8.13.0/24 [95/0] via 172.20.20.14
     217.10.164.0/32 is subnetted, 2 subnets
S       217.10.164.35 is directly connected, FastEthernet0/1.4
S       217.10.164.34 is directly connected, FastEthernet0/1.2
     78.0.0.0/23 is subnetted, 1 subnets
S       78.40.64.0 [95/0] via 172.20.20.2
     192.168.0.0/24 is variably subnetted, 2 subnets, 2 masks
S       192.168.0.32/28 [1/0] via 172.20.20.2
     209.239.70.0/32 is subnetted, 2 subnets
S       209.239.70.19 is directly connected, FastEthernet0/1.7
S       209.239.70.20 is directly connected, FastEthernet0/1.4
S*   0.0.0.0/0 [1/0] via 172.20.21.2

newwave_vpn#sh ip eigrp int
IP-EIGRP interfaces for process 65000

                        Xmit Queue   Mean   Pacing Time   Multicast    Pending
Interface        Peers  Un/Reliable  SRTT   Un/Reliable   Flow Timer   Routes
Fa0/0              1        0/0         1       0/1           50           0
Tu0                0        0/0         0      71/71           0           0
Tu1                0        0/0         0      71/71           0           0
Tu2                1        0/0       142      71/2702      3242           0
Tu3                1        0/0       252      71/2702      3794           0

newwave_vpn#sh ip eigrp top
IP-EIGRP Topology Table for AS(65000)/ID(195.219.82.122)

Codes: P - Passive, A - Active, U - Update, Q - Query, R - Reply,
       r - reply Status, s - sia Status

P 10.10.9.0/24, 1 successors, FD is 553244416
        via 172.20.20.14 (553244416/256025600), Tunnel2
        via 172.20.20.18 (796444416/256025600), Tunnel3
P 10.8.13.1/32, 1 successors, FD is 297270016
        via 172.20.20.14 (297270016/281600), Tunnel2
        via 172.20.20.18 (540470016/281600), Tunnel3
P 195.219.82.96/29, 1 successors, FD is 28416
        via 172.20.21.2 (28416/2816), FastEthernet0/0
P 192.168.10.32/28, 1 successors, FD is 297246976
        via 172.20.20.14 (297246976/28160), Tunnel2
        via 172.20.20.18 (540446976/28160), Tunnel3
P 192.168.0.16/29, 1 successors, FD is 30720
        via 172.20.21.2 (30720/28160), FastEthernet0/0
P 172.20.20.12/30, 1 successors, FD is 297244416
        via Connected, Tunnel2
P 172.20.20.8/30, 1 successors, FD is 297244416
        via Connected, Tunnel1
P 172.20.20.0/30, 1 successors, FD is 297244416
        via Connected, Tunnel0
P 172.20.21.0/24, 1 successors, FD is 28160
        via Connected, FastEthernet0/0
P 172.20.20.16/30, 1 successors, FD is 540444416
        via Connected, Tunnel3
P 24.142.114.0/29, 1 successors, FD is 297270016
        via 172.20.20.14 (297270016/281600), Tunnel2
        via 172.20.20.18 (540470016/281600), Tunnel3
newwave_vpn#