upgrade fpd auto
version 12.4
no service pad
service tcp-keepalives-in
service tcp-keepalives-out
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname XXXX1-PC1
!
boot-start-marker
boot-end-marker
!
logging message-counter syslog
logging buffered 6500
no logging console
logging monitor critical.
!
aaa new-model
!
!
aaa authentication login default local
!
!
aaa session-id common
no ip source-route
no ip gratuitous-arps
ip cef
!
!
ip vrf XXXX-0099
 description Management VRF
 rd 320:1111000099
 route-target export 320:1111000099
 route-target import 320:1111000099
!
!
!
no ip bootp server
no ip domain lookup
ip domain name test.lab
no ipv6 cef
!
multilink bundle-name authenticated
mpls traffic-eng tunnels
mpls ldp neighbor XXX.XXX.128.14 password 7 XXXXXXXXXXXXXXX
mpls ldp neighbor XXX.XXX.128.79 password 7 XXXXXXXXXXXXXXXX
mpls ldp neighbor XXX.XXX.128.55 password 7 XXXXXXXXXXXXXXXXX
mpls ldp session protection
mpls label protocol ldp
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!         
!
archive
 log config
  hidekeys
! 
!
!
!
!
ip tcp synwait-time 10
ip telnet hidden addresses
ip ssh time-out 60
!
class-map match-any TEST
 match mpls experimental topmost 0 
 match mpls experimental topmost 1 
 match mpls experimental topmost 2 
 match mpls experimental topmost 3 
 match mpls experimental topmost 4 
 match mpls experimental topmost 5 
 match mpls experimental topmost 6 
 match mpls experimental topmost 7 
!
!
policy-map TEST
 class TEST
!
!
!
!
!
interface Loopback0
 ip address XXX.XXX.128.15 255.255.255.255
!
interface Loopback99
 ip vrf forwarding XXXX-0099
 ip address XXX.XXX.132.133 255.255.255.255
!
interface Tunnel0
 description //Management//
 bandwidth 10000
 ip vrf forwarding XXXX-0099
 ip address 172.25.1.5 255.255.255.0
 no ip redirects
 no ip proxy-arp
 ip mtu 1289
 ip nhrp authentication bc
 ip nhrp map 172.25.1.1 172.24.2.34
 ip nhrp map multicast 172.24.2.34
 ip nhrp map 172.25.1.2 172.24.1.38
 ip nhrp map multicast 172.24.1.38
 ip nhrp network-id 1
 ip nhrp holdtime 600
 ip nhrp nhs 172.25.1.1
 ip nhrp nhs 172.25.1.2
 ip nhrp registration timeout 120
 ip tcp adjust-mss 1201
 ip ospf authentication message-digest
 ip ospf authentication-key 7   XXXXXX
 ip ospf network broadcast
 ip ospf priority 2
 tunnel source Loopback0
 tunnel mode gre multipoint
 tunnel key 1
!
interface Tunnel10
 description From XXXX1-PC1[P]->XXXX1-PC1[P]
 ip unnumbered Loopback0
 mpls ip
 tunnel destination XXX.XXX.128.55
 tunnel mode mpls traffic-eng
 tunnel mpls traffic-eng autoroute announce
 tunnel mpls traffic-eng priority 0 0
 tunnel mpls traffic-eng bandwidth 2000
 tunnel mpls traffic-eng path-option 10 dynamic
 tunnel mpls traffic-eng exp 5
 service-policy output TEST
 no routing dynamic
!
interface Tunnel20
 description From XXXX1-PC1[P]->XXXX1-PC1[P]_Default
 ip unnumbered Loopback0
 mpls ip
 tunnel destination XXX.XXX.128.55
 tunnel mode mpls traffic-eng
 tunnel mpls traffic-eng autoroute announce
 tunnel mpls traffic-eng priority 5 5
 tunnel mpls traffic-eng bandwidth 2000
 tunnel mpls traffic-eng path-option 10 dynamic
 tunnel mpls traffic-eng exp 0 1 2 3 4 6 7
 service-policy output TEST
 no routing dynamic
!
interface FastEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface FastEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface Ethernet1/0
 description //XXXX-PC1:100000//
 ip address 172.24.2.38 255.255.255.252
 no ip redirects
 no ip proxy-arp
 ip ospf authentication message-digest
 ip ospf authentication-key 7 XXXXXXXXXXXXXXXX
 duplex half
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth 7500
!
interface Ethernet1/1
 description //XXXX1-PC1:100000//
 ip address 172.24.1.33 255.255.255.252
 no ip redirects
 no ip proxy-arp
 ip ospf authentication message-digest
 ip ospf authentication-key 7 XXXXXXXXXXXXXXX
 duplex half
 mpls traffic-eng tunnels
 mpls ip
 service-policy output TEST
 ip rsvp bandwidth 7500
!
interface Ethernet1/2
 description //XXXX1-PE1:10000//
 ip address 172.24.1.37 255.255.255.252
 no ip redirects
 no ip proxy-arp
 ip ospf authentication message-digest
 ip ospf authentication-key 7 XXXXXXXXXXXX
 duplex half
 mpls ip
 service-policy input TEST
 ip rsvp bandwidth 7500
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex half
!
interface Ethernet1/4
 no ip address
 shutdown
 duplex half
!
interface Ethernet1/5
 no ip address
 shutdown
 duplex half
!
interface Ethernet1/6
 no ip address
 shutdown 
 duplex half
!
interface Ethernet1/7
 no ip address
 shutdown
 duplex half
!
router ospf 99 vrf XXXX-0099
 log-adjacency-changes
 area 0 authentication message-digest
 passive-interface default
 no passive-interface Tunnel0
 network 172.25.1.5 0.0.0.0 area 0
 network XXX.XXX.132.133 0.0.0.0 area 0
!
router ospf 320
 mpls traffic-eng router-id Loopback0
 mpls traffic-eng area 0
 router-id XXX.XXX.128.15
 log-adjacency-changes
 area 0 authentication message-digest
 passive-interface default
 no passive-interface Ethernet1/0
 no passive-interface Ethernet1/1
 no passive-interface Ethernet1/2
 network 172.24.1.33 0.0.0.0 area 0
 network 172.24.1.37 0.0.0.0 area 0
 network 172.24.2.38 0.0.0.0 area 0
 network XXX.XXX.128.15 0.0.0.0 area 0
!
ip forward-protocol nd
no ip http server
no ip http secure-server
!
!
!
!
!
!
!
!
mpls ldp router-id Loopback0
!
control-plane
!
!         
!
!
!
!
!
gatekeeper
 shutdown
!

!
line con 0
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 session-timeout 10 
 logging synchronous
 transport input ssh
 transport output ssh
line vty 5 15
 session-timeout 10 
 logging synchronous
 transport input ssh
 transport output ssh
!
end