Current configuration : 17460 bytes
!
! Last configuration change at 01:59:18 UTC Thu May 30 2013 by wsc
version 15.3
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname Hayden2911
!
boot-start-marker
boot system flash:c2900-universalk9-mz.SPA.153-2.T.bin
boot-end-marker
!
!
card type t1 0 0
logging buffered 20000000
!
no aaa new-model
network-clock-participate wic 0 
!
ip cef
!
!
!
!
!
!
ip domain name XXXXXXX.net
ip name-server 10.0.11.52
ip name-server 10.0.1.39
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
isdn switch-type primary-dms100
!
!
crypto pki trustpoint TP-self-signed-1454265054
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1454265054
 revocation-check none
 rsakeypair TP-self-signed-1454265054
!
crypto pki trustpoint godaddy.trustpoint
 enrollment terminal
 fqdn cube.XXXXXXX.net
 subject-name CN=cube.XXXXXXX.net,OU=IT,O=Deangelo Brothers Inc,C=US,ST=Pennsylvania
 chain-validation continue godaddy.root
 revocation-check crl
 rsakeypair GDkey
!
crypto pki trustpoint godaddy.root
 enrollment terminal
 revocation-check none
!
crypto pki trustpoint geotrust
 enrollment terminal pem
 revocation-check none
!
!
crypto pki certificate chain TP-self-signed-1454265054
 certificate self-signed 01
  	quit
crypto pki certificate chain godaddy.trustpoint
 certificate   	quit
 certificate ca   	quit
crypto pki certificate chain godaddy.root
 certificate ca 0
  	quit
crypto pki certificate chain geotrust
 certificate ca   	quit
voice-card 0
 dspfarm
 dsp services dspfarm
!
!
!
voice service voip
 ip address trusted list
  ipv4 0.0.0.0 0.0.0.0
 srtp fallback
 allow-connections h323 to h323
 allow-connections h323 to sip
 allow-connections sip to h323
 allow-connections sip to sip
 fax protocol t38 version 0 ls-redundancy 0 hs-redundancy 0 fallback none
 sip
  localhost dns:cube.XXXXXXX.net
!
voice class codec 1
 codec preference 1 g711ulaw
 codec preference 2 g729r8
!
!
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1548AJG9
license boot module c2900 technology-package securityk9
hw-module pvdm 0/0
!
hw-module pvdm 0/1
!
!
!
!
redundancy
!
!
!
!
!
controller T1 0/0/0
 fdl both
 cablelength long 0db
 pri-group timeslots 1-24 service mgcp
!
controller T1 0/0/1
 cablelength long 0db
!
ip ftp username cisco
ip ftp password cisco
! 
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 10.0.254.110 255.255.255.255
!
interface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 description $ETH-LAN$$ETH-SW-LAUNCH$$INTF-INFO-GE 0/0$
 ip address 10.0.10.5 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 ip address 24.229.88.66 255.255.255.240
 duplex auto
 speed auto
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface Serial0/0/0:23
 no ip address
 encapsulation hdlc
 isdn switch-type primary-ni
 isdn incoming-voice voice
 isdn bind-l3 ccm-manager
 isdn bchan-number-order ascending 
 no cdp enable
!
ip forward-protocol nd
!
ip http server
ip http access-class 23
ip http authentication local
ip http secure-server
ip http secure-trustpoint godaddy.trustpoint
ip http timeout-policy idle 60 life 86400 requests 10000
!
ip route 0.0.0.0 0.0.0.0 99.99.99.1
ip route 10.0.0.0 255.0.0.0 10.0.10.1
!
!
!
access-list 23 permit 10.10.10.0 0.0.0.7
access-list 23 permit any log
!
control-plane
!
!
voice-port 0/0/0:23
 !
 !
 !
!
ccm-manager redundant-host 10.0.100.12
ccm-manager mgcp
no ccm-manager fax protocol cisco
ccm-manager music-on-hold
ccm-manager config server 10.0.100.13  
ccm-manager config
!
mgcp
mgcp call-agent 10.0.100.13 2427 service-type mgcp version 0.1
mgcp dtmf-relay voip codec all mode out-of-band
mgcp rtp unreachable timeout 1000 action notify
mgcp modem passthrough voip mode nse
mgcp package-capability rtp-package
mgcp package-capability sst-package
mgcp package-capability pre-package
no mgcp package-capability res-package
no mgcp package-capability fxr-package
no mgcp timer receive-rtcp
mgcp sdp simple
mgcp fax t38 inhibit
mgcp bind control source-interface Loopback0
mgcp bind media source-interface Loopback0
mgcp behavior rsip-range tgcp-only
mgcp behavior comedia-role none
mgcp behavior comedia-check-media-src disable
mgcp behavior comedia-sdp-force disable
!
mgcp profile default
!         
sccp local GigabitEthernet0/0
sccp ccm 10.0.100.13 identifier 1 version 7.0 
!
dial-peer voice 500 pots
 service mgcpapp
 port 0/0/0:23
!
dial-peer voice 10 voip
 session protocol sipv2
 session target ipv4:10.0.100.13
 incoming called-number 1922
 dtmf-relay rtp-nte
 codec g711ulaw
!
dial-peer voice 1 voip
 destination-pattern 1922
 session protocol sipv2
 session target dns:XXXXXXX.um.outlook.com:5061
 session transport tcp tls
 voice-class sip url sips
 dtmf-relay rtp-nte
 srtp
 codec g711ulaw
 no vad
!
!
sip-ua 
 retry invite 10
 crypto signaling default trustpoint godaddy.trustpoint 
!
!
!
gatekeeper
 shutdown
!
!
!
line con 0
 login local
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport input all
 transport output pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 privilege level 15
 login local
 transport input telnet ssh
line vty 5 15
 privilege level 15
 login local
 transport input telnet ssh
!
scheduler allocate 20000 1000
!
end