version 15.1
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname hlsm-2821
!
boot-start-marker
boot-end-marker
!
!
enable password xxxxxxxx
!
aaa new-model
!
!
!
!
!
!
!
aaa session-id common
!
clock timezone est -5 0
clock summer-time est recurring
!
dot11 syslog
ip source-route
!
!
ip cef
!
ip dhcp excluded-address 172.20.100.1 172.20.100.99
ip dhcp excluded-address 172.20.100.200 172.20.100.254
!
ip dhcp pool voip
 network 172.20.100.0 255.255.255.0
 option 150 ip 172.20.100.10 
 default-router 172.20.100.1 
 dns-server 75.75.75.75 75.75.74.74 
!
!
ip domain lookup source-interface GigabitEthernet0/1
ip name-server 216.37.204.4
ip name-server 4.2.2.2
ip name-server 4.2.2.3
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
trunk group 1
 carrier-id Frontier
 description POTS telephone lines from Frontier Communications.
 hunt-scheme round-robin
!         
!
!
voice service voip
 ip address trusted list
  ipv4 172.20.100.0 255.255.255.0
  ipv4 208.73.146.0 255.255.255.0
  ipv4 208.73.144.0 255.255.255.0
  ipv4 10.0.10.0 255.255.255.0
 no ip address trusted authenticate
 allow-connections sip to sip
 sip
  e911
  registrar server expires max 3600 min 3600
  midcall-signaling passthru
!
!
voice register global
 mode cme
 source-address 172.20.100.10 port 5060
 max-dn 40
 max-pool 42
 authenticate register
 authenticate realm 172.20.100.10
 tftp-path flash:
 file text
 create profile sync 0000414354828629
!
voice register dn  1
 number 1111
 allow watch
 no-reg
!
voice register pool  1
 id mac 0000.0000.1111
 type ATA
 number 1 dn 1
 username 1111 password cisco
 codec g711ulaw
!
voice hunt-group 1 parallel
 final 1199
 list 1102,1103,1104,1105,1106,1109
 timeout 30 
 pilot 1180 
!
!
!
!
voice translation-rule 1
 rule 1 /.+/ /1191/
!
!
voice translation-profile 1
 translate called 1
!
!
voice-card 0
 dspfarm
 dsp services dspfarm
!
crypto pki token default removal timeout 0
!
!
!         
!
license udi pid CISCO2821 sn FHK1209F1Q6
username xxxxx password 0 xxxxxxxx
username xxxxxxx password 0 xxxxxxx 
username admin password 0 xxxxxxxxx 
!
redundancy
!
!
ip ssh time-out 60
ip ssh authentication-retries 2
! 
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 172.20.100.10 255.255.255.0
 ip route-cache same-interface
 duplex auto
 speed auto
!
interface Service-Engine0/1
 ip unnumbered GigabitEthernet0/0
 service-module ip address 172.20.100.20 255.255.255.0
 service-module ip default-gateway 172.20.100.10
!
interface GigabitEthernet0/1
 ip address dhcp
 ip route-cache same-interface
 duplex auto
 speed auto
!
interface Analysis-Module1/0
 ip unnumbered GigabitEthernet0/0
 hold-queue 60 out
!
ip forward-protocol nd
ip forward-protocol spanning-tree
ip http server
ip http authentication local
no ip http secure-server
ip http path flash:
!
!
ip route 10.0.10.0 255.255.255.0 172.20.100.1
ip route 172.16.0.0 255.255.255.0 172.20.100.1
ip route 172.20.100.20 255.255.255.255 Service-Engine0/1
ip route 192.168.10.0 255.255.255.0 172.20.100.1
!
!
!
!
!
!
tftp-server usbflash0:ringtones/RingList.xml alias RingList.xml
tftp-server usbflash0:ringtones/Analog2.raw alias Analog2.raw
tftp-server usbflash0:ringtones/AreYouThere.raw alias AreYouThere.raw
tftp-server usbflash0:ringtones/AreYouThereF.raw alias AreYouThereF.raw
tftp-server usbflash0:ringtones/Bass.raw alias Bass.raw
tftp-server usbflash0:ringtones/CallBack.raw alias CallBack.raw
tftp-server usbflash0:ringtones/Chime.raw alias Chime.raw
tftp-server usbflash0:ringtones/Classic1.raw alias Classic1.raw
tftp-server usbflash0:ringtones/Classic2.raw alias Classic2.raw
tftp-server usbflash0:ringtones/ClockShop.raw alias ClockShop.raw
tftp-server usbflash0:ringtones/Drums1.raw alias Drums1.raw
tftp-server usbflash0:ringtones/Drums2.raw alias Drums2.raw
tftp-server usbflash0:ringtones/FilmScore.raw alias FilmScore.raw
tftp-server usbflash0:ringtones/HarpSynth.raw alias HarpSynth.raw
tftp-server usbflash0:ringtones/Jamaica.raw alias Jamaica.raw
tftp-server usbflash0:ringtones/KotoEffect.raw alias KotoEffect.raw
tftp-server usbflash0:ringtones/MusicBox.raw alias MusicBox.raw
tftp-server usbflash0:ringtones/Piano1.raw alias Piano1.raw
tftp-server usbflash0:ringtones/Piano2.raw alias Piano2.raw
tftp-server usbflash0:ringtones/Pop.raw alias Pop.raw
tftp-server usbflash0:ringtones/Pulse1.raw alias Pulse1.raw
tftp-server usbflash0:ringtones/Ring1.raw alias Ring1.raw
tftp-server usbflash0:ringtones/Ring2.raw alias Ring2.raw
tftp-server usbflash0:ringtones/Ring3.raw alias Ring3.raw
tftp-server usbflash0:ringtones/Ring4.raw alias Ring4.raw
tftp-server usbflash0:ringtones/Ring5.raw alias Ring5.raw
tftp-server usbflash0:ringtones/Ring6.raw alias Ring6.raw
tftp-server usbflash0:ringtones/Ring7.raw alias Ring7.raw
tftp-server usbflash0:ringtones/Sax1.raw alias Sax1.raw
tftp-server usbflash0:ringtones/Sax2.raw alias Sax2.raw
tftp-server usbflash0:music-on-hold.au alias music-on-hold.au
tftp-server usbflash0:ringtones/DistinctiveRingList.xml alias DistinctiveRingList.xml
tftp-server usbflash0:Phones/9971/rootfs9971.9-1-1SR1.sebn alias rootfs9971.9-1-1SR1.sebn
tftp-server usbflash0:Phones/9971/sboot9971.031610R1-9-1-1SR1.sebn alias sboot9971.031610R1-9-1-1SR1.sebn
tftp-server usbflash0:Phones/9971/skern9971.022809R2-9-1-1SR1.sebn alias skern9971.022809R2-9-1-1SR1.sebn
tftp-server usbflash0:PHONES/7940/P00308010200.bin alias P00308010200.bin
tftp-server usbflash0:PHONES/7940/P00308010200.loads alias P00308010200.loads
tftp-server usbflash0:PHONES/7940/P00308010200.sb2 alias P00308010200.sb2
tftp-server usbflash0:PHONES/7940/P00308010200.sbn alias P00308010200.sbn
tftp-server usbflash0:ringtones/analog1.raw alias Analog1.raw
tftp-server usbflash0:PHONES/9971/sip9971.9-1-1SR1.loads alias sip9971.9-1-1SR1.loads
tftp-server usbflash0:PHONES/9971/dkern9971.100609R2-9-1-1SR1.sebn alias dkern9971.100609R2-9-1-1SR1.sebn
tftp-server usbflash0:PHONES/9971/kern9971.9-1-1SR1.sebn alias kern9971.9-1-1SR1.sebn
!
!
!
control-plane
!
!
voice-port 0/0/0
 mwi
 description FXS Port 0
 station-id number 1120
 caller-id enable
!
voice-port 0/0/1
!
!
no ccm-manager fax protocol cisco
!
no mgcp package-capability res-package
no mgcp package-capability fxr-package
no mgcp timer receive-rtcp
!
mgcp profile default
!
sccp local GigabitEthernet0/0
sccp ccm 172.20.100.10 identifier 1 version 7.0 
sccp
!
sccp ccm group 1
 bind interface GigabitEthernet0/0
 associate ccm 1 priority 1
 associate profile 1 register conference
 keepalive retries 6
 switchback method graceful
!
dspfarm profile 1 conference  
 codec g729br8
 codec g729r8
 codec g729abr8
 codec g729ar8
 codec g711alaw
 codec g711ulaw
 maximum sessions 4
 associate application SCCP
!
dial-peer voice 10 voip
 description Cisco Unity Express access
 destination-pattern 119[0-8]
 session protocol sipv2
 session target ipv4:172.20.100.20
 dtmf-relay sip-notify
 codec g711ulaw
 no vad
!
dial-peer voice 1 voip
 description **Incoming Call from SIP Trunk**
 translation-profile incoming 1
 session protocol sipv2
 session target dns:trunking.voipdnsservers.com
 incoming called-number .+
 voice-class sip dtmf-relay force rtp-nte
 dtmf-relay rtp-nte
 codec g711ulaw
 no vad
!
dial-peer voice 2 voip
 description **Outgoing Call to SIP Trunk**
 destination-pattern .T
 session protocol sipv2
 session target dns:trunking.voipdnsservers.com:5060
 voice-class sip dtmf-relay force rtp-nte
 no voice-class sip pass-thru headers
 no voice-class sip pass-thru content unsupp
 dtmf-relay rtp-nte
 clid network-number xxxxxxxxx
 no vad
!
!
gateway 
 timer receive-rtp 1200
!
sip-ua 
 credentials username xxxxxxxxx password 7 xxxxxxxxxxxxxxxxxxxx realm voip.nextiva.com
 credentials username xxxxxxxxx password 7 xxxxxxxxxxxxxxxxxxxx realm trunking.voipdnsservers.com
 authentication username xxxxxxxxx:xxxxxxxxx@trunking.voipdnsservers.com/xxxxxxxxx password 7 xxxxxxxxxxxxxxxxxxxx realm trunking.voipdnsservers.com
 authentication username xxxxxxxxx:xxxxxxxxx@trunking.voipdnsservers.com/xxxxxxxxx password 7 xxxxxxxxxxxxxxxxxxxx realm voip.nextiva.com
 no remote-party-id
 retry invite 2
 retry register 10
 timers connect 100
 mwi-server ipv4:172.20.100.20 expires 86400 port 5060 transport udp unsolicited
 registrar dns:trunking.voipdnsservers.com:5060 expires 3600
 sip-server dns:trunking.voipdnsservers.com:5060
!
!
!
telephony-service
 sdspfarm units 8
 sdspfarm transcode sessions 32
 sdspfarm tag 1 conference
 conference hardware
 pin 1994
 max-ephones 50
 max-dn 180
 ip source-address 172.20.100.10 port 2000
 system message HLSM, LLC.
 url services http://172.20.100.20/voiceview/common/login.dou.xml 
 url authentication http://172.20.100.20/voiceview/authentication/authenticate.do  
 load 7960-7940 tftp:P00308010200.loads
 live-record 1195
 voicemail 1190
 mwi relay
 max-conferences 8 gain -6
 call-forward pattern .T
 call-forward system redirecting-expanded
 moh music-on-hold.au
 web admin system name admin password xxxxxx
 dn-webedit 
 time-webedit 
 transfer-system full-consult
 secondary-dialtone **
 directory entry 2 1102 name xxxx xxxxxx
 directory entry 3 1103 name Mike Hilty
 directory entry 4 1104 name xxxxx xxxxxx
 directory entry 5 1105 name xxxxxxxx xxxxxxxxxx
 directory entry 6 1106 name xxxx xxxx
 directory entry 1 1109 name xxxx xxxxxx
 create cnf-files version-stamp 7960 Jul 17 2013 16:36:17
!
!
ephone-template  1
 conference drop-mode creator
 conference add-mode creator
 conference admin
 softkeys remote-in-use  CBarge Newcall
 softkeys hold  Resume Newcall Join Select
 softkeys connected  Hold Trnsfer Endcall LiveRcd Confrn TrnsfVM
 max-calls-per-button 3
 busy-trigger-per-button 2
!
!
ephone-dn  2  dual-line
 number 1102 no-reg primary
 label xxxx xxxxxx
 name xxxx xxxxxx
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  3  dual-line
 number 1103 no-reg primary
 label Mike Hilty
 name Mike Hilty
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  4  dual-line
 number 1104 no-reg primary
 label xxxxx xxxxxx
 name xxxxx xxxxxx
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  5  dual-line
 number 1105 no-reg primary
 label xxxxxxxx xxxxxxxxxx
 name xxxxxxxx xxxxxxxxxx
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  6  dual-line
 number 1106 no-reg primary
 label xxxx xxxx
 name xxxx xxxx
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  7  dual-line
 number 1109 no-reg primary
 label xxxx xxxxxx
 name xxxx xxxxxx
 call-forward busy 1190
 call-forward noan 1190 timeout 15
 mwi sip
!
!
ephone-dn  10  dual-line
 number 1110 no-reg primary
 label Kitchen Phone
 name Kitchen phone
 no huntstop
 mwi sip
 hold-alert 30 originator
!
!
ephone-dn  40  octo-line
 number 1199 no-reg primary
 label General Incoming
 call-forward busy 1190
 call-forward noan 1190 timeout 3
 mwi sip
!
!
ephone-dn  50
 number 8001.... no-reg primary
 mwi off
!
!
ephone-dn  51
 number 8002.... no-reg primary
 mwi on
!
!
ephone-dn  99
 number xxxxxxxxx
!
!
ephone-dn  100  octo-line
 number 1195 no-reg primary
 description *** Live Record DN ***
 call-forward all 1190
!
!
ephone-dn  101  octo-line
 number 2000 no-reg primary
 name Conference Bridge
 conference meetme
!
!
ephone-dn  102  octo-line
 number 2001 no-reg primary
 name Conference Bridge
 conference ad-hoc
 preference 1
 no huntstop
!         
!
ephone  2
 conference admin
 device-security-mode none
 mac-address 0012.434C.ABCB
 ephone-template 1
 username "xxxxxxx"
 type 7940
 mwi-line 2
 button  1:2 2:40
!
!
!
ephone  3
 conference admin
 device-security-mode none
 mac-address 0013.6037.4D98
 ephone-template 1
 username "xxxxx"
 type 7940
 mwi-line 2
 button  1:3 2:40
!
!
!
ephone  4
 conference admin
 device-security-mode none
 mac-address 000F.9093.42FF
 ephone-template 1
 username "xxxxxxxxx"
 type 7940
 mwi-line 2
 button  1:5 2:40
!
!
!
ephone  5
 device-security-mode none
 mac-address 0017.0EF6.D359
 ephone-template 1
 username "xxxxxxxx"
 type 7940
 mwi-line 2
 button  1:6 2:40
!
!
!
ephone  6
 device-security-mode none
 mac-address 000A.B8DE.247A
 ephone-template 1
 username "xxxxxxxxx"
 type 7940
 mwi-line 2
 button  1:4 2:40
!
!
!
ephone  7
 device-security-mode none
 mac-address 0013.60C3.E1D7
 ephone-template 1
 username "xxxxxxxxx"
 type 7940
 mwi-line 2
 button  1:7 2:40
!
!
!
!
line con 0
line aux 0
line 66
 no activation-character
 no exec
 transport preferred none
 transport input all
 transport output lat pad telnet rlogin lapb-ta mop udptn v120 ssh
line 258
 no activation-character
 no exec
 transport preferred none
 transport input all
 transport output lat pad telnet rlogin lapb-ta mop udptn v120 ssh
line vty 0 4
 transport input ssh
!
scheduler allocate 20000 1000
ntp master 1
ntp server 74.122.204.3
ntp server 198.58.100.237
end