CME_2801#
*Oct 20 19:37:35.635: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK596e7146
Max-Forwards: 70
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
CSeq: 3 INVITE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
Contact: <sip:2003@192.168.3.4:5060>
Content-Type: application/sdp
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 391

v=0
o=- 1420070554 1420070555 IN IP4 192.168.3.4
s=-
c=IN IP4 192.168.3.4
t=0 0
m=audio 16108 RTP/AVP 8 18 0 101
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendonly
a=ptime:20
m=video 0 RTP/AVP 102
b=AS:2120
a=rtpmap:102 H264/90000
a=fmtp:102 profile-level-id=42401E; packetization-mode=0
a=sendonly

*Oct 20 19:37:35.651: //163/6798985480D9/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK596e7146
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
Date: Sat, 20 Oct 2018 19:37:35 GMT
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
CSeq: 3 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

*Oct 20 19:37:35.651: //163/6798985480D9/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK596e7146
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
Date: Sat, 20 Oct 2018 19:37:35 GMT
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
CSeq: 3 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 252

v=0
o=CiscoSystemsSIP-GW-UserAgent 7651 389 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 18682 RTP/AVP 8
c=IN IP4 192.168.3.254
a=recvonly
a=rtpmap:8 PCMA/8000
a=ptime:20
m=video 0 RTP/AVP 102
c=IN IP4 192.168.3.254

*Oct 20 19:37:35.707: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK0e2804e5
Max-Forwards: 70
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
CSeq: 3 ACK
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#unhold now
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
*Oct 20 19:37:46.383: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK6514aaa6
Max-Forwards: 70
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
CSeq: 4 INVITE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
Contact: <sip:2003@192.168.3.4:5060>
Content-Type: application/sdp
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 391

v=0
o=- 1420070554 1420070556 IN IP4 192.168.3.4
s=-
c=IN IP4 192.168.3.4
t=0 0
m=audio 16108 RTP/AVP 8 18 0 101
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
a=ptime:20
m=video 0 RTP/AVP 102
b=AS:2120
a=rtpmap:102 H264/90000
a=fmtp:102 profile-level-id=42401E; packetization-mode=0
a=sendrecv

*Oct 20 19:37:46.399: //163/6798985480D9/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK6514aaa6
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
Date: Sat, 20 Oct 2018 19:37:46 GMT
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
CSeq: 4 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

*Oct 20 19:37:46.399: //163/6798985480D9/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK6514aaa6
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
Date: Sat, 20 Oct 2018 19:37:46 GMT
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
CSeq: 4 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 240

v=0
o=CiscoSystemsSIP-GW-UserAgent 7651 389 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 18682 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
a=ptime:20
m=video 0 RTP/AVP 102
c=IN IP4 192.168.3.254

*Oct 20 19:37:46.455: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK2d97c85c
Max-Forwards: 70
Call-ID: 06e30180-1a05321cde6d1e5e5e830080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=1039063419
To: <sip:2002@192.168.3.254>;tag=4ED1B4-288
CSeq: 4 ACK
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#undebug all
All possible debugging has been turned off
CME_2801#