*Oct 20 19:25:37.467: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK1aeb9d1f
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
Max-Forwards: 70
Date: Sat, 20 Oct 2018 19:25:36 GMT
CSeq: 102 INVITE
User-Agent: Cisco-CP9971/9.2.1
Contact: <sip:2001@192.168.3.3:5060;transport=udp>
Accept: application/sdp
Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Call-Info: <urn:x-cisco-remotecc:hold>
Supported: replaces,join,sdp-anat,norefersub,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-5.1.0,X-cisco-xsi-8.0.1
Allow-Events: kpml,dialog
Content-Length: 572
Content-Type: application/sdp
Content-Disposition: session;handling=optional

v=0
o=Cisco-SIPUA 4440 1 IN IP4 192.168.3.3
s=SIP Call
t=0 0
m=audio 18194 RTP/AVP 8 0 18 102 116 101
c=IN IP4 192.168.3.3
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:102 L16/16000
a=rtpmap:116 iLBC/8000
a=fmtp:116 mode=20
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendonly
m=video 32400 RTP/AVP 97
c=IN IP4 192.168.3.3
b=TIAS:1000000
a=rtpmap:97 H264/90000
a=fmtp:97 profile-level-id=42801E;packetization-mode=0;level-asymmetry-allowed=1
a=imageattr:* recv [x=640,y=480,q=0.50]
a=sendonly

*Oct 20 19:25:37.491: //135/BA2E2F6980BC/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK1aeb9d1f
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Date: Sat, 20 Oct 2018 19:25:37 GMT
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
CSeq: 102 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

*Oct 20 19:25:37.491: //135/BA2E2F6980BC/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK1aeb9d1f
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Date: Sat, 20 Oct 2018 19:25:37 GMT
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
CSeq: 102 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 240

v=0
o=CiscoSystemsSIP-GW-UserAgent 2288 8916 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17116 RTP/AVP 8
c=IN IP4 192.168.3.254
a=recvonly
a=rtpmap:8 PCMA/8000
m=video 0 RTP/AVP 97
c=IN IP4 192.168.3.254

*Oct 20 19:25:37.499: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK61e6375d
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
Max-Forwards: 70
Date: Sat, 20 Oct 2018 19:25:36 GMT
CSeq: 102 ACK
User-Agent: Cisco-CP9971/9.2.1
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#unhold now
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
*Oct 20 19:25:53.619: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK6856f875
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
Max-Forwards: 70
Date: Sat, 20 Oct 2018 19:25:52 GMT
CSeq: 103 INVITE
User-Agent: Cisco-CP9971/9.2.1
Contact: <sip:2001@192.168.3.3:5060;transport=udp>
Accept: application/sdp
Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Call-Info: <urn:x-cisco-remotecc:resume>
Supported: replaces,join,sdp-anat,norefersub,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-5.1.0,X-cisco-xsi-8.0.1
Allow-Events: kpml,dialog
Content-Length: 573
Content-Type: application/sdp
Content-Disposition: session;handling=optional

v=0
o=Cisco-SIPUA 16213 2 IN IP4 192.168.3.3
s=SIP Call
t=0 0
m=audio 18194 RTP/AVP 8 0 18 102 116 101
c=IN IP4 192.168.3.3
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:102 L16/16000
a=rtpmap:116 iLBC/8000
a=fmtp:116 mode=20
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
m=video 32400 RTP/AVP 97
c=IN IP4 192.168.3.3
b=TIAS:1000000
a=rtpmap:97 H264/90000
a=fmtp:97 profile-level-id=42801E;packetization-mode=0;level-asymmetry-allowed=1
a=imageattr:* recv [x=640,y=480,q=0.50]
a=sendrecv

*Oct 20 19:25:53.635: //135/BA2E2F6980BC/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK6856f875
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Date: Sat, 20 Oct 2018 19:25:53 GMT
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
CSeq: 103 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

*Oct 20 19:25:53.635: //135/BA2E2F6980BC/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK6856f875
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Date: Sat, 20 Oct 2018 19:25:53 GMT
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
CSeq: 103 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 228

v=0
o=CiscoSystemsSIP-GW-UserAgent 2288 8916 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17116 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
m=video 0 RTP/AVP 97
c=IN IP4 192.168.3.254

*Oct 20 19:25:53.643: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK12abc914
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300122dca3124-01001c13
To: <sip:2002@192.168.3.254>;tag=43D384-116D
Call-ID: 18339d14-d673000b-7655985f-1b26e1a6@192.168.3.3
Max-Forwards: 70
Date: Sat, 20 Oct 2018 19:25:52 GMT
CSeq: 103 ACK
User-Agent: Cisco-CP9971/9.2.1
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#undebug all
All possible debugging has been turned off
CME_2801#
CME_2801#
CME_2801#
CME_2801#