CME_2801#
000082: *Oct 22 20:07:34: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4ad44da8;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>
CSeq: 1 INVITE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
Supported: 100rel,replaces,early-session
Content-Disposition: session
Contact: <sip:2003@192.168.3.4:5060>
Content-Type: application/sdp
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 503

v=0
o=- 1420070504 1420070504 IN IP4 192.168.3.4
s=-
c=IN IP4 192.168.3.4
t=0 0
m=audio 16152 RTP/AVP 9 8 99 18 0 101
a=rtpmap:9 G722/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:99 AMR-WB/16000
a=fmtp:99 mode-set=8; max-red=0; mode-change-capability=2
a=rtpmap:18 G729/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
a=ptime:20
m=video 0 RTP/AVP 102
b=AS:2120
a=rtpmap:102 H264/90000
a=fmtp:102 profile-level-id=42401E; packetization-mode=0
a=sendrecv

000083: *Oct 22 20:07:34: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4ad44da8;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>
Date: Mon, 22 Oct 2018 20:07:34 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 1 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000084: *Oct 22 20:07:34: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 180 Ringing
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4ad44da8;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:07:34 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 1 INVITE
Require: 100rel
RSeq: 661
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000085: *Oct 22 20:07:34: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
PRACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK019224ea;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 2 PRACK
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
RAck: 661 1 INVITE
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

000086: *Oct 22 20:07:34: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK019224ea;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:07:34 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
Server: Cisco-SIPGateway/IOS-12.x
CSeq: 2 PRACK
Content-Length: 0

000087: *Oct 22 20:07:37: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4ad44da8;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:07:34 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 1 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Disposition: session;handling=required
Content-Length: 241

v=0
o=CiscoSystemsSIP-GW-UserAgent 4330 6030 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17208 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
a=ptime:20
m=video 0 RTP/AVP 102
c=IN IP4 192.168.3.254

000088: *Oct 22 20:07:37: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 

CME_2801#
CME_2801#ACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK2610c507;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 1 ACK
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#hold button now——————————————————————————Press HOLD button to put the call on hold——————————————————
          ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000089: *Oct 22 20:07:46: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4c8b8da6;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 3 INVITE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
Contact: <sip:2003@192.168.3.4:5060>
Content-Type: application/sdp
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 391

v=0
o=- 1420070504 1420070505 IN IP4 192.168.3.4
s=-
c=IN IP4 192.168.3.4
t=0 0
m=audio 16152 RTP/AVP 8 18 0 101
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendonly
a=ptime:20
m=video 0 RTP/AVP 102
b=AS:2120
a=rtpmap:102 H264/90000
a=fmtp:102 profile-level-id=42401E; packetization-mode=0
a=sendonly

000090: *Oct 22 20:07:46: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4c8b8da6;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:07:46 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 3 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000091: *Oct 22 20:07:46: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK4c8b8da6;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:07:46 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 3 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 253

v=0
o=CiscoSystemsSIP-GW-UserAgent 4330 6031 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17208 RTP/AVP 8
c=IN IP4 192.168.3.254
a=recvonly
a=rtpmap:8 PCMA/8000
a=ptime:20
m=video 0 RTP/AVP 102
c=IN IP4 192.168.3.254

000092: *Oct 22 20:07:46: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK0dc21f3d;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 3 ACK
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#un-hold now——————————————————————————————Press HOLD button again—————————
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000093: *Oct 22 20:08:03: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK15ef66aa;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 4 INVITE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
Contact: <sip:2003@192.168.3.4:5060>
Content-Type: application/sdp
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 391

v=0
o=- 1420070504 1420070506 IN IP4 192.168.3.4
s=-
c=IN IP4 192.168.3.4
t=0 0
m=audio 16152 RTP/AVP 8 18 0 101
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
a=ptime:20
m=video 0 RTP/AVP 102
b=AS:2120
a=rtpmap:102 H264/90000
a=fmtp:102 profile-level-id=42401E; packetization-mode=0
a=sendrecv

000094: *Oct 22 20:08:03: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK15ef66aa;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:08:03 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 4 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000095: *Oct 22 20:08:03: //25/F2F927528017/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK15ef66aa;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:08:03 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
CSeq: 4 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 241

v=0
o=CiscoSystemsSIP-GW-UserAgent 4330 6031 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17208 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
a=ptime:20
m=video 0 RTP/AVP 102
c=IN IP4 192.168.3.254

000096: *Oct 22 20:08:03: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK52dde9a9;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 4 ACK
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#end call now—————————————————————End the Call——————————————————————
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000097: *Oct 22 20:08:17: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
BYE sip:2002@192.168.3.254:5060 SIP/2.0
Max-Breadth: 60
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK41866d03;rport
Max-Forwards: 70
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
CSeq: 5 BYE
Allow: INVITE,ACK,CANCEL,BYE,PRACK,INFO,UPDATE,OPTIONS,MESSAGE,NOTIFY,REFER
User-Agent: Panasonic-KX-HDV430X/01.003 (bcc34221714a)
Content-Length: 0

000098: *Oct 22 20:08:17: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.4:5060;branch=z9hG4bK41866d03;rport
From: <sip:2003@192.168.3.254>;tag=93775076
To: <sip:2002@192.168.3.254>;tag=B0C24-1B29
Date: Mon, 22 Oct 2018 20:08:17 GMT
Call-ID: 67f022ee-e804321c155040412c9a0080f0808080@KX-HDV430X
Server: Cisco-SIPGateway/IOS-12.x
CSeq: 5 BYE
Reason: Q.850;cause=16
P-RTP-Stat: PS=1167,OS=186720,PR=1156,OR=184960,PL=0,JI=0,LA=0,DU=40
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#undebug all
All possible debugging has been turned off
CME_2801#
CME_2801#