Router#sh run

Building configuration...

Current configuration : 17358 bytes

!

! Last configuration change at 13:53:33 UTC Fri Oct 21 2022

!

version 17.3

service timestamps debug datetime msec

service timestamps log datetime msec

service call-home

platform qfp utilization monitor load 80

platform punt-keepalive disable-kernel-core

!

hostname Router

!

boot-start-marker

boot system bootflash:isr4300-universalk9.17.03.05.SPA.bin

boot-end-marker

!

!

vrf definition Mgmt-intf

!

address-family ipv4

exit-address-family

!

address-family ipv6

exit-address-family

!

!

no aaa new-model

!

!

!

!

!

!

!

ip dhcp excluded-address 10.80.80.1

ip dhcp excluded-address 10.80.80.254

ip dhcp excluded-address 10.80.80.253

ip dhcp excluded-address 10.90.90.1

ip dhcp excluded-address 10.90.90.90

!

ip dhcp pool voice

network 10.90.80.0 255.255.255.0

default-router 10.90.80.1

option 150 ip 10.90.80.1

!

!

!

login on-success log

!

!

!

!

!

!

!

subscriber templating

multilink bundle-name authenticated

no device-tracking logging theft

!

!

!

!

!

!

!

trunk group FXO

hunt-scheme longest-idle

!

!

crypto pki trustpoint TP-self-signed-1038756133

enrollment selfsigned

subject-name cn=IOS-Self-Signed-Certificate-1038756133

revocation-check none

rsakeypair TP-self-signed-1038756133

!

crypto pki trustpoint SLA-TrustPoint

enrollment terminal

revocation-check crl

!

!

crypto pki certificate chain TP-self-signed-1038756133

certificate self-signed 01

30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030

31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274

69666963 6174652D 31303338 37353631 3333301E 170D3232 30393132 30393338

34305A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649

4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 30333837

35363133 33308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201

0A028201 0100A2EB C8537F91 5F645445 E363728A F6B11142 641D6F43 DEB31CEB

410B2F56 60D74368 2AC592D8 E765B41F 4F6B969A 7450ADBA 07E7FA57 C76E2396

7019F693 AFB5CBB6 C9CB30FB 631DC442 34256015 F160EAAE D207C16B 786C566D

E740FF6B 7DE20A8C 9B11C9EF 957027EB B0B144BA 5FC2AF96 E70EFC42 7EC031FA

B5C46EB4 51D3AED5 BEDC3005 F39D6D85 DC5EDEAF B2D3F38B 85BB5D83 CF4A4EC5

C89176A4 9EFA8148 AD4C246C 08FCF2FE 230D3640 DF6C8294 5BA603A9 4EDBFBC0

4B458F9E D1BA2C62 B5C1FD93 46424919 006426E0 4C15D74F 130FA4FD D55F95FE

954F8D1C 5E1AA531 8D3C574E 23D7D7FD A3A1FC57 6BD82C54 0A2922C3 5ADEA644

C1B60B96 1C750203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF

301F0603 551D2304 18301680 14F7B310 8D72988A 9971FF68 9C4882C1 D32BE109

E8301D06 03551D0E 04160414 F7B3108D 72988A99 71FF689C 4882C1D3 2BE109E8

300D0609 2A864886 F70D0101 05050003 82010100 469B01C7 48FB53A4 58E2A3AB

F065CCBD 0B26004D 9538D54E 4E8E3B5E CC86CFE9 8389F1DF 94292227 53BD361F

442CF236 9AEC3588 2868481D 949462B7 26102F5A 0171593D 95569594 2DBE1719

8DE2B03B F0C04152 DE7F0800 10D801D1 8DC1CB71 CF5DE7E6 7304C78E CA8F9030

BDECD4A3 DD36EC62 A5A20E8F F264DC0A 136104DC 4F569CAB 205C7C7C EF169E63

9242ACAE 02647D9A FFB603A5 5E82C3A6 CD0FE622 70CE359A 74428D8A 04D4ACBC

B3C173F2 6FA36349 BB67B96D 3BED1B7D 522C0307 60C4E5F6 8F76288D FDFA10D4

05A84168 6FCCC5C0 219D7658 B14D2338 9F8C58AA 4DE159F0 3671854F 55E137FC

1C001B48 A94B9024 3A5DA512 11493D6A 7787B9EE

quit

crypto pki certificate chain SLA-TrustPoint

certificate ca 01

30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030

32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363

6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934

3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305

43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720

526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030

82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D

CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520

1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE

4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC

7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188

68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7

C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191

C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44

DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201

06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85

4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500

03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905

604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B

D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8

467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C

7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B

5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678

80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB

418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0

D697DF7F 28

quit

!

!

!

!

voice service voip

ip address trusted list

ipv4 0.0.0.0 0.0.0.0

allow-connections sip to h323

allow-connections sip to sip

supplementary-service h450.12

no supplementary-service sip moved-temporarily

no supplementary-service sip refer

fax protocol t38 version 0 ls-redundancy 0 hs-redundancy 0 fallback none

trace

sip

bind control source-interface GigabitEthernet0/0/0

bind media source-interface GigabitEthernet0/0/0

registrar server expires max 1200 min 300

!

voice class codec 1

codec preference 1 g711ulaw

!

!

!

!

voice class dualtone-detect-params 1

freq-max-deviation 50

!

voice class custom-cptone UAE-Default

dualtone disconnect

frequency 400

cadence 400 350 225 525

!

!

!

voice register global

mode cme

source-address 10.90.80.1 port 5060

max-dn 50

max-pool 30

load 7811 sip78xx.14-1-1-0107-157

authenticate register

authenticate realm local

voicemail 1000

tftp-path flash:

create profile sync 0001344382202193

auto-register

!

!

voice register dn 1

number 801

call-forward b2bua noan 1000 timeout 20

allow watch

name Basel Thaher

label WZP2609982P

!

voice register dn 2

number 802

call-forward b2bua noan 1000 timeout 20

allow watch

name Michael Kolta

label WZP2609982P1

!

voice register dn 3

number 803

call-forward b2bua noan 1000 timeout 20

allow watch

name Murad Salman

label WZP2609982P2

!

voice register dn 4

number 804

call-forward b2bua noan 1000 timeout 20

allow watch

name Duraid Al-Rammahy

label WZP2609982P3

!

voice register dn 5

number 805

call-forward b2bua noan 1000 timeout 20

allow watch

name Pauline Chichiricco

label WZP2609982P4

!

voice register dn 6

number 806

call-forward b2bua noan 1000 timeout 20

allow watch

name Amro Ali

label WZP2609982P5

!

voice register dn 7

number 807

call-forward b2bua noan 1000 timeout 20

allow watch

name Yosra Saadalla

label WZP2609982P6

!

voice register dn 8

number 808

call-forward b2bua noan 1000 timeout 20

allow watch

name Redouane Amokrane

label WZP2609982P7

!

voice register dn 9

number 809

call-forward b2bua noan 1000 timeout 20

allow watch

name Ola Darwicheh

label WZP2609982P8

!

voice register dn 10

number 810

call-forward b2bua noan 1000 timeout 20

allow watch

name Ossama Deghidy

label WZP2609982P9

!

voice register dn 11

number 811

call-forward b2bua noan 1000 timeout 20

allow watch

name Mohamed Kayali

label WZP2609982P10

!

voice register dn 12

number 812

call-forward b2bua noan 1000 timeout 20

allow watch

name Rachal Shami

label WZP2609982P11

!

voice register dn 13

number 813

call-forward b2bua noan 1000 timeout 20

allow watch

name Linda Dabat

label WZP2609982P12

!

voice register dn 14

number 814

call-forward b2bua noan 1000 timeout 20

allow watch

name Dinara Munbayeva

label WZP2609982P13

!

voice register dn 15

number 815

call-forward b2bua noan 1000 timeout 20

allow watch

name Nelricia Franco

label WZP2609982P14

!

voice register dn 16

number 816

call-forward b2bua noan 1000 timeout 20

allow watch

name Ansam Al-Tekreeti

label WZP2609982P15

!

voice register dn 17

number 817

call-forward b2bua noan 1000 timeout 20

allow watch

name Mohamed Mahmoud

label WZP2609982P16

!

voice register dn 18

number 818

call-forward b2bua noan 1000 timeout 20

allow watch

name Charles Challita

label WZP2609982P17

!

voice register dn 19

number 800

call-forward b2bua noan 1000 timeout 20

allow watch

name Tatsiana Zakharenka

label WZP2609982P18

!

voice register pool 1

busy-trigger-per-button 2

id mac 00DF.1D88.6A20

type 7811

number 1 dn 1

presence call-list

dtmf-relay sip-notify

username 801 password Cisco123

codec g711ulaw

!

voice register pool 2

busy-trigger-per-button 2

id mac 00DF.1D88.B4B5

type 7811

number 1 dn 2

presence call-list

dtmf-relay sip-notify

!

voice register pool 3

busy-trigger-per-button 2

id mac 00DF.1D88.B4A7

type 7811

number 1 dn 3

presence call-list

dtmf-relay sip-notify

!

voice register pool 4

busy-trigger-per-button 2

id mac 00DF.1D88.B3AC

type 7811

number 1 dn 4

presence call-list

dtmf-relay sip-notify

!

voice register pool 5

busy-trigger-per-button 2

id mac 00DF.1D88.BE80

type 7811

number 1 dn 5

presence call-list

dtmf-relay sip-notify

!

voice register pool 6

busy-trigger-per-button 2

id mac 00DF.1D88.B47F

type 7811

number 1 dn 6

presence call-list

dtmf-relay sip-notify

!

voice register pool 7

busy-trigger-per-button 2

id mac 00DF.1D88.B88C

type 7811

number 1 dn 7

presence call-list

dtmf-relay sip-notify

!

voice register pool 8

busy-trigger-per-button 2

id mac 00DF.1D88.B641

type 7811

number 1 dn 8

presence call-list

dtmf-relay sip-notify

!

voice register pool 9

busy-trigger-per-button 2

id mac 00DF.1D88.B5FA

type 7811

number 1 dn 9

presence call-list

dtmf-relay sip-notify

!

voice register pool 10

busy-trigger-per-button 2

id mac 00DF.1D88.B434

type 7811

number 1 dn 10

presence call-list

dtmf-relay sip-notify

!

voice register pool 11

busy-trigger-per-button 2

id mac 00DF.1D88.B3EE

type 7811

number 1 dn 11

presence call-list

dtmf-relay sip-notify

!

voice register pool 12

busy-trigger-per-button 2

id mac 00DF.1D88.B3C4

type 7811

number 1 dn 12

presence call-list

dtmf-relay sip-notify

!

voice register pool 13

busy-trigger-per-button 2

id mac 00DF.1D88.B6FA

type 7811

number 1 dn 13

presence call-list

dtmf-relay sip-notify

!

voice register pool 14

busy-trigger-per-button 2

id mac 00DF.1D88.6967

type 7811

number 1 dn 14

presence call-list

dtmf-relay sip-notify

!

voice register pool 15

busy-trigger-per-button 2

id mac 00DF.1D88.C083

type 7811

number 1 dn 15

presence call-list

dtmf-relay sip-notify

!

voice register pool 16

busy-trigger-per-button 2

id mac 00DF.1D88.B425

type 7811

number 1 dn 16

presence call-list

dtmf-relay sip-notify

!

voice register pool 17

busy-trigger-per-button 2

id mac 00DF.1D88.B465

type 7811

number 1 dn 17

presence call-list

dtmf-relay sip-notify

!

voice register pool 18

busy-trigger-per-button 2

id mac 00DF.1D88.6AF8

type 7811

number 1 dn 18

presence call-list

dtmf-relay sip-notify

!

voice register pool 19

busy-trigger-per-button 2

id mac 00DF.1D88.B41F

type 7811

number 1 dn 19

presence call-list

dtmf-relay sip-notify

!

voice hunt-group 1 sequential

final 1000

list 800,816,801

pilot 800

!

!

!

!

!

!

application

service app-b-acd-aa flash:app-b-acd-aa-3.0.0.8.tcl

!

service app-b-acd flash:app-b-acd-3.0.0.8.tcl

!

!

!

!

!

voice-card 0/1

no watchdog

!

voice-card 0/2

no watchdog

!

voice-card 0/4

no watchdog

!

license udi pid ISR4321/K9 sn FDO26300QM1

license boot suite AdvUCSuiteK9

license boot level uck9

license smart reservation

memory free low-watermark processor 69596

!

diagnostic bootup level minimal

!

spanning-tree extend system-id

!

!

redundancy

mode none

!

!

!

!

!

!

!

!

interface GigabitEthernet0/0/0

ip address 10.90.80.1 255.255.255.0

negotiation auto

!

interface GigabitEthernet0/0/1

no ip address

negotiation auto

!

interface Service-Engine0/1/0

!

interface Service-Engine0/2/0

!

interface Service-Engine0/4/0

!

interface GigabitEthernet0

vrf forwarding Mgmt-intf

no ip address

shutdown

negotiation auto

!

ip http server

ip http authentication local

ip http secure-server

ip forward-protocol nd

!

!

!

!

!

tftp-server bootflash:sip78xx.14-1-1-0107-157.loads

tftp-server bootflash:sboot78xx.14-1-1-0107-157.sbn

tftp-server bootflash:sboot2.78xx.14-1-1-0107-157.sbn

tftp-server bootflash:rootfs78xx.14-1-1-0107-157.sbn

tftp-server bootflash:rootfs2.78xx.14-1-1-0107-157.sbn

tftp-server bootflash:kern78xx.14-1-1-0107-157.sbn

tftp-server bootflash:kern2.78xx.14-1-1-0107-157.sbn

!

control-plane

!

!

voice-port 0/1/0

trunk-group FXO

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

voice-port 0/1/1

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

voice-port 0/2/0

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

voice-port 0/2/1

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

voice-port 0/2/2

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

voice-port 0/2/3

translation-profile incoming prefix

supervisory disconnect dualtone mid-call

supervisory custom-cptone UAE-Default

supervisory dualtone-detect-params 1

input gain 14

cptone AE

timeouts interdigit 2

timeouts call-disconnect 3

timeouts wait-release 1

connection plar 801

bearer-cap Speech

caller-id enable

!

mgcp behavior rsip-range tgcp-only

mgcp behavior comedia-role none

mgcp behavior comedia-check-media-src disable

mgcp behavior comedia-sdp-force disable

!

mgcp profile default

!

!

!

!

telephony-service

protocol mode dual-stack preference ipv4

sdspfarm conference mute-on 111 mute-off 222

sdspfarm units 2

sdspfarm transcode sessions 24

sdspfarm tag 1 conference

sdspfarm tag 2 mtpgarswlpro001

conference hardware

max-ephones 30

max-dn 100

ip source-address 10.90.80.1 port 2000

system message Menarini UAE

time-zone 35

voicemail 1000

max-conferences 8 gain -6

call-park system application

transfer-system full-consult

transfer-pattern T

secondary-dialtone 9

fac custom voicemail \*98

!

!

dial-peer voice 1 pots

trunkgroup FXO

destination-pattern 90[234679].......

prefix 0

!

dial-peer voice 2 pots

trunkgroup FXO

destination-pattern 9[2-8][0-9][1-9]....

forward-digits 7

!

dial-peer voice 5 pots

trunkgroup FXO

destination-pattern 900T

prefix 00

!

dial-peer voice 7 pots

trunkgroup FXO

destination-pattern 9800T

prefix 800

!

dial-peer voice 6 pots

trunkgroup FXO

destination-pattern 9600T

prefix 600

!

dial-peer voice 3 pots

trunkgroup FXO

destination-pattern 905[0456].......

prefix 05

!

dial-peer voice 20 voip

destination-pattern 1000

session protocol sipv2

session target ipv4:10.90.80.3

dtmf-relay sip-notify

codec g711ulaw

no vad

!

dial-peer voice 30 voip

session protocol sipv2

session target ipv4:10.90.80.3

incoming called-number 8..

dtmf-relay sip-notify

codec g711ulaw

!

dial-peer voice 40 voip

destination-pattern 1...

session protocol sipv2

session target ipv4:10.90.80.3

dtmf-relay sip-notify rtp-nte

codec g711ulaw

!

!

!

ephone-template 1

softkeys hold Resume Newcall Join Select

softkeys idle Redial Newcall Cfwdall Dnd ConfList Join

softkeys seized Endcall Callback Redial Meetme Cfwdall

softkeys connected Hold Endcall Trnsfer Join Confrn ConfList

!

!

line con 0

stopbits 1

line aux 0

stopbits 1

line vty 0 4

login

transport input ssh

!

call-home

! If contact email address in call-home is configured as sch-smart-licensing@cisco.com

! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.

contact-email-addr sch-smart-licensing@cisco.com

profile "CiscoTAC-1"

active

destination transport-method http

!

!

!

!

!

!

end

Router#