=~=~=~=~=~=~=~=~=~=~=~= PuTTY log 2024.06.20 10:05:58 =~=~=~=~=~=~=~=~=~=~=~=

sh run | s voice service voip

voice service voip

ip address trusted list

ipv4 172.17.27.59

ipv4 192.168.5.8

ipv4 172.17.40.8

ipv4 10.125.41.230

ipv4 10.5.109.147

ipv4 10.5.64.98

ipv4 10.5.64.99

ipv4 10.5.64.114

ipv4 10.5.64.115

ipv4 10.5.64.66

ipv4 10.5.64.67

ipv4 10.5.64.82

ipv4 10.5.64.83

allow-connections h323 to h323

allow-connections h323 to sip

allow-connections sip to h323

allow-connections sip to sip

no supplementary-service sip moved-temporarily

no supplementary-service sip refer

supplementary-service media-renegotiate

fax protocol t38 version 0 ls-redundancy 0 hs-redundancy 0 fallback none

--More-- trace

sip

registrar server expires max 120 min 60

VTZ\_ISR\_4331#sh run | s voice service voip dial-peer

dial-peer voice 900 voip

description KolCUCM

destination-pattern 9..

session protocol sipv2

session target ipv4:172.17.27.59

session transport tcp

incoming called-number 1..

voice-class sip bind control source-interface GigabitEthernet0/0/0

voice-class sip bind media source-interface GigabitEthernet0/0/0

dtmf-relay rtp-nte

codec g711ulaw

dial-peer voice 1 voip

description KkdCME

destination-pattern 8..

session protocol sipv2

session target ipv4:192.168.5.8

incoming called-number 1..

voice-class sip bind control source-interface GigabitEthernet0/0/0

voice-class sip bind media source-interface GigabitEthernet0/0/0

dtmf-relay rtp-nte

codec g711ulaw

dial-peer voice 300 voip

description \*Outbound Calls\*

--More-- translation-profile outgoing OUTGOING

destination-pattern 9T

session protocol sipv2

session target sip-server

voice-class codec 1

voice-class sip early-offer forced

voice-class sip profiles 1

voice-class sip tenant 3

voice-class sip bind control source-interface GigabitEthernet0/0/2

voice-class sip bind media source-interface GigabitEthernet0/0/2

dtmf-relay rtp-nte

no vad

dial-peer voice 500 voip

description \*Inbound calls\*

translation-profile incoming INCOMING

session protocol sipv2

session target ipv4:10.5.109.147

incoming called-number .%

incoming uri via PSTN

voice-class codec 1

voice-class sip transport switch udp tcp

voice-class sip early-offer forced

voice-class sip bind control source-interface GigabitEthernet0/0/2

--More-- voice-class sip bind media source-interface GigabitEthernet0/0/2

dtmf-relay rtp-nte

no vad

VTZ\_ISR\_4331#sh run | s dial-peer translation

voice translation-rule 1

rule 1 /^9/ //

voice translation-rule 2

rule 1 /187/ /+918914560050/

voice translation-rule 3

rule 1 /8914560050/ /187/

voice translation-rule 100

rule 1 /918914560050/ /187/

rule 2 /918914560051/ /190/

voice translation-profile INCOMING

translate called 3

voice translation-profile OUTGOING

translate calling 2

translate called 1

translation-profile outgoing OUTGOING

translation-profile incoming INCOMING

VTZ\_ISR\_4331# sh run | s translation profi

VTZ\_ISR\_4331#sh run | s profile

voice class sip-profiles 1

request INVITE sip-header P-Asserted-Identity modify "ap.ims.airtel.in" "10.5.109.147"

request INVITE sip-header From modify "ap.ims.airtel.in" "10.5.109.147"

create profile sync 0015144571460343

voice translation-profile INCOMING

translate called 3

voice translation-profile OUTGOING

translate calling 2

translate called 1

mgcp profile default

dspfarm profile 1 transcode universal

associate application CUBE

shutdown

translation-profile outgoing OUTGOING

voice-class sip profiles 1

translation-profile incoming INCOMING

profile "CiscoTAC-1"

active

destination transport-method http

VTZ\_ISR\_4331#sh run | s profile sip-ua

VTZ\_ISR\_4331#deb conf t

Enter configuration commands, one per line. End with CNTL/Z.

VTZ\_ISR\_4331(config)#sip

VTZ\_ISR\_4331(config)#sip-ua

VTZ\_ISR\_4331(config-sip-ua)#regis

VTZ\_ISR\_4331(config-sip-ua)#registrar

VTZ\_ISR\_4331(config-sip-ua)#registrar ipv4:10.125.41.229 expires 3600

VTZ\_ISR\_4331(config-sip-ua)#conn

VTZ\_ISR\_4331(config-sip-ua)#connection-reuse

VTZ\_ISR\_4331(config-sip-ua)#retr

VTZ\_ISR\_4331(config-sip-ua)#retry in

VTZ\_ISR\_4331(config-sip-ua)#retry inv

VTZ\_ISR\_4331(config-sip-ua)#retry invite 2

VTZ\_ISR\_4331(config-sip-ua)#timer

VTZ\_ISR\_4331(config-sip-ua)#timers try

VTZ\_ISR\_4331(config-sip-ua)#timers trying 300

VTZ\_ISR\_4331(config-sip-ua)#g72

VTZ\_ISR\_4331(config-sip-ua)#g729-annexb ove

VTZ\_ISR\_4331(config-sip-ua)#g729-annexb override

VTZ\_ISR\_4331(config-sip-ua)#^Z

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#debu

VTZ\_ISR\_4331#debug ccsip mess

VTZ\_ISR\_4331#debug ccsip messages

SIP Call messages tracing is enabled

VTZ\_ISR\_4331#term mon

VTZ\_ISR\_4331#

Jun 20 04:39:41.291: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

INVITE sip:9@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

Max-Forwards: 70

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:41 GMT

CSeq: 101 INVITE

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Expires: 180

Accept: application/sdp

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO

Remote-Party-ID: "IT" <sip:187@172.17.40.8>;party=calling;id-type=subscriber;privacy=off;screen=yes

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Allow-Events: kpml,dialog

Recv-Info: conference

Recv-Info: x-cisco-conference

Content-Length: 351

Content-Type: application/sdp

Content-Disposition: session;handling=optional

v=0

o=Cisco-SIPUA 27035 0 IN IP4 172.17.40.137

s=SIP Call

b=AS:4064

t=0 0

m=audio 30594 RTP/AVP 0 8 116 18 101

c=IN IP4 172.17.40.137

b=TIAS:64000

a=rtpmap:0 PCMU/8000

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=sendrecv

Jun 20 04:39:41.297: //144654/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 100 Trying

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>

Date: Thu, 20 Jun 2024 04:39:41 GMT

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Session-ID: 00000000000000000000000000000000;remote=347f91a300105000a0003891b747f240

Content-Length: 0

Jun 20 04:39:41.382: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

NOTIFY sip:9@172.17.40.8:5060 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK1761c8ac

To: <sip:9@172.17.40.8>;tag=F664C52-15F0

From: <sip:187@172.17.40.137>;tag=3891b747f24001fa35033fda-11e9edb8

Call-ID: F174DC16-2DF511EF-8180F36B-BE441B40@172.17.40.8

Session-ID: e2c886d400105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:41 GMT

CSeq: 1000 NOTIFY

Event: kpml

Subscription-State: active; expires=7200

Max-Forwards: 70

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE

Content-Length: 0

Jun 20 04:39:42.965: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

NOTIFY sip:9@172.17.40.8:5060 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK30070556

To: <sip:9@172.17.40.8>;tag=F664C52-15F0

From: <sip:187@172.17.40.137>;tag=3891b747f24001fa35033fda-11e9edb8

Call-ID: F174DC16-2DF511EF-8180F36B-BE441B40@172.17.40.8

Session-ID: e2c886d400105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:42 GMT

CSeq: 1001 NOTIFY

Event: kpml

Subscription-State: active; expires=7200

Max-Forwards: 70

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE

Content-Length: 205

Content-Type: application/kpml-response+xml

Content-Disposition: session;handling=required

<?xml version="1.0" encoding="UTF-8"?>

<kpml-response xmlns="urn:ietf:params:xml:ns:kpml-response" version="1.0" code="200" text="OK" suppressed="false" forced\_flush="false" digits="8" tag="Backspace OK"/>

Jun 20 04:39:43.380: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

NOTIFY sip:9@172.17.40.8:5060 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK5f355fff

To: <sip:9@172.17.40.8>;tag=F664C52-15F0

From: <sip:187@172.17.40.137>;tag=3891b747f24001fa35033fda-11e9edb8

Call-ID: F174DC16-2DF511EF-8180F36B-BE441B40@172.17.40.8

Session-ID: e2c886d400105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:43 GMT

CSeq: 1002 NOTIFY

Event: kpml

Subscription-State: active; expires=7200

Max-Forwards: 70

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE

Content-Length: 205

Content-Type: application/kpml-response+xml

Content-Disposition: session;handling=required

<?xml version="1.0" encoding="UTF-8"?>

<kpml-response xmlns="urn:ietf:params:xml:ns:kpml-response" version="1.0" code="200" text="OK" suppressed="false" forced\_flush="false" digits="9" tag="Backspace OK"/>

Jun 20 04:39:43.387: //144655/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Sent:

INVITE sip:89@10.5.109.147:5060 SIP/2.0

Via: SIP/2.0/UDP 10.125.41.230:5060;branch=z9hG4bK103BDFA5

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

To: <sip:89@10.5.109.147>

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Min-SE: 1800

Cisco-Guid: 4050897540-0771035631-2172384107-3192134464

User-Agent: Cisco-SIPGateway/IOS-17.6.1a

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

CSeq: 101 INVITE

Timestamp: 1718858383

Contact: <sip:+918914560050@10.125.41.230:5060>

Expires: 180

Allow-Events: telephone-event

Max-Forwards: 69

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 250

v=0

o=CiscoSystemsSIP-GW-UserAgent 1482 6820 IN IP4 10.125.41.230

s=SIP Call

c=IN IP4 10.125.41.230

t=0 0

m=audio 10706 RTP/AVP 0 101

c=IN IP4 10.125.41.230

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

Jun 20 04:39:43.406: //144655/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 100 Trying

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Via: SIP/2.0/UDP 10.125.41.230:5060;received=10.125.41.230;branch=z9hG4bK103BDFA5

To: <sip:89@10.5.109.147>

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

CSeq: 101 INVITE

Date: Thu, 20 Jun 2024 04:39:43 GMT

Timestamp: 1718858383

Content-Length: 0

Jun 20 04:39:43.406: //144655/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 407 Proxy Authentication Required

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Via: SIP/2.0/UDP 10.125.41.230:5060;received=10.125.41.230;branch=z9hG4bK103BDFA5

To: <sip:89@10.5.109.147>;tag=662bf1c3-6673b28f17a44738

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

CSeq: 101 INVITE

Date: Thu, 20 Jun 2024 04:39:43 GMT

Warning: 399 apa37.org "IP association no match, user not registered"

Content-Length: 0

Jun 20 04:39:43.414: //144656/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Sent:

INVITE sip:989@172.17.27.59:5060 SIP/2.0

Via: SIP/2.0/TCP 172.17.40.8:5060;branch=z9hG4bK103BEC1C

Remote-Party-ID: "IT" <sip:187@172.17.40.8>;party=calling;screen=yes;privacy=off

From: "IT" <sip:187@10.125.41.229>;tag=F665494-A25

To: <sip:989@172.17.27.59>

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B71FD8-2DF511EF-8184F36B-BE441B40@172.17.40.8

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Min-SE: 1800

Cisco-Guid: 4050897540-0771035631-2172384107-3192134464

User-Agent: Cisco-SIPGateway/IOS-17.6.1a

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

CSeq: 101 INVITE

Timestamp: 1718858383

Contact: <sip:187@172.17.40.8:5060;transport=tcp>

Expires: 180

Allow-Events: telephone-event

Max-Forwards: 69

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 267

v=0

o=CiscoSystemsSIP-GW-UserAgent 991 3531 IN IP4 172.17.40.8

s=SIP Call

c=IN IP4 172.17.40.8

t=0 0

m=audio 10708 RTP/AVP 0 101 19

c=IN IP4 172.17.40.8

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=rtpmap:19 CN/8000

a=ptime:20

Jun 20 04:39:43.415: //144655/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Sent:

ACK sip:89@10.5.109.147:5060 SIP/2.0

Via: SIP/2.0/UDP 10.125.41.230:5060;branch=z9hG4bK103BDFA5

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

To: <sip:89@10.5.109.147>;tag=662bf1c3-6673b28f17a44738

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Max-Forwards: 70

CSeq: 101 ACK

Allow-Events: telephone-event

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Length: 0

Jun 20 04:39:43.420: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

NOTIFY sip:9@172.17.40.8:5060 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK00539fb8

To: <sip:9@172.17.40.8>;tag=F664C52-15F0

From: <sip:187@172.17.40.137>;tag=3891b747f24001fa35033fda-11e9edb8

Call-ID: F174DC16-2DF511EF-8180F36B-BE441B40@172.17.40.8

Session-ID: e2c886d400105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:43 GMT

CSeq: 1003 NOTIFY

Event: kpml

Subscription-State: terminated; reason=timeout

Max-Forwards: 70

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE

Content-Length: 218

Content-Type: application/kpml-response+xml

Content-Disposition: session;handling=required

<?xml version="1.0" encoding="UTF-8"?>

<kpml-response xmlns="urn:ietf:params:xml:ns:kpml-response" version="1.0" code="487" text="Subscription Exp" suppressed="false" forced\_flush="false" digits="" tag="Backspace OK"/>

Jun 20 04:39:43.461: //144656/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 100 Trying

Via: SIP/2.0/TCP 172.17.40.8:5060;branch=z9hG4bK103BEC1C

From: "IT" <sip:187@10.125.41.229>;tag=F665494-A25

To: <sip:989@172.17.27.59>

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B71FD8-2DF511EF-8184F36B-BE441B40@172.17.40.8

CSeq: 101 INVITE

Allow-Events: presence

Content-Length: 0

Jun 20 04:39:43.463: //144656/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 404 Not Found

Via: SIP/2.0/TCP 172.17.40.8:5060;branch=z9hG4bK103BEC1C

From: "IT" <sip:187@10.125.41.229>;tag=F665494-A25

To: <sip:989@172.17.27.59>;tag=1271810~c961babc-d78c-40c7-9169-6d3071fa2c18-22673913

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B71FD8-2DF511EF-8184F36B-BE441B40@172.17.40.8

CSeq: 101 INVITE

Allow-Events: presence

Reason: Q.850;cause=1

Server: Cisco-CUCM14.0

Session-ID: 00000000000000000000000000000000;remote=347f91a300105000a0003891b747f240

Content-Length: 0

Jun 20 04:39:43.466: //144654/F173CA84817B/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 404 Not Found

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>;tag=F6654CA-4A1

Date: Thu, 20 Jun 2024 04:39:41 GMT

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Warning: 399 172.17.40.8 "No matching outgoing dial-peer"

Server: Cisco-SIPGateway/IOS-17.6.1a

Reason: Q.850;cause=1

Session-ID: 00000000000000000000000000000000;remote=347f91a300105000a0003891b747f240

Content-Length: 0

Jun 20 04:39:43.467: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

ACK sip:989@172.17.27.59:5060 SIP/2.0

Via: SIP/2.0/TCP 172.17.40.8:5060;branch=z9hG4bK103BEC1C

From: "IT" <sip:187@10.125.41.229>;tag=F665494-A25

To: <sip:989@172.17.27.59>;tag=1271810~c961babc-d78c-40c7-9169-6d3071fa2c18-22673913

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B71FD8-2DF511EF-8184F36B-BE441B40@172.17.40.8

Max-Forwards: 70

CSeq: 101 ACK

Allow-Events: telephone-event

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Length: 0

Jun 20 04:39:43.480: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

ACK sip:9@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>;tag=F6654CA-4A1

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Max-Forwards: 70

Date: Thu, 20 Jun 2024 04:39:43 GMT

CSeq: 101 ACK

Content-Length: 0

Jun 20 04:39:43.762: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

REGISTER sip:172.17.40.8 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.160:5060;branch=z9hG4bK4a5dc465

From: <sip:124@172.17.40.8>;tag=3891b747f09d6d4902fbe37a-7782fc8a

To: <sip:124@172.17.40.8>

Call-ID: 3891b747-f09d01d7-2d4dfd38-659eab10@172.17.40.160

Max-Forwards: 70

Session-ID: d705d7ff00105000a0003891b747f09d;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:51 GMT

CSeq: 26914 REGISTER

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DEEC-435@172.17.40.160:5060;transport=udp>;+sip.instance="<urn:uuid:00000000-0000-0000-0000-3891b747f09d>";+u.sip!devicename.ccm.cisco.com="SEP3891B747F09D";+u.sip!model.ccm.cisco.com="622"

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Content-Length: 0

Expires: 3600

Jun 20 04:39:43.765: //144657/F2ECFC118185/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/UDP 172.17.40.160:5060;branch=z9hG4bK4a5dc465

From: <sip:124@172.17.40.8>;tag=3891b747f09d6d4902fbe37a-7782fc8a

To: <sip:124@172.17.40.8>;tag=F6655F4-2076

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: 3891b747-f09d01d7-2d4dfd38-659eab10@172.17.40.160

Server: Cisco-SIPGateway/IOS-17.6.1a

CSeq: 26914 REGISTER

Supported: X-cisco-cme-sis-9.0.0

Supported: X-cisco-srtp-fallback

Contact: <sip:124@172.17.40.160:5060>;expires=120

Expires: 120

Content-Length: 0

Jun 20 04:39:44.039: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

REGISTER sip:172.17.40.8 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.119:5060;branch=z9hG4bK279f9381

From: <sip:131@172.17.40.8>;tag=8c1e809a257e1f813a6d752d-667ede3b

To: <sip:131@172.17.40.8>

Call-ID: 8c1e809a-257e0061-6b7643cb-4b37bc6e@172.17.40.119

Max-Forwards: 70

Session-ID: 2062a8d700105000a0008c1e809a257e;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:44 GMT

CSeq: 7954 REGISTER

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DEFB-1824@172.17.40.119:5060;transport=udp>;+sip.instance="<urn:uuid:00000000-0000-0000-0000-8c1e809a257e>";+u.sip!devicename.ccm.cisco.com="SEP8C1E809A257E";+u.sip!model.ccm.cisco.com="622"

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Content-Length: 0

Expires: 3600

Jun 20 04:39:44.041: //144658/F31742288186/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/UDP 172.17.40.119:5060;branch=z9hG4bK279f9381

From: <sip:131@172.17.40.8>;tag=8c1e809a257e1f813a6d752d-667ede3b

To: <sip:131@172.17.40.8>;tag=F665709-10B

Date: Thu, 20 Jun 2024 04:39:44 GMT

Call-ID: 8c1e809a-257e0061-6b7643cb-4b37bc6e@172.17.40.119

Server: Cisco-SIPGateway/IOS-17.6.1a

CSeq: 7954 REGISTER

Supported: X-cisco-cme-sis-9.0.0

Supported: X-cisco-srtp-fallback

Contact: <sip:131@172.17.40.119:5060>;expires=120

Expires: 120

Content-Length: 0

89116: Jun 20 04:39:44.358: //144654/F173CA84817B/

------------------ Cover Buffer ---------------

Search-key = 187:9:144654

Timestamp = Jun 20 04:39:41.291

CallID = 144654

Peer-CallID = 144656

Correlator = NA

Called-Number = 9

Calling-Number = 187

SIP CallID = 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

SIP SessionID =

GUID = F173CA84817B

-----------------------------------------------

88984: Jun 20 04:39:41.291: //144654/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 172.17.40.137:5060 to 172.17.40.8:5060

INVITE sip:9@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

Max-Forwards: 70

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:41 GMT

CSeq: 101 INVITE

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Expires: 180

Accept: application/sdp

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO

Remote-Party-ID: "IT" <sip:187@172.17.40.8>;party=calling;id-type=subscriber;privacy=off;screen=yes

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Allow-Events: kpml,dialog

Recv-Info: conference

Recv-Info: x-cisco-conference

Content-Length: 351

Content-Type: application/sdp

Content-Disposition: session;handling=optional

v=0

o=Cisco-SIPUA 27035 0 IN IP4 172.17.40.137

s=SIP Call

b=AS:4064

t=0 0

m=audio 30594 RTP/AVP 0 8 116 18 101

c=IN IP4 172.17.40.137

b=TIAS:64000

a=rtpmap:0 PCMU/8000

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=sendrecv

88988: Jun 20 04:39:41.291: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_NONE, Next State = STATE\_IDLE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

88989: Jun 20 04:39:41.293: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Matched Dialpeer: Dir:Inbound, Peer-Tag: 40014

88990: Jun 20 04:39:41.293: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/Offer-Answer: Event = E\_SIP\_INVITE\_SDP\_RCVD, Current State = S\_SIP\_EARLY\_DIALOG\_IDLE, Next State = S\_SIP\_EARLY\_DIALOG\_OFFER\_RCVD

88991: Jun 20 04:39:41.294: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_RCVD\_SDP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = S\_SIP\_IWF\_SDP\_RCVD\_AWAIT\_PEER\_EVENT

88992: Jun 20 04:39:41.294: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Media Stream Parameters: Stream Type = voice-only, Stream State = STREAM\_ADDING Negotiated Codec = g711ulaw, Negotiated DTMF Type = inband-voice, Stream Index = 1

88993: Jun 20 04:39:41.295: //144654/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

88994: Jun 20 04:39:41.295: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_allocate\_port (10704)

88995: Jun 20 04:39:41.295: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Media Stream Parameters: Stream Type = voice-only, Stream State = STREAM\_ADDING Negotiated Codec = g711ulaw, Negotiated DTMF Type = inband-voice, Stream Index = 1

88996: Jun 20 04:39:41.294: //144654/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_call\_setup\_ind\_with\_callID (0)

88997: Jun 20 04:39:41.295: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_IDLE, Next State = STATE\_RECD\_INVITE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

88998: Jun 20 04:39:41.296: //144654/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 172.17.40.8:5060 to 172.17.40.137:5060

SIP/2.0 100 Trying

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>

Date: Thu, 20 Jun 2024 04:39:41 GMT

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Session-ID: 00000000000000000000000000000000;remote=347f91a300105000a0003891b747f240

Content-Length: 0

88999: Jun 20 04:39:42.964: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/DTMF Digit: Type: KPML-Digit-Notify, Dir: Received, DIGIT: /'8/'

89000: Jun 20 04:39:43.065: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/Timer-Action: Event = SIP\_TIMER\_DIGIT, Current State = STATE\_RECD\_INVITE

89001: Jun 20 04:39:43.380: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/DTMF Digit: Type: KPML-Digit-Notify, Dir: Received, DIGIT: /'9/'

89006: Jun 20 04:39:43.383: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_SET\_MODE, Current State = CNFSM\_CONTAINER\_STATE, Next State = CNFSM\_NO\_STATE\_CHANGE

89007: Jun 20 04:39:43.383: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_create\_session (0)

89008: Jun 20 04:39:43.383: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_set\_non\_rtp\_call (0)

89009: Jun 20 04:39:43.383: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89010: Jun 20 04:39:43.383: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_CC\_CALL\_PROCEEDING, Current State = STATE\_RECD\_INVITE

89055: Jun 20 04:39:43.408: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_SET\_MODE, Current State = CNFSM\_CONTAINER\_STATE, Next State = CNFSM\_NO\_STATE\_CHANGE

89056: Jun 20 04:39:43.408: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89057: Jun 20 04:39:43.408: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_set\_non\_rtp\_call (0)

89058: Jun 20 04:39:43.408: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89101: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Call Disconnect: Initiated at: 0x260070A, Originated at:0x260070B, Cause Code = 1

89102: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

89103: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_CC\_CALL\_DISCONNECT, Current State = STATE\_RECD\_INVITE

89104: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_RECD\_INVITE, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89105: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89106: Jun 20 04:39:43.464: //144654/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 172.17.40.8:5060 to 172.17.40.137:5060

SIP/2.0 404 Not Found

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>;tag=F6654CA-4A1

Date: Thu, 20 Jun 2024 04:39:41 GMT

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Warning: 399 172.17.40.8 "No matching outgoing dial-peer"

Server: Cisco-SIPGateway/IOS-17.6.1a

Reason: Q.850;cause=1

Session-ID: 00000000000000000000000000000000;remote=347f91a300105000a0003891b747f240

Content-Length: 0

89108: Jun 20 04:39:43.480: //144654/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 172.17.40.137:5060 to 172.17.40.8:5060

ACK sip:9@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK3b2920f6

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001f903a930b5-6d8e77fa

To: <sip:9@172.17.40.8>;tag=F6654CA-4A1

Call-ID: 3891b747-f2400010-284ab59e-5e415f9c@172.17.40.137

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Max-Forwards: 70

Date: Thu, 20 Jun 2024 04:39:43 GMT

CSeq: 101 ACK

Content-Length: 0

89109: Jun 20 04:39:43.480: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_NEW\_MESSAGE, Current State = STATE\_DISCONNECTING

89110: Jun 20 04:39:43.480: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_delete\_dp\_session (0)

89111: Jun 20 04:39:43.480: //144654/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_call\_disconnect\_done (0)

89112: Jun 20 04:39:43.480: //144654/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DEAD, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89113: Jun 20 04:39:43.482: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Error: sipSPIFlushDeferredQueue: Invalid deferredQueue

89114: Jun 20 04:39:43.482: //144654/F173CA84817B/CUBE\_VT/SIP/MISC/Error: ws\_call\_fork\_cleanup: ws\_info is NULL

89115: Jun 20 04:39:43.482: //144654/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_release\_port (10704)

Jun 20 04:39:52.475: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

INVITE sip:0@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

Max-Forwards: 70

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:52 GMT

CSeq: 101 INVITE

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Expires: 180

Accept: application/sdp

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO

Remote-Party-ID: "IT" <sip:187@172.17.40.8>;party=calling;id-type=subscriber;privacy=off;screen=yes

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Allow-Events: kpml,dialog

Recv-Info: conference

Recv-Info: x-cisco-conference

Content-Length: 351

Content-Type: application/sdp

Content-Disposition: session;handling=optional

v=0

o=Cisco-SIPUA 26940 0 IN IP4 172.17.40.137

s=SIP Call

b=AS:4064

t=0 0

m=audio 24180 RTP/AVP 0 8 116 18 101

c=IN IP4 172.17.40.137

b=TIAS:64000

a=rtpmap:0 PCMU/8000

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=sendrecv

Jun 20 04:39:52.480: //144659/F81E555E8187/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 100 Trying

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>

Date: Thu, 20 Jun 2024 04:39:52 GMT

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Session-ID: 00000000000000000000000000000000;remote=23f3e7ad00105000a0003891b747f240

Content-Length: 0

Jun 20 04:39:52.481: //144659/F81E555E8187/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 484 Address Incomplete

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>;tag=F667801-B10

Date: Thu, 20 Jun 2024 04:39:52 GMT

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Reason: Q.850;cause=28

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=25d07e1704455cb092dbf8d5c2d9af82

Content-Length: 0

Jun 20 04:39:52.534: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

ACK sip:0@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>;tag=F667801-B10

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=23f3e7ad00105000a0003891b747f240

Max-Forwards: 70

Date: Thu, 20 Jun 2024 04:39:52 GMT

CSeq: 101 ACK

Content-Length: 0

89147: Jun 20 04:39:53.360: //144659/F81E555E8187/

------------------ Cover Buffer ---------------

Search-key = 187:0:144659

Timestamp = Jun 20 04:39:52.474

CallID = 144659

Peer-CallID = NA

Correlator = NA

Called-Number = 0

Calling-Number = 187

SIP CallID = 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

SIP SessionID =

GUID = F81E555E8187

-----------------------------------------------

89117: Jun 20 04:39:52.474: //144659/F81E555E8187/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 172.17.40.137:5060 to 172.17.40.8:5060

INVITE sip:0@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

Max-Forwards: 70

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:52 GMT

CSeq: 101 INVITE

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DF88-FDE@172.17.40.137:5060;transport=udp>;+u.sip!devicename.ccm.cisco.com="SEP3891B747F240"

Expires: 180

Accept: application/sdp

Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO

Remote-Party-ID: "IT" <sip:187@172.17.40.8>;party=calling;id-type=subscriber;privacy=off;screen=yes

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Allow-Events: kpml,dialog

Recv-Info: conference

Recv-Info: x-cisco-conference

Content-Length: 351

Content-Type: application/sdp

Content-Disposition: session;handling=optional

v=0

o=Cisco-SIPUA 26940 0 IN IP4 172.17.40.137

s=SIP Call

b=AS:4064

t=0 0

m=audio 24180 RTP/AVP 0 8 116 18 101

c=IN IP4 172.17.40.137

b=TIAS:64000

a=rtpmap:0 PCMU/8000

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=sendrecv

89121: Jun 20 04:39:52.475: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_NONE, Next State = STATE\_IDLE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89122: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Matched Dialpeer: Dir:Inbound, Peer-Tag: 40014

89123: Jun 20 04:39:52.478: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/Offer-Answer: Event = E\_SIP\_INVITE\_SDP\_RCVD, Current State = S\_SIP\_EARLY\_DIALOG\_IDLE, Next State = S\_SIP\_EARLY\_DIALOG\_OFFER\_RCVD

89124: Jun 20 04:39:52.478: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_RCVD\_SDP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = S\_SIP\_IWF\_SDP\_RCVD\_AWAIT\_PEER\_EVENT

89125: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Media Stream Parameters: Stream Type = voice-only, Stream State = STREAM\_ADDING Negotiated Codec = g711ulaw, Negotiated DTMF Type = inband-voice, Stream Index = 1

89126: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

89127: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/API: voip\_rtp\_allocate\_port (10710)

89128: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Media Stream Parameters: Stream Type = voice-only, Stream State = STREAM\_ADDING Negotiated Codec = g711ulaw, Negotiated DTMF Type = inband-voice, Stream Index = 1

89129: Jun 20 04:39:52.477: //144659/F81E555E8187/CUBE\_VT/SIP/API: cc\_api\_call\_setup\_ind\_with\_callID (0)

89130: Jun 20 04:39:52.478: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_IDLE, Next State = STATE\_RECD\_INVITE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89131: Jun 20 04:39:52.479: //144659/F81E555E8187/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 172.17.40.8:5060 to 172.17.40.137:5060

SIP/2.0 100 Trying

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>

Date: Thu, 20 Jun 2024 04:39:52 GMT

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Session-ID: 00000000000000000000000000000000;remote=23f3e7ad00105000a0003891b747f240

Content-Length: 0

89132: Jun 20 04:39:52.479: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Call Disconnect: Initiated at: 0x260070A, Originated at:0x260070B, Cause Code = 28

89133: Jun 20 04:39:52.479: //144659/F81E555E8187/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

89134: Jun 20 04:39:52.479: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_CC\_CALL\_DISCONNECT, Current State = STATE\_RECD\_INVITE

89135: Jun 20 04:39:52.479: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_RECD\_INVITE, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89136: Jun 20 04:39:52.480: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89137: Jun 20 04:39:52.481: //144659/F81E555E8187/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 172.17.40.8:5060 to 172.17.40.137:5060

SIP/2.0 484 Address Incomplete

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>;tag=F667801-B10

Date: Thu, 20 Jun 2024 04:39:52 GMT

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

CSeq: 101 INVITE

Allow-Events: telephone-event

Server: Cisco-SIPGateway/IOS-17.6.1a

Reason: Q.850;cause=28

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=25d07e1704455cb092dbf8d5c2d9af82

Content-Length: 0

89139: Jun 20 04:39:52.535: //144659/F81E555E8187/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 172.17.40.137:5060 to 172.17.40.8:5060

ACK sip:0@172.17.40.8;user=phone SIP/2.0

Via: SIP/2.0/UDP 172.17.40.137:5060;branch=z9hG4bK0821807a

From: "IT" <sip:187@172.17.40.8>;tag=3891b747f24001fc318792ab-3c79302c

To: <sip:0@172.17.40.8>;tag=F667801-B10

Call-ID: 3891b747-f2400012-292e8882-1628d6bd@172.17.40.137

Session-ID: 23f3e7ad00105000a0003891b747f240;remote=23f3e7ad00105000a0003891b747f240

Max-Forwards: 70

Date: Thu, 20 Jun 2024 04:39:52 GMT

CSeq: 101 ACK

Content-Length: 0

89140: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_NEW\_MESSAGE, Current State = STATE\_DISCONNECTING

89141: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/API: voip\_rtp\_release\_port (10710)

89142: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/API: cc\_api\_call\_disconnect\_done (0)

89143: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DEAD, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89144: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Error: sipSPIFlushDeferredQueue: Invalid deferredQueue

89145: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/MISC/Error: ws\_call\_fork\_cleanup: ws\_info is NULL

89146: Jun 20 04:39:52.534: //144659/F81E555E8187/CUBE\_VT/SIP/API: voip\_rtp\_release\_port (10710)

Jun 20 04:39:58.958: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

REGISTER sip:172.17.40.8 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.166:5060;branch=z9hG4bK4a887e05

From: <sip:101@172.17.40.8>;tag=8c1e809a247867803ebe3600-0f96c7d1

To: <sip:101@172.17.40.8>

Call-ID: 8c1e809a-247800de-5c78849e-07c68358@172.17.40.166

Max-Forwards: 70

Session-ID: 9f8b934000105000a0008c1e809a2478;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:39:59 GMT

CSeq: 26218 REGISTER

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DE67-1791@172.17.40.166:5060;transport=udp>;+sip.instance="<urn:uuid:00000000-0000-0000-0000-8c1e809a2478>";+u.sip!devicename.ccm.cisco.com="SEP8C1E809A2478";+u.sip!model.ccm.cisco.com="622"

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Content-Length: 0

Expires: 3600

Jun 20 04:39:58.960: //144660/FBFBB5FC818C/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/UDP 172.17.40.166:5060;branch=z9hG4bK4a887e05

From: <sip:101@172.17.40.8>;tag=8c1e809a247867803ebe3600-0f96c7d1

To: <sip:101@172.17.40.8>;tag=F669150-1F8

Date: Thu, 20 Jun 2024 04:39:58 GMT

Call-ID: 8c1e809a-247800de-5c78849e-07c68358@172.17.40.166

Server: Cisco-SIPGateway/IOS-17.6.1a

CSeq: 26218 REGISTER

Supported: X-cisco-cme-sis-9.0.0

Supported: X-cisco-srtp-fallback

Contact: <sip:101@172.17.40.166:5060>;expires=120

Expires: 120

Content-Length: 0

VTZ\_ISR\_4331#

Jun 20 04:40:04.000: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

REGISTER sip:172.17.40.8 SIP/2.0

Via: SIP/2.0/UDP 172.17.40.135:5060;branch=z9hG4bK36f28fe3

From: <sip:143@172.17.40.8>;tag=3891b747f1bd3a5b40cb4409-0fa2088e

To: <sip:143@172.17.40.8>

Call-ID: 3891b747-f1bd0076-3b2e011b-3e79d575@172.17.40.135

Max-Forwards: 70

Session-ID: b9db464000105000a0003891b747f1bd;remote=00000000000000000000000000000000

Date: Thu, 20 Jun 2024 04:40:06 GMT

CSeq: 14815 REGISTER

User-Agent: Cisco-CP7841/14.0.1

Contact: <sip:1DF28-BE2@172.17.40.135:5060;transport=udp>;+sip.instance="<urn:uuid:00000000-0000-0000-0000-3891b747f1bd>";+u.sip!devicename.ccm.cisco.com="SEP3891B747F1BD";+u.sip!model.ccm.cisco.com="622"

Supported: replaces,join,sdp-anat,norefersub,resource-priority,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-7.0.0,X-cisco-xsi-8.5.1

Content-Length: 0

Expires: 3600

Jun 20 04:40:04.003: //144661/FEFD10BD818D/SIP/Msg/ccsipDisplayMsg:

Sent:

u allSIP/2.0 200 OK

Via: SIP/2.0/UDP 172.17.40.135:5060;branch=z9hG4bK36f28fe3

From: <sip:143@172.17.40.8>;tag=3891b747f1bd3a5b40cb4409-0fa2088e

To: <sip:143@172.17.40.8>;tag=F66A502-9EA

Date: Thu, 20 Jun 2024 04:40:04 GMT

Call-ID: 3891b747-f1bd0076-3b2e011b-3e79d575@172.17.40.135

Server: Cisco-SIPGateway/IOS-17.6.1a

CSeq: 14815 REGISTER

Supported: X-cisco-cme-sis-9.0.0

Supported: X-cisco-srtp-fallback

Contact: <sip:143@172.17.40.135:5060>;expires=120

Expires: 120

Content-Length: 0

All possible debugging has been turned off

VTZ\_ISR\_4331#u all

All possible debugging has been turned off

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#

VTZ\_ISR\_4331#

89152: Jun 20 04:40:16.366: //144655/F173CA84817B/

------------------ Cover Buffer ---------------

Search-key = +918914560050:89:144655

Timestamp = Jun 20 04:39:43.383

CallID = 144655

Peer-CallID = 144654

Correlator = NA

Called-Number = 89

Calling-Number = +918914560050

SIP CallID = F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

SIP SessionID =

GUID = F173CA84817B

-----------------------------------------------

89002: Jun 20 04:39:43.383: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Matched Dialpeer: Dir:Outbound, Peer-Tag: 300

89003: Jun 20 04:39:43.383: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_NONE, Next State = STATE\_IDLE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89004: Jun 20 04:39:43.383: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_SET\_MODE, Current State = CNFSM\_CONTAINER\_STATE, Next State = CNFSM\_NO\_STATE\_CHANGE

89005: Jun 20 04:39:43.383: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_PRE\_SETUP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = CNFSM\_NO\_STATE\_CHANGE

89011: Jun 20 04:39:43.383: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_PEER\_MULTIMEDIA\_CHANNEL\_IND, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = CNFSM\_NO\_STATE\_CHANGE

89012: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Media Stream Parameters: Stream Type = voice-only, Stream State = STREAM\_ADDING Negotiated Codec = No Codec , Negotiated DTMF Type = inband-voice, Stream Index = 1

89013: Jun 20 04:39:43.385: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_allocate\_port (10706)

89014: Jun 20 04:39:43.385: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Media-State: Event = E\_IPIP\_MEDIA\_SERV\_EV\_PEER\_CHNL\_IND, Current State = S\_IPIP\_MEDIA\_SERV\_STATE\_IDLE, Next State = S\_IPIP\_MEDIA\_SERV\_STATE\_INIT\_XCODER\_RESERVED

89015: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Software-Error: Type: Error in Transcoder Reservation, Code-location:0x30040D0

89016: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/API: ccsip\_xcoder\_reserve (-1)

89017: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_CONTINUE\_PRE\_SETUP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = CNFSM\_NO\_STATE\_CHANGE

89018: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_INIT\_CALL\_SETUP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = CNFSM\_NO\_STATE\_CHANGE

89019: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_create\_session (0)

89020: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_set\_non\_rtp\_call (0)

89021: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89022: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

89023: Jun 20 04:39:43.384: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_CC\_CALL\_SETUP, Current State = STATE\_IDLE

89024: Jun 20 04:39:43.385: //144655/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_call\_proceeding (0)

89025: Jun 20 04:39:43.385: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Offer-Answer: Event = E\_SIP\_INVITE\_SDP\_SENT, Current State = S\_SIP\_EARLY\_DIALOG\_IDLE, Next State = S\_SIP\_EARLY\_DIALOG\_OFFER\_SENT

89026: Jun 20 04:39:43.385: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/IWF: Event = E\_SIP\_IWF\_EV\_SENT\_SDP, Current State = S\_SIP\_IWF\_SDP\_IDLE, Next State = S\_SIP\_IWF\_SDP\_SENT\_AWAIT\_SDP

89027: Jun 20 04:39:43.386: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_IDLE, Next State = STATE\_SENT\_INVITE, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89028: Jun 20 04:39:43.386: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89029: Jun 20 04:39:43.386: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_set\_non\_rtp\_call (0)

89030: Jun 20 04:39:43.386: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_update\_callinfo (0)

89031: Jun 20 04:39:43.386: //144655/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 10.125.41.230:5060 to 10.5.109.147:5060

INVITE sip:89@10.5.109.147:5060 SIP/2.0

Via: SIP/2.0/UDP 10.125.41.230:5060;branch=z9hG4bK103BDFA5

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

To: <sip:89@10.5.109.147>

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Min-SE: 1800

Cisco-Guid: 4050897540-0771035631-2172384107-3192134464

User-Agent: Cisco-SIPGateway/IOS-17.6.1a

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

CSeq: 101 INVITE

Timestamp: 1718858383

Contact: <sip:+918914560050@10.125.41.230:5060>

Expires: 180

Allow-Events: telephone-event

Max-Forwards: 69

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 250

v=0

o=CiscoSystemsSIP-GW-UserAgent 1482 6820 IN IP4 10.125.41.230

s=SIP Call

c=IN IP4 10.125.41.230

t=0 0

m=audio 10706 RTP/AVP 0 101

c=IN IP4 10.125.41.230

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

89034: Jun 20 04:39:43.405: //144655/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 10.5.109.147:5060 to 10.125.41.230:5060

SIP/2.0 100 Trying

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Via: SIP/2.0/UDP 10.125.41.230:5060;received=10.125.41.230;branch=z9hG4bK103BDFA5

To: <sip:89@10.5.109.147>

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

CSeq: 101 INVITE

Date: Thu, 20 Jun 2024 04:39:43 GMT

Timestamp: 1718858383

Content-Length: 0

89035: Jun 20 04:39:43.405: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_NEW\_MESSAGE, Current State = STATE\_SENT\_INVITE

89036: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_SENT\_INVITE, Next State = STATE\_RECD\_PROCEEDING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_SETUP\_BUFFERED

89037: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Received: SIP UDP message from 10.5.109.147:5060 to 10.125.41.230:5060

SIP/2.0 407 Proxy Authentication Required

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Via: SIP/2.0/UDP 10.125.41.230:5060;received=10.125.41.230;branch=z9hG4bK103BDFA5

To: <sip:89@10.5.109.147>;tag=662bf1c3-6673b28f17a44738

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

CSeq: 101 INVITE

Date: Thu, 20 Jun 2024 04:39:43 GMT

Warning: 399 apa37.org "IP association no match, user not registered"

Content-Length: 0

89038: Jun 20 04:39:43.405: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_NEW\_MESSAGE, Current State = STATE\_RECD\_PROCEEDING

89039: Jun 20 04:39:43.405: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Offer-Answer: Event = E\_SIP\_OFFER\_ANSWER\_RESET, Current State = S\_SIP\_EARLY\_DIALOG\_OFFER\_SENT, Next State = S\_SIP\_EARLY\_DIALOG\_IDLE

89040: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_RECD\_PROCEEDING, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_SETUP\_BUFFERED, Next Sub-State = STATE\_NONE

89041: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Call Disconnect: Initiated at: 0x1701CA8, Originated at:0x5A07E89, Cause Code = 47

89042: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_call\_disconnected (0)

89043: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DISCONNECTING, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89044: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Call Disconnect: Initiated at: 0x260070A, Originated at:0x260070B, Cause Code = 47

89045: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_update\_interface\_cac\_resource (0)

89046: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Event-Action: Event = SIPSPI\_EV\_CC\_CALL\_DISCONNECT, Current State = STATE\_DISCONNECTING

89047: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Call Disconnect: Initiated at: 0x1702FDC, Originated at:0x5A07E89, Cause Code = 47

89048: Jun 20 04:39:43.406: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_delete\_dp\_session (0)

89049: Jun 20 04:39:43.408: //144655/F173CA84817B/CUBE\_VT/SIP/API: cc\_api\_call\_disconnect\_done (0)

89050: Jun 20 04:39:43.408: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/SPI-State-Change: Current State = STATE\_DISCONNECTING, Next State = STATE\_DEAD, Current Sub-State = STATE\_NONE, Next Sub-State = STATE\_NONE

89082: Jun 20 04:39:43.415: //144655/F173CA84817B/CUBE\_VT/SIP/Msg/ccsipDisplayMsg:

Sent: SIP UDP message from 10.125.41.230:5060 to 10.5.109.147:5060

ACK sip:89@10.5.109.147:5060 SIP/2.0

Via: SIP/2.0/UDP 10.125.41.230:5060;branch=z9hG4bK103BDFA5

From: "IT" <sip:+918914560050@10.125.41.230>;tag=F66547B-D18

To: <sip:89@10.5.109.147>;tag=662bf1c3-6673b28f17a44738

Date: Thu, 20 Jun 2024 04:39:43 GMT

Call-ID: F2B3764F-2DF511EF-8182F36B-BE441B40@10.125.41.230

Max-Forwards: 70

CSeq: 101 ACK

Allow-Events: telephone-event

Session-ID: 347f91a300105000a0003891b747f240;remote=00000000000000000000000000000000

Content-Length: 0

89148: Jun 20 04:40:15.408: //144655/F173CA84817B/CUBE\_VT/SIP/FSM/Timer-Action: Event = SIP\_TIMER\_REMOVE\_TRANSACTION, Current State = STATE\_DEAD

89149: Jun 20 04:40:15.408: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Error: sipSPIFlushDeferredQueue: Invalid deferredQueue

89150: Jun 20 04:40:15.408: //144655/F173CA84817B/CUBE\_VT/SIP/MISC/Error: ws\_call\_fork\_cleanup: ws\_info is NULL

89151: Jun 20 04:40:15.408: //144655/F173CA84817B/CUBE\_VT/SIP/API: voip\_rtp\_release\_port (10706)