ip host ap.ims.airtel.in 10.5.109.147

ip name-server 172.17.40.63 172.16.10.51 8.8.8.8

voice service voip

ip address trusted list

ipv4 172.17.27.59

ipv4 192.168.5.8

ipv4 172.17.40.8

ipv4 10.125.41.230

ipv4 10.5.109.147

ipv4 10.5.64.98

ipv4 10.5.64.99

ipv4 10.5.64.114

ipv4 10.5.64.115

ipv4 10.5.64.66

ipv4 10.5.64.67

ipv4 10.5.64.82

ipv4 10.5.64.83

--More-- allow-connections h323 to h323

allow-connections h323 to sip

allow-connections sip to h323

allow-connections sip to sip

no supplementary-service sip moved-temporarily

no supplementary-service sip refer

supplementary-service media-renegotiate

fax protocol t38 version 0 ls-redundancy 0 hs-redundancy 0 fallback none

trace

sip

registrar server expires max 120 min 60

!

!

voice class uri PSTN sip

host ipv4:10.5.109.147

voice class codec 1

codec preference 1 g711ulaw

!

!

voice class sip-profiles 1

request INVITE sip-header P-Asserted-Identity modify "ap.ims.airtel.in" "10.5.109.147"

request INVITE sip-header From modify "ap.ims.airtel.in" "10.5.109.147"

--More-- !

!

!

voice class tenant 3

registrar 1 ipv4:10.5.109.147:5060 expires 3600

credentials username +918914560050 password xxxx realm ap.ims.airtel.in

authentication username +918914560050 password xxxx realm ap.ims.airtel.in

no remote-party-id

retry invite 4

retry response 3

retry bye 2

retry cancel 2

retry register 5

timers register 250

sip-server ipv4:10.5.109.147

connection-reuse via-port

bind control source-interface GigabitEthernet0/0/2

bind media source-interface GigabitEthernet0/0/2

outbound-proxy ipv4:10.5.109.147:5060

!

!

--More-- !

voice register global

mode cme

source-address 172.17.40.8 port 5600

max-dn 200

max-pool 100

timezone 39

date-format D/M/Y

create profile sync 0015144571460343

auto-register

!

!

voice register dn 1

number 101

name Reception

label Reception

!

voice register pool 3

busy-trigger-per-button 2

id mac 3891.B747.F1E6

type 7841

number 1 dn 3

dtmf-relay cisco-rtp

username Ipphone183 password xxxx

!

!

voice translation-rule 1

rule 1 /^9\(.\*\)/ /\1/

!

voice translation-rule 2

rule 1 /.\*/ /8914560050/

!

voice translation-rule 3

rule 1 /918914560050/ /187/

!

voice translation-rule 100

rule 1 /918914560050/ /187/

rule 2 /918914560051/ /190/

--More-- !

!

voice translation-profile INCOMING

translate called 3

!

voice translation-profile OUTGOING

translate calling 2

translate called 1

interface GigabitEthernet0/0/0

ip address 172.17.40.8 255.255.255.0

negotiation auto

!

interface GigabitEthernet0/0/1

ip address 172.49.53.22 255.255.255.252

negotiation auto

!

interface GigabitEthernet0/0/2

ip address 10.125.41.230 255.255.255.252

negotiation auto

!

ip http server

ip http authentication local

ip http secure-server

ip http client source-interface GigabitEthernet0/0/0

ip http path flash:CME\_GUI

ip forward-protocol nd

ip route 0.0.0.0 0.0.0.0 172.17.40.1

ip route 10.5.64.0 255.255.255.0 10.125.41.229

ip route 10.5.109.0 255.255.255.0 10.125.41.229

ip route 172.17.24.0 255.255.252.0 172.49.53.21

ip route 172.17.27.0 255.255.255.0 172.49.53.21

ip route 172.38.44.0 255.255.255.0 172.49.53.21

ip route 192.168.5.0 255.255.255.0 172.49.53.21

!

!

mgcp behavior rsip-range tgcp-only

mgcp behavior comedia-role none

mgcp behavior comedia-check-media-src disable

mgcp behavior comedia-sdp-force disable

!

mgcp profile default

!

!

!

!

telephony-service

max-ephones 50

--More-- max-dn 100

ip source-address 172.17.40.8 port 2000

time-zone 39

date-format dd-mm-yy

max-conferences 8 gain -6

transfer-system full-consult

directory entry 1 187 name IT

create cnf-files version-stamp 7960 Jun 17 2024 10:26:13

!

!

dspfarm profile 1 transcode universal

associate application CUBE

shutdown

!

dial-peer voice 900 voip

description KolCUCM

destination-pattern 9..

session protocol sipv2

session target ipv4:172.17.27.59

session transport tcp

incoming called-number 1..

voice-class sip bind control source-interface GigabitEthernet0/0/0

voice-class sip bind media source-interface GigabitEthernet0/0/0

--More-- dtmf-relay rtp-nte

codec g711ulaw

!

dial-peer voice 1 voip

description KkdCME

destination-pattern 8..

session protocol sipv2

session target ipv4:192.168.5.8

incoming called-number 1..

voice-class sip bind control source-interface GigabitEthernet0/0/0

voice-class sip bind media source-interface GigabitEthernet0/0/0

dtmf-relay rtp-nte

codec g711ulaw

!

dial-peer voice 300 voip

description \*Outbound Calls\*

translation-profile outgoing OUTGOING

destination-pattern 9[2-9].........

session protocol sipv2

session target ipv4:10.5.109.147

voice-class codec 1

voice-class sip early-offer forced

voice-class sip profiles 1

--More-- voice-class sip tenant 3

dtmf-relay rtp-nte

no vad

!

dial-peer voice 500 voip

description \*Inbound calls\*

translation-profile incoming INCOMING

session protocol sipv2

incoming called-number .%

incoming uri via PSTN

voice-class codec 1

voice-class sip transport switch udp tcp

voice-class sip early-offer forced

voice-class sip tenant 3

dtmf-relay rtp-nte

no vad

!

!

sip-ua

retry invite 2

timers trying 300

registrar ipv4:10.125.41.229 expires 3600

registrar dns:ap.ims.airtel.in expires 3600 secondary

--More-- connection-reuse

g729-annexb override

ntp server time.cloudflare.com

ntp server 0.in.pool.ntp.org