VG224_D#show run
Building configuration...

Current configuration : 3119 bytes
!
version 12.4
service config
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname VG224_D
!
boot-start-marker
boot system slot0:vg224-i6s-mz.124-9.T2.bin
boot-end-marker
!
logging buffered 5000000 debugging
no logging console
enable secret ..................(removed)
enable password .................(removed)
!
no aaa new-model
!
resource policy
!
clock timezone CST -6
clock summer-time CST date Mar 11 2007 2:00 Nov 4 2007 2:00
ip domain name bchealth.info
!
!
!
stcapp ccm-group 1
stcapp
!
voice-card 0
 dsp services dspfarm
!
!
!
!
!
!
!
username r00t privilege 15 password 0 bchcadmin
!

!
interface FastEthernet0/0
 ip address 10.0.0.168 255.255.255.0
 duplex auto
 speed auto
 vlan-range dot1q 23 23
  description VoIP_23_VLAN
  exit-vlan-config
 !
!
interface FastEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
!
ip default-gateway 10.0.0.254
ip route 0.0.0.0 0.0.0.0 10.0.0.175
!
ip http server
ip http access-class 23
!
snmp-server community BCHVG224D RO
!
!
control-plane
!
!
voice-port 2/0
 cptone C1
!
voice-port 2/1
 cptone C1
!
voice-port 2/2
!
voice-port 2/3
 cptone C1
!
voice-port 2/4
 cptone C1
!
voice-port 2/5
 cptone C1
!
voice-port 2/6
 cptone C1
!
voice-port 2/7
 cptone C1
!
voice-port 2/8
!
voice-port 2/9
 cptone C1
!
voice-port 2/10
!
voice-port 2/11
!
voice-port 2/12
!
voice-port 2/13
!
voice-port 2/14
!
voice-port 2/15
!
voice-port 2/16
!
voice-port 2/17
!
voice-port 2/18
!
voice-port 2/19
!
voice-port 2/20
!
voice-port 2/21
!
voice-port 2/22
!
voice-port 2/23
!
ccm-manager redundant-host 10.0.0.177
ccm-manager mgcp
no ccm-manager fax protocol cisco
ccm-manager music-on-hold
ccm-manager config server 10.0.0.176
ccm-manager config
ccm-manager config dialpeer-prefix
ccm-manager download-tones
!
mgcp
mgcp call-agent 10.0.0.176 2427 service-type mgcp version 0.1
mgcp dtmf-relay voip codec all mode out-of-band
mgcp rtp unreachable timeout 1000 action notify
mgcp modem passthrough voip mode nse
mgcp package-capability rtp-package
no mgcp package-capability res-package
mgcp package-capability sst-package
no mgcp package-capability fxr-package
no mgcp timer receive-rtcp
mgcp sdp simple
mgcp fax t38 inhibit
mgcp rtp payload-type g726r16 static
mgcp bind control source-interface FastEthernet0/0
mgcp bind media source-interface FastEthernet0/0
!
mgcp profile default
!
!
!
dial-peer voice 99920 pots
 service mgcpapp
 port 2/0
!
dial-peer voice 99921 pots
 service mgcpapp
 port 2/1
!
dial-peer voice 99923 pots
 service mgcpapp
 port 2/3
!
dial-peer voice 99924 pots
 service mgcpapp
 port 2/4
!
dial-peer voice 99925 pots
 service mgcpapp
 port 2/5
!
dial-peer voice 99926 pots
 service mgcpapp
 port 2/6
!
dial-peer voice 99927 pots
 service mgcpapp
 port 2/7
!
dial-peer voice 99929 pots
 service mgcpapp
 port 2/9
!
!
gateway
 timer receive-rtp 600
!
banner motd ^CVG224D^C
!
line con 0
 login local
line aux 0
line vty 0 4
 access-class 23 in
 privilege level 15
 password bchcadmin
 login local
 transport input telnet
!
ntp clock-period 17179885
ntp server 192.5.41.40
end