Show Run 

Current configuration : 3544 bytes                                  
! 
version 12.4            
service timestamps debug datetim                              
service timestamps log datetime msec                                    
no service password-encryption                              
! 
hostname ROUTER_BKE-TP                      
! 
boot-start-marker                 
boot-end-marker               
! 
enable password pr0p3l                      
! 
no aaa new-model                
network-clock-participate wic 2                               
! 
! 
ip cef      
! 
! 
no ip domain lookup                   
isdn switch-type primary-qsig                             
! 
voice-card 0            
 no dspfarm           
! 
! 
voice call carrier capacity active                                  
! 
voice service voip                  
 signaling forward rawmsg                         
 sip    
! 
! 
voice class codec 1                   
 codec preference 2 g711ulaw                            
! 
! 
! 
! 
! 
! 
! 
! 
! 
! 
! 
archive       
 log config           
  hidekeys          
! 
! 
controller E1 0/2/0                   
 pri-group timeslot                  
! 
! 
class-map match-any AutoQoS-VoIP-Remark                                       
 match ip dscp ef                 
 match ip dscp cs3                  
 match ip dscp af31                   
class-map match-any AutoQoS-VoIP-Control-UnTrust                                                
 match access-group name AutoQoS-VoIP-Control                                             
class-map match-any AutoQoS-VoIP-RTP-UnTrust                                            
 match protocol rtp audio                         
 match access-group name AutoQoS-VoIP-RTCP                                          
! 
! 
policy-map AutoQoS-Policy-UnTrust                                 
 class AutoQoS-VoIP-RTP-UnTrust                               
  priority percent 70                     
  set dscp ef             
 class AutoQoS-VoIP-Control-UnTrust                                   
  bandwidth percent 5                     
  set dscp af31               
 class AutoQoS-VoIP-Remark                          
  set dscp default                  
 class class-default                    
  fair-queue            
! 
! 
! 
! 
interface Loopback0                   
 ip address 10.192.1.28 255.255.255.255                                       
! 
interface FastEthernet0/0                         
 description Connect to PBX                           
 ip address 172.16.4.2 255.255.255.0                                    
 shutdown         
 duplex auto            
 speed auto           
! 
interface FastEthernet0/1                         
 description Connect to CAT3750E BKE                                    
 ip address 10.192.33.9 255.255.255.252                                       
 duplex auto            
 speed auto           
! 
interface Serial0/1/0                     
 description Connect To TM Leased Line                                      
 bandwidth 2048               
 ip address 10.192.33.6 255.255.255.252                                       
 ip tcp header-compression i                          
 auto qos voip              
 service-policy output AutoQoS-Policy-UnTrust                                             
 ip rtp header-compression iphc-format                                      
 ip rsvp bandwidth 1024 1024                            
! 
interface Serial0/2/0:15                        
 no ip address              
 encapsulation hdlc                   
 no logging event link-status                             
 isdn switch-type primary-qsig                              
 isdn overlap-receiving                       
 isdn incoming-voice voice                          
 isdn send-alerting                   
 isdn bchan-number-order ascending                                  
 isdn sending-complete                      
 isdn outgoing display-ie                         
 no cdp enable              
! 
router eigrp 101                
 network 10.0.0.0                 
 network 192.0.0.0                  
 network 200.1.2.0                  
 no auto-summary                
! 
ip forward-protocol nd                      
! 
! 
ip http server              
no ip http secure-server                        
! 
ip access-list extended AutoQoS-VoIP-Control                                            
 permit tcp any any eq 1720                           
 permit tcp any any range 11000 11999                                     
 permit udp any any eq 2427                           
 permit tcp any any eq 2428                           
 permit tcp any any range 2000 2002                                   
 permit udp any any eq 1719                           
 permit udp any any eq 5060                           
ip access-list extended AutoQoS-VoIP-RTCP                                         
 permit udp any any range 16384 32767                                     
! 
! 
! 
! 
control-plane             
! 
rmon event 33333 log trap AutoQoS description "AutoQoS SNMP traps for Voice Drop                                                                                
s" owner Au         
rmon alarm 33333 cbQosCMDropBitRate.1169.1171 30 absolute rising-threshold 1 333                                                                                
33 falling-threshold 0 owner AutoQoS                                    
! 
! 
voice-port 0/0/0                
! 
voice-port 0/0/1                
! 
voice-port 0/0/2                
! 
voice-port 0/0/3                
! 
voice-port 0/2/0:15                   
! 
! 
! 
! 
! 
dial-peer voice 1 voip                      
 description ROUTER_BKE-TP to ROUTER_BRT-RCC                                            
 destination-pattern ....                         
 signaling forward rawmsg                         
 session protocol sipv2                       
 session target ipv4:10.192.1.29                                
 req-qos guaranteed-delay                         
 codec g711ulaw               
! 
dial-peer voice 2015 pots                         
 description ROUTER_BKE-TP to PBX_BKE-TP                                        
 destination-pattern ....                         
 direct-inward-dial                   
 port 0/2/0:15              
 forward-digits all
!
gateway
 timer receive-rtp 1200
!
sip-ua
 reason-header override
!
!
!
line con 0
 password cisco
 login
line aux 0
line vty 0 4
 password cisco
 login
!
exception data-corruption buffer truncate
scheduler allocate 20000 1000
!
end

ROUTER_BKE-TP#sh int
FastEthernet0/0 is administratively down, line protocol is down
  Hardware is MV96340 Ethernet, address is 0023.04e6.e138 (bia 0023.04e6.e138)
  Description: Connect to PBX
  Internet address is 172.16.4.2/24
  MTU 1500 bytes, BW 100000 Kbit, DLY 100 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation ARPA, loopback not set
  Keepalive set (10 sec)
  Auto-duplex, Auto Speed, 100BaseTX/FX
  ARP type: ARPA, ARP Timeout 04:00:00
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: fifo
  Output queue: 0/40 (size/max)
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored
     0 watchdog
     0 input packets with dribble condition detected
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 babbles, 0 late collision, 0 deferred
     0 lost carrier, 0 no carrier
     0 output buffer failures, 0 output buffers swapped out
FastEthernet0/1 is up, line protocol is up
  Hardware is MV96340 Ethernet, address is 0023.04e6.e139 (bia 0023.04e6.e139)
  Description: Connect to CAT3750E BKE
  Internet address is 10.192.33.9/30
  MTU 1500 bytes, BW 100000 Kbit, DLY 100 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation ARPA, loopback not set
  Keepalive set (10 sec)
  Full-duplex, 100Mb/s, 100BaseTX/FX
  ARP type: ARPA, ARP Timeout 04:00:00
  Last input 00:00:00, output 00:00:00, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: fifo
  Output queue: 0/40 (size/max)
  5 minute input rate 18000 bits/sec, 14 packets/sec
  5 minute output rate 323000 bits/sec, 26 packets/sec
     80886557 packets input, 1833249218 bytes
     Received 1569833 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored
     0 watchdog
     0 input packets with dribble condition detected
     108862124 packets output, 91329044 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 babbles, 0 late collision, 0 deferred
     0 lost carrier, 0 no carrier
     0 output buffer failures, 0 output buffers swapped out
Serial0/1/0 is up, line protocol is up
  Hardware is GT96K Serial
  Description: Connect To TM Leased Line
  Internet address is 10.192.33.6/30
  MTU 1500 bytes, BW 2048 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 42/255
  Encapsulation HDLC, loopback not set
  Keepalive set (10 sec)
  Last input 00:00:00, output 00:00:00, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 338
  Queueing strategy: Class-based queueing
  Output queue: 0/1000/64/221 (size/max total/threshold/drops)
     Conversations  0/12/256 (active/max active/max total)
     Reserved Conversations 1/1 (allocated/max allocated)
     Available Bandwidth 1 kilobits/sec
  5 minute input rate 338000 bits/sec, 44 packets/sec
  5 minute output rate 11000 bits/sec, 42 packets/sec
     120697166 packets input, 3998173608 bytes, 0 no buffer
     Received 785945 broadcasts, 0 runts, 3 giants, 0 throttles
     717 input errors, 717 CRC, 74 frame, 17 overrun, 0 ignored, 233 abort
     94366870 packets output, 1603461867 bytes, 0 underruns
     0 output errors, 0 collisions, 357 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     136 carrier transitions
     DCD=up  DSR=up  DTR=up  RTS=up  CTS=up
Serial0/2/0:0 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:1 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:2 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:3 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:4 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:5 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:6 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:7 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:8 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:9 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:10 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:11 is down, line protocol is down
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Keepalive not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/0/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
Serial0/2/0:15 is up, line protocol is up (spoofing)
  Hardware is DSX1
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation HDLC, loopback not set
  Last input 00:00:02, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: weighted fair
  Output queue: 0/1000/64/0 (size/max total/threshold/drops)
     Conversations  0/1/256 (active/max active/max total)
     Reserved Conversations 0/0 (allocated/max allocated)
     Available Bandwidth 48 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     914018 packets input, 4667441 bytes, 0 no buffer
     Received 0 broadcasts, 1186 runts, 0 giants, 0 throttles
     24130 input errors, 24130 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     914093 packets output, 4269778 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out
     145 carrier transitions
  Timeslot(s) Used:16, SCC: 0, Transmitter delay is 0 flags
Loopback0 is up, line protocol is up
  Hardware is Loopback
  Internet address is 10.192.1.28/32
  MTU 1514 bytes, BW 8000000 Kbit, DLY 5000 usec,
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation LOOPBACK, loopback not set
  Last input 00:00:03, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: fifo
  Output queue: 0/0 (size/max)
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     1458240 packets output, 87494400 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 unknown protocol drops
     0 output buffer failures, 0 output buffers swapped out

ROUTER_BKE-TP#sh ver
Cisco IOS Software, 2800 Software (C2800NM-ENTSERVICESK9-M), Version 12.4(19b),
RELEASE SOFTWARE (fc1)
Technical Support: http://www.cisco.com/techsupport
Copyright (c) 1986-2008 by Cisco Systems, Inc.
Compiled Fri 13-Jun-08 04:12 by prod_rel_team

ROM: System Bootstrap, Version 12.4(13r)T, RELEASE SOFTWARE (fc1)

ROUTER_BKE-TP uptime is 11 weeks, 1 day, 2 hours, 16 minutes
System returned to ROM by power-on
System image file is "flash:c2800nm-entservicesk9-mz.124-19b.bin"

Cisco 2811 (revision 53.51) with 249856K/12288K bytes of memory.
Processor board ID FHK1242F1JU
2 FastEthernet interfaces
13 Serial interfaces
1 Serial(sync/async) interface
1 Channelized E1/PRI port
4 Voice FXO interfaces
DRAM configuration is 64 bits wide with parity enabled.
239K bytes of non-volatile configuration memory.
62720K bytes of ATA CompactFlash (Read/Write)

Configuration register is 0x2102

ROUTER_BKE-TP#sh diag
Slot 0:
        C2811 Motherboard with 2FE and integrated VPN Port adapter, 2 ports
        Port adapter is analyzed
        Port adapter insertion time 11w1d ago
        EEPROM contents at hardware discovery:
        PCB Serial Number        : FOC12414Q5T
        Hardware Revision        : 1.0
        Top Assy. Part Number    : 800-26920-05
        Board Revision           : A0
        Deviation Number         : 0
        Fab Version              : 04
        RMA Test History         : 00
        RMA Number               : 0-0-0-0
        RMA History              : 00
        Processor type           : 87
        Hardware date code       : 20081012
        Chassis Serial Number    : FHK1242F1JU
        Chassis MAC Address      : 0023.04e6.e138
        MAC Address block size   : 24
        CLEI Code                : COMWL10CRA
        Product (FRU) Number     : CISCO2811
        Part Number              : 73-10258-05
        Version Identifier       : V06
        EEPROM format version 4
        EEPROM contents (hex):
          0x00: 04 FF C1 8B 46 4F 43 31 32 34 31 34 51 35 54 40
          0x10: 03 E7 41 01 00 C0 46 03 20 00 69 28 05 42 41 30
          0x20: 88 00 00 00 00 02 04 03 00 81 00 00 00 00 04 00
          0x30: 09 87 83 01 32 69 74 C2 8B 46 48 4B 31 32 34 32
          0x40: 46 31 4A 55 C3 06 00 23 04 E6 E1 38 43 00 18 C6
          0x50: 8A 43 4F 4D 57 4C 31 30 43 52 41 CB 8F 43 49 53
          0x60: 43 4F 32 38 31 31 20 20 20 20 20 20 82 49 28 12
          0x70: 05 89 56 30 36 20 D9 02 40 C1 FF FF FF FF FF FF

        PVDM Slot 0:
        16-channel (G.711) Voice/Fax PVDMII DSP SIMM PVDM daughter card
        Hardware Revision        : 4.0
        Part Number              : 73-8538-05
        Board Revision           : B0
        Deviation Number         : 0
        Fab Version              : 04
        PCB Serial Number        : FOC123848H1
        RMA Test History         : 00
        RMA Number               : 0-0-0-0
        RMA History              : 00
        Processor type           : 00
        Product (FRU) Number     : PVDM2-16
        Version Identifier       : V01
        EEPROM format version 4
        EEPROM contents (hex):
          0x00: 04 FF 40 03 EF 41 04 00 82 49 21 5A 05 42 42 30
          0x10: 88 00 00 00 00 02 04 C1 8B 46 4F 43 31 32 33 38
          0x20: 34 38 48 31 03 00 81 00 00 00 00 04 00 09 00 CB
          0x30: 88 50 56 44 4D 32 2D 31 36 89 56 30 31 20 D9 02
          0x40: 40 C1 FF FF FF FF FF FF FF FF FF FF FF FF FF FF
          0x50: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
          0x60: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
          0x70: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF

        WIC Slot 0:
        2nd generation - FXO Voice daughter card (4 port)
        Hardware Revision        : 5.0
        Top Assy. Part Number    : 800-21589-04
        Board Revision           : A0
        Deviation Number         : 0-0
        Fab Version              : 04
        PCB Serial Number        : FOC123647M9
        RMA Test History         : 00
        RMA Number               : 0-0-0-0
        RMA History              : 00
        Product (FRU) Number     : VIC2-4FXO
        Version Identifier       : V03
        CLEI Code                : CNUIAXJAAB
        EEPROM format version 4
        EEPROM contents (hex):
          0x00: 04 FF 40 00 4C 41 05 00 C0 46 03 20 00 54 55 04
          0x10: 42 41 30 80 00 00 00 00 02 04 C1 8B 46 4F 43 31
          0x20: 32 33 36 34 37 4D 39 03 00 81 00 00 00 00 04 00
          0x30: CB 89 56 49 43 32 2D 34 46 58 4F 89 56 30 33 20
          0x40: C6 8A 43 4E 55 49 41 58 4A 41 41 42 FF FF FF FF
          0x50: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
          0x60: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
          0x70: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF

        WIC Slot 1:
        Serial 1T WAN daughter card
        Hardware revision 1.0           Board revision D0
        Serial number     36495884      Part number    800-01514-02
        FRU Part Number     WIC-1T=
        Test history      0x0           RMA number     00-00-00
        Connector type    Wan Module
        EEPROM format version 1
        EEPROM contents (hex):
          0x20: 01 02 01 00 02 2C E2 0C 50 05 EA 02 00 00 00 00
          0x30: 68 00 00 00 08 05 22 01 FF FF FF FF FF FF FF FF

        WIC Slot 2:
        E1 (1 port) Multi-Flex Trunk WAN daughter card
        Hardware revision 1.0           Board revision B0
        Serial number     29804746      Part number    800-04475-03
        FRU Part Number     VWIC-1MFT-E1=
        Test history      0x0           RMA number     00-00-00
        Connector type    PCI
        EEPROM format version 1
        EEPROM contents (hex):
          0x20: 01 21 01 00 01 C6 C8 CA 50 11 7B 03 00 00 00 00
          0x30: 58 00 00 00 03 02 12 00 FF FF FF FF FF FF FF FF