OAKFH_HG1_F#show frame pvc

PVC Statistics for interface Serial0/0 (Frame Relay DTE)

              Active     Inactive      Deleted       Static
  Local          1            1            0            0
  Switched       0            0            0            0
  Unused         1          190            0            0

DLCI = 17, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:05, last time pvc status changed 11:42:05

DLCI = 23, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:05, last time pvc status changed 11:42:05

DLCI = 25, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:17, last time pvc status changed 09:18:17

DLCI = 29, DLCI USAGE = LOCAL, PVC STATUS = INACTIVE, INTERFACE = Serial0/0.2

  input pkts 0             output pkts 15           in bytes 0
  out bytes 733            dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 5         out bcast bytes 433
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  pvc create time 9w3d, last time pvc status changed 11:41:48

DLCI = 31, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:17, last time pvc status changed 09:18:17

DLCI = 32, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:48, last time pvc status changed 11:41:48

DLCI = 33, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:20, last time pvc status changed 09:19:20

DLCI = 36, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:17, last time pvc status changed 09:18:17

DLCI = 45, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:48, last time pvc status changed 11:41:48

DLCI = 49, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:20, last time pvc status changed 09:19:20

DLCI = 50, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:05, last time pvc status changed 11:42:05

DLCI = 53, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:20, last time pvc status changed 09:19:20

DLCI = 55, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:48, last time pvc status changed 11:41:48

DLCI = 62, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:48, last time pvc status changed 11:38:48

DLCI = 65, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:05, last time pvc status changed 11:42:05

DLCI = 73, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:20, last time pvc status changed 09:19:20

DLCI = 78, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:05, last time pvc status changed 11:42:05

DLCI = 81, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:18, last time pvc status changed 09:17:18

DLCI = 83, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:49, last time pvc status changed 11:38:49

DLCI = 85, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:19, last time pvc status changed 09:17:19

DLCI = 87, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:17, last time pvc status changed 09:18:17

DLCI = 96, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 100, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 113, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 117, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 120, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 123, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 129, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 134, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 137, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 142, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 145, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:49, last time pvc status changed 11:41:49

DLCI = 152, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 161, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:19, last time pvc status changed 09:17:19

DLCI = 163, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:49, last time pvc status changed 11:41:49

DLCI = 164, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:19, last time pvc status changed 09:17:19

DLCI = 167, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 169, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 172, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:21, last time pvc status changed 09:19:21

DLCI = 173, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:21, last time pvc status changed 09:19:21

DLCI = 176, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:50, last time pvc status changed 11:38:50

DLCI = 177, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:21, last time pvc status changed 09:19:21

DLCI = 179, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 189, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 190, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:06, last time pvc status changed 11:42:06

DLCI = 191, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:18, last time pvc status changed 09:18:18

DLCI = 192, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:50, last time pvc status changed 11:41:50

DLCI = 193, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 200, DLCI USAGE = LOCAL, PVC STATUS = ACTIVE, INTERFACE = Serial0/0.1

  input pkts 32480770      output pkts 29322324     in bytes 2847934488
  out bytes 1663085686     dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 65216       in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 1092176   out bcast bytes 88684713
  5 minute input rate 3000 bits/sec, 4 packets/sec
  5 minute output rate 3000 bits/sec, 3 packets/sec
  pvc create time 9w3d, last time pvc status changed 09:08:20

DLCI = 202, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 211, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:50, last time pvc status changed 11:41:50

DLCI = 215, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:19, last time pvc status changed 09:18:19

DLCI = 217, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 224, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:20, last time pvc status changed 09:17:20

DLCI = 225, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:20, last time pvc status changed 09:17:20

DLCI = 234, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:20, last time pvc status changed 09:17:20

DLCI = 241, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 249, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:50, last time pvc status changed 11:41:50

DLCI = 252, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:19, last time pvc status changed 09:18:19

DLCI = 257, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 258, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 262, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 273, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:22, last time pvc status changed 09:19:22

DLCI = 275, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:50, last time pvc status changed 11:41:50

DLCI = 282, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 289, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:22, last time pvc status changed 09:19:22

DLCI = 292, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 293, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:50, last time pvc status changed 11:38:50

DLCI = 295, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:20, last time pvc status changed 09:17:20

DLCI = 305, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 306, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:21, last time pvc status changed 09:17:21

DLCI = 309, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 321, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 322, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:19, last time pvc status changed 09:18:19

DLCI = 330, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:51, last time pvc status changed 11:41:51

DLCI = 334, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:19, last time pvc status changed 09:18:19

DLCI = 337, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 339, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 343, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:51, last time pvc status changed 11:41:51

DLCI = 350, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 353, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:07, last time pvc status changed 11:42:07

DLCI = 366, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:21, last time pvc status changed 09:17:21

DLCI = 368, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 369, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:22, last time pvc status changed 09:19:22

DLCI = 370, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 376, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:23, last time pvc status changed 09:19:23

DLCI = 385, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:51, last time pvc status changed 11:41:51

DLCI = 398, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:51, last time pvc status changed 11:41:51

DLCI = 402, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:51, last time pvc status changed 11:38:51

DLCI = 410, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:23, last time pvc status changed 09:19:23

DLCI = 415, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 419, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 425, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:23, last time pvc status changed 09:19:23

DLCI = 428, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:23, last time pvc status changed 09:19:23

DLCI = 432, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 433, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 434, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:21, last time pvc status changed 09:17:21

DLCI = 445, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 449, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 450, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 457, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 458, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:52, last time pvc status changed 11:38:52

DLCI = 459, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:22, last time pvc status changed 09:17:22

DLCI = 466, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 469, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 473, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:20, last time pvc status changed 09:18:20

DLCI = 480, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:52, last time pvc status changed 11:41:52

DLCI = 481, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:08, last time pvc status changed 11:42:08

DLCI = 482, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:23, last time pvc status changed 09:19:23

DLCI = 485, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 488, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 500, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 504, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:22, last time pvc status changed 09:17:22

DLCI = 512, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 513, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 514, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:22, last time pvc status changed 09:17:22

DLCI = 529, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 530, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:24, last time pvc status changed 09:19:24

DLCI = 531, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 535, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 538, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 545, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 547, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:52, last time pvc status changed 11:41:52

DLCI = 548, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 561, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 565, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:52, last time pvc status changed 11:38:52

DLCI = 578, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:24, last time pvc status changed 09:19:24

DLCI = 584, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 594, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 601, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 608, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:24, last time pvc status changed 09:19:24

DLCI = 609, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 625, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:24, last time pvc status changed 09:19:24

DLCI = 633, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:23, last time pvc status changed 09:17:23

DLCI = 640, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 641, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 654, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:21, last time pvc status changed 09:18:21

DLCI = 657, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:53, last time pvc status changed 11:41:53

DLCI = 660, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:23, last time pvc status changed 09:17:23

DLCI = 673, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:09, last time pvc status changed 11:42:09

DLCI = 674, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:24, last time pvc status changed 09:19:24

DLCI = 680, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:23, last time pvc status changed 09:17:23

DLCI = 684, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 689, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:23, last time pvc status changed 09:17:23

DLCI = 697, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 701, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:53, last time pvc status changed 11:41:53

DLCI = 713, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 714, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 721, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 731, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 732, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 736, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 737, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:53, last time pvc status changed 11:38:53

DLCI = 741, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:22, last time pvc status changed 09:18:22

DLCI = 744, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:22, last time pvc status changed 09:18:22

DLCI = 745, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:22, last time pvc status changed 09:18:22

DLCI = 748, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 757, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:24, last time pvc status changed 09:17:24

DLCI = 761, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 769, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 774, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:22, last time pvc status changed 09:18:22

DLCI = 775, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:54, last time pvc status changed 11:41:54

DLCI = 785, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 786, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 793, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 795, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:22, last time pvc status changed 09:18:22

DLCI = 799, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 801, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:10, last time pvc status changed 11:42:10

DLCI = 804, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:25, last time pvc status changed 09:19:25

DLCI = 805, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:54, last time pvc status changed 11:38:54

DLCI = 807, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:54, last time pvc status changed 11:41:54

DLCI = 816, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 821, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 832, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 834, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 865, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:23, last time pvc status changed 09:18:23

DLCI = 866, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 881, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:54, last time pvc status changed 11:41:54

DLCI = 885, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 888, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:19:26, last time pvc status changed 09:19:26

DLCI = 889, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:23, last time pvc status changed 09:18:23

DLCI = 896, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:38:54, last time pvc status changed 11:38:54

DLCI = 905, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 913, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 945, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:24, last time pvc status changed 09:17:24

DLCI = 952, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 965, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 970, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:17:24, last time pvc status changed 09:17:24

DLCI = 977, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:42:11, last time pvc status changed 11:42:11

DLCI = 984, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:55, last time pvc status changed 11:41:55

DLCI = 988, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 09:18:23, last time pvc status changed 09:18:23

DLCI = 1000, DLCI USAGE = UNUSED, PVC STATUS = INACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 11:41:55, last time pvc status changed 11:41:55

DLCI = 1007, DLCI USAGE = UNUSED, PVC STATUS = ACTIVE, INTERFACE = Serial0/0

  input pkts 0             output pkts 0            in bytes 0
  out bytes 0              dropped pkts 0           in pkts dropped 0
  out pkts dropped 0                out bytes dropped 0
  in FECN pkts 0           in BECN pkts 0           out FECN pkts 0
  out BECN pkts 0          in DE pkts 0             out DE pkts 0
  out bcast pkts 0         out bcast bytes 0
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
  switched pkts 0
  Detailed packet drop counters:
  no out intf 0            out intf down 0          no out PVC 0
  in PVC down 0            out PVC down 0           pkt too big 0
  shaping Q full 0         pkt above DE 0           policing drop 0
  pvc create time 9w3d, last time pvc status changed 11:41:55