version 12.4
service timestamps debug uptime
service timestamps log datetime msec localtime
no service password-encryption
!
hostname chester
!
boot-start-marker
boot-end-marker
!
logging buffered 4096 debugging
enable secret 5.
enable password
!
no aaa new-model
memory-size iomem 25
clock timezone CST -6
clock summer-time CDT recurring
!
!
no ip cef
no ip domain lookup
!
!
ip sla monitor 1
 type echo protocol ipIcmpEcho 172.31.0.1
 timeout 1000
 threshold 2
 frequency 3
ip sla monitor schedule 1 life forever start-time now
!
chat-script dialout ABORT ERROR ABORT BUSY "" "AT" OK "ATDT \T" TIMEOUT 45 CONNE

modemcap entry EXT_MODEM:MSC=&F1S0=0M0
!
!
voice service voip
!
!
voice class codec 10
 codec preference 1 g729r8
 codec preference 2 g711ulaw
!
username lse_3640 password 0 rmtdialbkup
!
track 123 rtr 1 reachability
!
translation-rule 1
 Rule 1 ^5 035
 Rule 2 ^4 034
 Rule 3 ^2 032
 Rule 4 ^7 737
 Rule 5 ^9 939
!
interface Loopback0
 ip address 10.10.3.1 255.255.255.0
!
interface FastEthernet0/0
 no ip address
 ip helper-address 10.3.2.2
 no ip mroute-cache
 duplex auto
 speed auto
 no keepalive
!
interface FastEthernet0/0.2
 description workstations vlan 2
 encapsulation dot1Q 2
 ip address 10.3.2.16 255.255.255.0
!
interface FastEthernet0/0.3
 description tsunami vlan 3
 encapsulation dot1Q 3
 ip address 10.3.3.16 255.255.255.0
!
interface FastEthernet0/0.4
 description phones vlan 4
 encapsulation dot1Q 4
 ip address 10.3.4.16 255.255.255.0
!
interface FastEthernet0/0.5
 description wirelesss vlan 5
 encapsulation dot1Q 5
 ip address 10.3.5.16 255.255.255.0
 ip helper-address 10.3.2.2
!
interface FastEthernet0/0.6
 description management vlan 6
 encapsulation dot1Q 6 native
 ip address 10.3.6.16 255.255.255.0
!
interface FastEthernet0/0.7
 description guest vlan 7
 encapsulation dot1Q 7
 ip address 10.3.7.16 255.255.255.0
 ip access-group 195 in
 ip helper-address 10.3.2.2
!
interface FastEthernet0/1
 ip address 172.31.0.3 255.255.255.0
 duplex auto
 speed auto
!
interface Async129
 ip address 172.22.3.4 255.255.255.0
 ip access-group 105 out
 encapsulation ppp
 dialer in-band
 dialer idle-timeout 30
 dialer map ip 172.22.3.3 name lse_3640 broadcast 15555551212
 dialer map ip 172.31.0.0 name lse_3640 broadcast 15555551212
 dialer watch-disable 30
 dialer watch-group 10
 dialer-group 1
 async mode dedicated
 ppp authentication chap
 routing dynamic
!
router eigrp 100
 redistribute static
 network 10.3.2.0 0.0.0.255
 network 10.3.3.0 0.0.0.255
 network 10.3.4.0 0.0.0.255
 network 10.3.5.0 0.0.0.255
 network 10.3.6.0 0.0.0.255
 network 10.3.7.0 0.0.0.255
 network 10.10.3.0 0.0.0.255
 network 172.22.3.0 0.0.0.255
 network 172.31.0.0 0.0.0.255
 no auto-summary
 no eigrp log-neighbor-changes
!
no ip http server
ip flow-export source FastEthernet0/0
ip flow-export destination 10.3.6.12 2055
!
no ip forward-protocol nd
ip forward-protocol udp 5246
ip forward-protocol udp 5247
ip forward-protocol udp echo
ip route 0.0.0.0 0.0.0.0 10.3.2.8
!
!
access-list 105 deny   tcp any any eq www
access-list 105 deny   tcp any any eq smtp
access-list 105 deny   tcp any any eq pop3
access-list 105 permit ip any any
access-list 105 deny   tcp any any eq 8080
access-list 105 permit icmp any host 172.31.0.1 echo
access-list 195 permit tcp any host 10.3.2.1 eq domain
access-list 195 permit udp any host 10.3.2.1 eq domain
access-list 195 permit udp any eq bootpc host 10.3.2.2 eq bootps
access-list 195 permit udp any eq bootps host 10.3.2.2 eq bootps
access-list 195 permit udp any eq bootps host 10.3.2.2 eq bootpc
access-list 195 permit ip 10.3.7.0 0.0.0.255 10.1.7.0 0.0.0.255
access-list 195 permit ip 10.3.7.0 0.0.0.255 host 10.1.2.8
access-list 195 deny   ip any 10.0.0.0 0.255.255.255
access-list 195 permit ip any any
dialer-list 1 protocol ip deny
snmp-server community public RO
snmp-server enable traps snmp authentication linkdown linkup
snmp-server enable traps config
snmp-server host 10.3.2.2 public
!
!
!
control-plane
!
bridge 2 protocol dec
!
!
voice-port 1/0/0
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
voice-port 1/0/1
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
voice-port 1/1/0
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
voice-port 1/1/1
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
voice-port 2/0/0
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
voice-port 2/0/1
 operation 4-wire
 type 2
 output attenuation 1
 no comfort-noise
 timeouts wait-release 3
!
dial-peer cor custom
!
dial-peer voice 101 pots
 preference 1
 destination-pattern 3..
 no digit-strip
 port 1/0/1
!
dial-peer voice 102 pots
 preference 2
 destination-pattern 3..
 no digit-strip
 port 1/1/0
!
dial-peer voice 103 pots
 preference 3
 destination-pattern 3..
 no digit-strip
 port 1/1/1
!
dial-peer voice 200 voip
 destination-pattern 2..
 session target ipv4:10.8.2.2
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 500 voip
 destination-pattern 5..
 translate-outgoing called 1
 session target ipv4:172.31.0.1
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 700 voip
 destination-pattern 7...
 translate-outgoing called 1
 session target ipv4:172.31.0.1
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 900 voip
 destination-pattern 9.......
 translate-outgoing called 1
 session target ipv4:172.31.0.1
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 1 voip
 voice-class codec 10
 incoming called-number .
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 400 voip
 destination-pattern 4..
 session target ipv4:172.31.0.4
 dtmf-relay h245-signal h245-alphanumeric
 no vad
!
dial-peer voice 104 pots
 preference 4
 destination-pattern 3..
 no digit-strip
 port 2/0/0
!
dial-peer voice 105 pots
 preference 5
 destination-pattern 3..
 no digit-strip
 port 2/0/1
!
dial-peer voice 100 pots
 destination-pattern 3..
 no digit-strip
 port 1/0/0
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
 exec-timeout 0 0
 script dialer dialout
 modem InOut
 modem autoconfigure type EXT_MODEM
 transport input all
 stopbits 1
 speed 115200
 flowcontrol hardware
line vty 0 4
 password 
 login
!
ntp clock-period 17180055
ntp server 10.1.2.2
!
end