version 15.1

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname xxx

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

memory-size iomem 10

crypto pki token default removal timeout 0

!

!

ip source-route

!

!

!

!

ip cef

no ipv6 cef

!

!

license udi pid CISCO887VA-K9 sn FCZ1706908Q

!

!

!

controller VDSL 0

!

!

bridge irb

!

!

!

!

interface Ethernet0

no ip address

shutdown

no fair-queue

!

interface ATM0

no ip address

ip virtual-reassembly in

no atm ilmi-keepalive

pvc 0/38

encapsulation aal5mux ppp dialer

dialer pool-member 1

!

!

interface FastEthernet0

switchport access vlan 2

no ip address

!

interface FastEthernet1

no ip address

!

interface FastEthernet2

no ip address

!

interface FastEthernet3

no ip address

!

interface Vlan1

interface Vlan1

no ip address

shutdown

!

interface Vlan2

no ip address

bridge-group 1

bridge-group 1 input-address-list 700

bridge-group 1 output-address-list 700

!

interface Dialer0

ip address xxx.xxx.xxx.xxx xxx.xxx.xxx.xxx

ip mtu 1492

ip nat outside

ip virtual-reassembly in

encapsulation ppp

dialer pool 1

ppp authentication chap callin

ppp chap hostname xxx

ppp chap password 0 xxxv

ppp ipcp route default

ppp ipcp address accept

no cdp enable

!

interface BVI1

ip address 192.168.1.1 255.255.255.0

!

ip forward-protocol nd

ip http server

no ip http secure-server

!

ip nat inside source list 1 interface Dialer0 overload

ip route 0.0.0.0 0.0.0.0 Dialer0

ip route xxx.xxx.xxx.xxx xxx.xxx.xxx.xxx Dialer0

!

access-list 700 permit 0000.0000.0000 ffff.ffff.ffff

dialer-list 1 protocol ip permit

!

!

!

!

!

line con 0

line aux 0

line vty 0 4

login

transport input all

!

end