Current configuration : 4734 bytes
!
version 12.4
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname Cisco877
!
boot-start-marker
boot-end-marker
!
enable secret 5 ********************************
!
no aaa new-model
clock timezone acst 9 30
clock summer-time acst recurring 1 Sun Oct 2:00 1 Sun Apr 2:00
!
crypto pki trustpoint TP-self-signed-152119483
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-152119483
 revocation-check none
 rsakeypair TP-self-signed-152119483
!
!
crypto pki certificate chain TP-self-signed-152119483
 certificate self-signed 01
  30820251 308201BA A0030201 02020101 300D0609 2A864886 F70D0101 04050030
  30312E30 2C060355 04031325 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31353231 31393438 33301E17 0D303230 33303130 30323431
  385A170D 32303031 30313030 30303030 5A303031 2E302C06 03550403 1325494F
  532D5365 6C662D53 69676E65 642D4365 72746966 69636174 652D3135 32313139
  34383330 819F300D 06092A86 4886F70D 01010105 0003818D 00308189 02818100
  A3CD4BBC 82A01A88 5D40A1B5 6A75680A ABE77A66 3AD8F7CA CC4CB032 3611F8B0
  19074D33 66752E15 215E47DA 13DB1CB3 2DDDEE07 52FF9109 657A8BEB 0BBD34CA
  F080A990 026C8CA3 2CC2C6A1 6668C88E 4DE25C2B 22017FB5 A32718DC 7DE81FFD
  BAEEEA5E CE334574 2A6676D4 FB206F7A 7BC292B3 E67A56F1 D736C80A FBF51E6F
  02030100 01A37B30 79300F06 03551D13 0101FF04 05300301 01FF3026 0603551D
  11041F30 1D821B43 6973636F 3837372E 6E657470 6F70756C 61726573 2E6C6F63
  616C301F 0603551D 23041830 16801490 B0B8513E F48EE6D3 181AEC75 BFFBE711
  5A191330 1D060355 1D0E0416 041490B0 B8513EF4 8EE6D318 1AEC75BF FBE7115A
  1913300D 06092A86 4886F70D 01010405 00038181 009D7AAC 382DFE78 CD2800F8
  92785082 70244016 8C714314 3A54D019 26D244B1 A4447FA6 31ECB622 919A8124
  BC902E2D 60D93CF0 65552084 6A4D2B5E 5CE1CAFD 9F5DE3A9 9836A6BB AF4A77AC
  0EE97396 34654776 A4452399 494BAB4A BEB59405 15D52F62 5DAFBDC6 771E4701
  609E0367 3D2E888A 4206D12F AEED8014 68B32B7B 7D
        quit
dot11 syslog
!
dot11 ssid Corazon
   vlan 1
   authentication open
   authentication key-management wpa
   guest-mode
   wpa-psk ascii 7 ********************************
!
no ip source-route
ip cef
no ip dhcp use vrf connected
ip dhcp excluded-address 192.168.0.1 192.168.0.15
!
ip dhcp pool dpool1
   import all
   network 192.168.0.0 255.255.255.0
   default-router 192.168.0.1
   lease infinite
   update arp
!
!
ip auth-proxy max-nodata-conns 3
ip admission max-nodata-conns 3
no ip bootp server
no ip domain lookup
ip domain name belong.com.au
ip name-server 208.67.222.222
ip name-server 208.67.220.220
!
!
!
!
!
archive
 log config
  hidekeys
!
!
!
bridge irb
!
!
interface ATM0
 description ----- ADSL Connection ----
 no ip address
 ip virtual-reassembly
 no atm ilmi-keepalive
 pvc 8/35
  tx-ring-limit 3
  encapsulation aal5snap
  pppoe-client dial-pool-number 1
 !
 dsl operating-mode auto
!
interface FastEthernet0
!
interface FastEthernet1
!
interface FastEthernet2
!
interface FastEthernet3
!
interface Dot11Radio0
 no ip address
 !
 encryption vlan 1 mode ciphers aes-ccm
 !
 encryption mode ciphers aes-ccm
 !
 broadcast-key vlan 1 change 45
 !
 !
 ssid Corazon
 !
 speed basic-1.0 basic-2.0 basic-5.5 6.0 9.0 basic-11.0 12.0 18.0 24.0 36.0 48.0 54.0
 station-role root
 no cdp enable
!
interface Dot11Radio0.1
 encapsulation dot1Q 1 native
 ip virtual-reassembly
 no cdp enable
 bridge-group 1
 bridge-group 1 subscriber-loop-control
 bridge-group 1 spanning-disabled
 bridge-group 1 block-unknown-source
 no bridge-group 1 source-learning
 no bridge-group 1 unicast-flooding
!
interface Vlan1
 no ip address
 ip virtual-reassembly
 bridge-group 1
!
interface Dialer0
 description ---- ADSL ----
 ip address 144.138.131.214 255.255.255.0
 no ip redirects
 no ip unreachables
 ip mtu 1492
 ip nat outside
 ip virtual-reassembly
 encapsulation ppp
 dialer pool 1
 dialer-group 1
 no cdp enable
 ppp chap hostname 571549@belong.com.au
 ppp chap password 7 ********************************
!
interface BVI1
 ip address 192.168.0.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly
 ip tcp adjust-mss 1452
!
ip forward-protocol nd
ip route 0.0.0.0 0.0.0.0 Dialer0
!
no ip http server
no ip http secure-server
ip nat inside source list NAT interface Dialer0 overload
!
ip access-list extended NAT
 permit ip 192.168.0.0 0.0.0.255 any
!
dialer-list 1 protocol ip permit
!
!
!
control-plane
!
bridge 1 protocol ieee
bridge 1 route ip
!
line con 0
 password 7 ********************************
 logging synchronous
 login
 no modem enable
line aux 0
line vty 0 4
 password 7 ********************************
 logging synchronous
 login local
 transport input ssh
!
scheduler max-task-time 5000
end