Router B 2-12-19
!
!
interface GigabitEthernet0/0/0
 no ip address
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 192.168.2.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/2
 ip address 192.168.3.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial1/0/0
 ip address 100.100.100.2 255.255.255.0
 dsu bandwidth 44210
 framing c-bit
 cablelength 10
 no cdp enable
!
interface Serial2/0/0
 ip address 200.200.200.1 255.255.255.0
 dsu bandwidth 44210
 framing c-bit
 cablelength 10
 no cdp enable
!
interface GigabitEthernet0
 vrf forwarding Mgmt-intf
 ip address 194.169.1.65 255.255.255.0
 negotiation auto
!
interface Vlan1
 no ip address
 shutdown
!
ip forward-protocol nd
no ip http server
no ip http secure-server
ip route 0.0.0.0 0.0.0.0 100.100.100.1
ip route 192.168.1.0 255.255.255.0 100.100.100.1
ip route 192.168.4.0 255.255.255.0 200.200.200.2
ip route 192.168.5.0 255.255.255.0 200.200.200.2
!
!
!
!
!