CE

*******************************************************************************
router bgp 7
 template peer-session SECURITY-SESSION_EBGP
  remote-as 1
 exit-peer-session
 !
 template peer-session DATA-SESSION_EBGP
  remote-as 1
 exit-peer-session
 !
 no synchronization
 bgp router-id 192.168.50.7
 bgp log-neighbor-changes
 no auto-summary
 !
 address-family ipv4 vrf SECURITY
 neighbor 192.168.60.3 inherit peer-session SECURITY-SESSION_EBGP
 neighbor 192.168.60.3 activate
 neighbor 192.168.60.3 soft-reconfiguration inbound
 no synchronization
 network 172.16.50.7 mask 255.255.255.255
 network 172.16.50.8 mask 255.255.255.255
 network 192.168.50.7 mask 255.255.255.255
 network 192.168.60.0
 exit-address-family
 !        
 address-family ipv4 vrf PHONE
 no synchronization
 exit-address-family
 !        
 address-family ipv4 vrf DATA
 redistribute static route-map MY_LOCAL
 redistribute eigrp 100
 neighbor 192.168.61.3 inherit peer-session DATA-SESSION_EBGP
 neighbor 192.168.61.3 activate
 neighbor 192.168.61.3 soft-reconfiguration inbound
 no synchronization
 network 10.55.55.0 mask 255.255.255.0
 network 172.16.51.7 mask 255.255.255.255
 network 172.16.51.8 mask 255.255.255.255
 network 192.168.51.7 mask 255.255.255.255
 network 192.168.61.0
 exit-address-family

************************************************************************************
R7#sh ip bgp vpnv4 vrf DATA
BGP table version is 17, local router ID is 192.168.50.7
Status codes: s suppressed, d damped, h history, * valid, > best, i - internal,
              r RIB-failure, S Stale
Origin codes: i - IGP, e - EGP, ? - incomplete

   Network          Next Hop            Metric LocPrf Weight Path
Route Distinguisher: 20:20 (default for vrf DATA)
*> 172.16.51.7/32   0.0.0.0                  0         32768 i
*> 172.16.51.8/32   0.0.0.0                  0         32768 i
*> 192.168.51.7/32  0.0.0.0                  0         32768 i
*> 192.168.61.0     0.0.0.0                  0         32768 i
R7#
R7#

************************************************************************************

R7#sh ip bgp vpnv4 vrf SECURITY
BGP table version is 17, local router ID is 192.168.50.7
Status codes: s suppressed, d damped, h history, * valid, > best, i - internal,
              r RIB-failure, S Stale
Origin codes: i - IGP, e - EGP, ? - incomplete

   Network          Next Hop            Metric LocPrf Weight Path
Route Distinguisher: 10:10 (default for vrf SECURITY)
*> 172.16.50.7/32   0.0.0.0                  0         32768 i
*> 172.16.50.8/32   0.0.0.0                  0         32768 i
*> 192.168.50.7/32  0.0.0.0                  0         32768 i
*> 192.168.60.0     0.0.0.0                  0         32768 i

************************************************************************************

R7#sh ip bgp vpnv4 vrf DATA summary 
BGP router identifier 192.168.50.7, local AS number 7
BGP table version is 17, main routing table version 17
4 network entries using 548 bytes of memory
4 path entries using 272 bytes of memory
3/2 BGP path/bestpath attribute entries using 372 bytes of memory
2 BGP extended community entries using 274 bytes of memory
0 BGP route-map cache entries using 0 bytes of memory
0 BGP filter-list cache entries using 0 bytes of memory
BGP using 1466 total bytes of memory
BGP activity 8/0 prefixes, 8/0 paths, scan interval 15 secs

Neighbor        V    AS MsgRcvd MsgSent   TblVer  InQ OutQ Up/Down  State/PfxRcd
192.168.61.3    4     1      19      19       17    0    0 00:14:32        0

************************************************************************************

Neighbor        V    AS MsgRcvd MsgSent   TblVer  InQ OutQ Up/Down  State/PfxRcd
192.168.61.3    4     1      19      19       17    0    0 00:14:32        0
R7#
R7#
R7#
R7#sh ip bgp vpnv4 vrf SECURITY summary 
BGP router identifier 192.168.50.7, local AS number 7
BGP table version is 17, main routing table version 17
4 network entries using 548 bytes of memory
4 path entries using 272 bytes of memory
3/2 BGP path/bestpath attribute entries using 372 bytes of memory
2 BGP extended community entries using 274 bytes of memory
0 BGP route-map cache entries using 0 bytes of memory
0 BGP filter-list cache entries using 0 bytes of memory
BGP using 1466 total bytes of memory
BGP activity 8/0 prefixes, 8/0 paths, scan interval 15 secs

Neighbor        V    AS MsgRcvd MsgSent   TblVer  InQ OutQ Up/Down  State/PfxRcd
192.168.60.3    4     1      19      19       17    0    0 00:14:46        0

************************************************************************************
R7#sh ip bgp vpnv4 vrf DATA neighbors 192.168.61.3 received-routes 

Total number of prefixes 0 
************************************************************************************
R7#sh ip bgp vpnv4 vrf SECURITY neighbors 192.168.60.3 received-routes 

Total number of prefixes 0 
*************************************************************************************