FW1# packet-tracer input InterstingTrafficInterface icmp 10.45.54.13(siteA) 0 0 100.100.226.10(siteC) de

Phase: 1
Type: ACCESS-LIST
Subtype:
Result: ALLOW
Config:
Implicit Rule
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xaf255f70, priority=1, domain=permit, deny=false
        hits=42709, user_data=0x0, cs_id=0x0, l3_type=0x8
        src mac=0000.0000.0000, mask=0000.0000.0000
        dst mac=0000.0000.0000, mask=0100.0000.0000
        input_ifc=Tablet, output_ifc=any

Phase: 2
Type: ROUTE-LOOKUP
Subtype: input
Result: ALLOW
Config:
Additional Information:
in   0.0.0.0         0.0.0.0         Outside

Phase: 3
Type: NAT
Subtype: per-session
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xad9acd08, priority=0, domain=nat-per-session, deny=true
        hits=5286844, user_data=0x0, cs_id=0x0, reverse, use_real_addr, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=any, output_ifc=any

Phase: 4
Type: IP-OPTIONS
Subtype:
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xae0c0f68, priority=0, domain=inspect-ip-options, deny=true
        hits=42362, user_data=0x0, cs_id=0x0, reverse, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=Tablet, output_ifc=any

Phase: 5
Type: INSPECT
Subtype: np-inspect
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xaecff708, priority=66, domain=inspect-icmp-error, deny=false
        hits=557, user_data=0xae130b10, cs_id=0x0, use_real_addr, flags=0x0, protocol=1
        src ip/id=0.0.0.0, mask=0.0.0.0, icmp-type=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, icmp-code=0, tag=0, dscp=0x0
        input_ifc=Tablet, output_ifc=any

Phase: 6
Type: VPN
Subtype: ipsec-tunnel-flow
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xae0bca20, priority=13, domain=ipsec-tunnel-flow, deny=true
        hits=2129, user_data=0x0, cs_id=0x0, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=Tablet, output_ifc=any

Phase: 7
Type: USER-STATISTICS
Subtype: user-statistics
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 out id=0xafeb1ac0, priority=0, domain=user-statistics, deny=false
        hits=301202, user_data=0xb03d4f50, cs_id=0x0, reverse, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=any, output_ifc=Outside

Phase: 8
Type: FLOW-CREATION
Subtype:
Result: ALLOW
Config:
Additional Information:
New flow created with id 4526562, packet dispatched to next module
Module information for forward flow ...
snp_fp_tracer_drop
snp_fp_inspect_ip_options
snp_fp_adjacency
snp_fp_fragment
snp_ifc_stat

Module information for reverse flow ...

Result:
input-interface:  Intersting-Traffic-Interface 
input-status: up
input-line-status: up
output-interface: Outside
output-status: up
output-line-status: up
Action: allow

SAT-HQ-IFW1# packet-tracer input HUB_PTP_INT icmp 10.45.54.13(siteA) 0 0 100.100.226.10(siteC) de

Phase: 1
Type: ROUTE-LOOKUP
Subtype: input
Result: ALLOW
Config:
Additional Information:
in   0.0.0.0         0.0.0.0         Outside

Phase: 2
Type: NAT
Subtype: per-session
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xad9acd08, priority=0, domain=nat-per-session, deny=true
        hits=5286847, user_data=0x0, cs_id=0x0, reverse, use_real_addr, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=any, output_ifc=any

Phase: 3
Type: IP-OPTIONS
Subtype:
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xae18c468, priority=0, domain=inspect-ip-options, deny=true
        hits=107237, user_data=0x0, cs_id=0x0, reverse, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=UHS_PTP, output_ifc=any

Phase: 4
Type: INSPECT
Subtype: np-inspect
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xaecf3cc8, priority=66, domain=inspect-icmp-error, deny=false
        hits=231, user_data=0xae1596b0, cs_id=0x0, use_real_addr, flags=0x0, protocol=1
        src ip/id=0.0.0.0, mask=0.0.0.0, icmp-type=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, icmp-code=0, tag=0, dscp=0x0
        input_ifc=UHS_PTP, output_ifc=any

Phase: 5
Type: VPN
Subtype: ipsec-tunnel-flow
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 in  id=0xaf8fe2f0, priority=13, domain=ipsec-tunnel-flow, deny=true
        hits=4354, user_data=0x0, cs_id=0x0, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=UHS_PTP, output_ifc=any

Phase: 6
Type: USER-STATISTICS
Subtype: user-statistics
Result: ALLOW
Config:
Additional Information:
 Forward Flow based lookup yields rule:
 out id=0xafeb1ac0, priority=0, domain=user-statistics, deny=false
        hits=301209, user_data=0xb03d4f50, cs_id=0x0, reverse, flags=0x0, protocol=0
        src ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0
        dst ip/id=0.0.0.0, mask=0.0.0.0, port=0, tag=0, dscp=0x0
        input_ifc=any, output_ifc=Outside

Phase: 7
Type: FLOW-CREATION
Subtype:
Result: ALLOW
Config:
Additional Information:
New flow created with id 4526569, packet dispatched to next module
Module information for forward flow ...
snp_fp_tracer_drop
snp_fp_inspect_ip_options
snp_fp_adjacency
snp_fp_fragment
snp_ifc_stat

Module information for reverse flow ...

Result:
input-interface: HUB_PTP
input-status: up
input-line-status: up
output-interface: Outside - Shouldn't the output interface be the PTP interface?
output-status: up
output-line-status: up
Action: allow