: Saved
:
ASA Version 8.2(5)46 
!
hostname ksiasa03
domain-name ksmfg.com

names
name 192.168.0.0 MOS
name 192.168.32.0 Plant1
name 192.168.16.0 Plant2
name 192.168.48.0 Plant3

!
interface Ethernet0/0
 switchport access vlan 2
!
interface Ethernet0/1
 switchport access vlan 420
!
interface Ethernet0/2
 switchport access vlan 420
!
interface Ethernet0/3
 switchport access vlan 420
!
interface Ethernet0/4
 switchport access vlan 420
!
interface Ethernet0/5
 switchport access vlan 420
!
interface Ethernet0/6
 switchport access vlan 420
!
interface Ethernet0/7
 switchport access vlan 420
!
interface Vlan1
 nameif inside
 security-level 100
 ip address 192.168.1.1 255.255.255.0 
!
interface Vlan2
 nameif outside
 security-level 0
 ip address dhcp 
!
interface Vlan420
 nameif business
 security-level 100
 ip address 192.168.48.1 255.255.255.0 
!
boot system disk0:/asa825-46-k8.bin
ftp mode passive
clock timezone PST -8
clock summer-time PDT recurring
dns server-group DefaultDNS
 domain-name ksmfg.com
object-group network Plant1Plant2MOS
 network-object MOS 255.255.240.0
 network-object Plant2 255.255.240.0
 network-object Plant1 255.255.240.0
access-list outside_1_cryptomap extended permit ip Plant3 255.255.240.0 object-group Plant1Plant2MOS 
access-list outside_1_cryptomap extended permit icmp Plant3 255.255.240.0 object-group Plant1Plant2MOS 
access-list business_nat0_outbound extended permit ip Plant3 255.255.240.0 object-group Plant1Plant2MOS 
access-list outside_access_in extended permit icmp any any 
access-list outside_access_in extended permit ip Plant3 255.255.240.0 object-group Plant1Plant2MOS 
access-list business_access_in extended permit icmp any any 
access-list business_access_in extended permit ip any any 
pager lines 24
logging enable
logging asdm informational
mtu inside 1500
mtu outside 1500
mtu business 1500
no failover
icmp unreachable rate-limit 1 burst-size 1
asdm image disk0:/asdm-715-100.bin
no asdm history enable
arp timeout 14400
global (outside) 1 interface
nat (inside) 1 0.0.0.0 0.0.0.0
nat (business) 0 access-list business_nat0_outbound
nat (business) 1 Plant3 255.255.240.0
nat (business) 101 0.0.0.0 0.0.0.0
access-group outside_access_in in interface outside
access-group business_access_in in interface business
!
router eigrp 10
 network Plant3 255.255.255.0
 passive-interface outside
!
route outside 0.0.0.0 0.0.0.0 x.x.x.x 1
timeout xlate 3:00:00
timeout conn 1:00:00 half-closed 0:10:00 udp 0:02:00 icmp 0:00:02
timeout sunrpc 0:10:00 h323 0:05:00 h225 1:00:00 mgcp 0:05:00 mgcp-pat 0:05:00
timeout sip 0:30:00 sip_media 0:02:00 sip-invite 0:03:00 sip-disconnect 0:02:00
timeout sip-provisional-media 0:02:00 uauth 0:05:00 absolute
timeout tcp-proxy-reassembly 0:01:00
timeout floating-conn 0:00:00
dynamic-access-policy-record DfltAccessPolicy
aaa authentication ssh console LOCAL 
http server enable
http 192.168.1.0 255.255.255.0 inside
http Plant3 255.255.255.0 business
http MOS 255.255.0.0 business
http MOS 255.255.0.0 inside
snmp-server location xxxx
snmp-server contact xxxx
snmp-server community *****
snmp-server enable traps snmp authentication linkup linkdown coldstart
crypto ipsec transform-set ESP-3DES-SHA esp-3des esp-sha-hmac 
crypto ipsec transform-set ESP-AES-128-SHA esp-aes esp-sha-hmac 
crypto ipsec transform-set ESP-AES-128-MD5 esp-aes esp-md5-hmac 
crypto ipsec transform-set ESP-AES-192-SHA esp-aes-192 esp-sha-hmac 
crypto ipsec transform-set ESP-AES-192-MD5 esp-aes-192 esp-md5-hmac 
crypto ipsec transform-set ESP-AES-256-SHA esp-aes-256 esp-sha-hmac 
crypto ipsec transform-set ESP-AES-256-MD5 esp-aes-256 esp-md5-hmac 
crypto ipsec transform-set ESP-AES-128-SHA-TRANS esp-aes esp-sha-hmac 
crypto ipsec transform-set ESP-AES-128-SHA-TRANS mode transport
crypto ipsec transform-set ESP-AES-128-MD5-TRANS esp-aes esp-md5-hmac 
crypto ipsec transform-set ESP-AES-128-MD5-TRANS mode transport
crypto ipsec transform-set ESP-AES-192-SHA-TRANS esp-aes-192 esp-sha-hmac 
crypto ipsec transform-set ESP-AES-192-SHA-TRANS mode transport
crypto ipsec transform-set ESP-AES-192-MD5-TRANS esp-aes-192 esp-md5-hmac 
crypto ipsec transform-set ESP-AES-192-MD5-TRANS mode transport
crypto ipsec transform-set ESP-AES-256-SHA-TRANS esp-aes-256 esp-sha-hmac 
crypto ipsec transform-set ESP-AES-256-SHA-TRANS mode transport
crypto ipsec transform-set ESP-AES-256-MD5-TRANS esp-aes-256 esp-md5-hmac 
crypto ipsec transform-set ESP-AES-256-MD5-TRANS mode transport
crypto ipsec transform-set ESP-3DES-MD5 esp-3des esp-md5-hmac 
crypto ipsec transform-set ESP-3DES-SHA-TRANS esp-3des esp-sha-hmac 
crypto ipsec transform-set ESP-3DES-SHA-TRANS mode transport
crypto ipsec transform-set ESP-3DES-MD5-TRANS esp-3des esp-md5-hmac 
crypto ipsec transform-set ESP-3DES-MD5-TRANS mode transport
crypto ipsec transform-set ESP-DES-SHA esp-des esp-sha-hmac 
crypto ipsec transform-set ESP-DES-MD5 esp-des esp-md5-hmac 
crypto ipsec transform-set ESP-DES-SHA-TRANS esp-des esp-sha-hmac 
crypto ipsec transform-set ESP-DES-SHA-TRANS mode transport
crypto ipsec transform-set ESP-DES-MD5-TRANS esp-des esp-md5-hmac 
crypto ipsec transform-set ESP-DES-MD5-TRANS mode transport
crypto ipsec security-association lifetime seconds 28800
crypto ipsec security-association lifetime kilobytes 4608000
crypto map outside_map 100 match address outside_1_cryptomap
crypto map outside_map 100 set peer 1.1.1.1 
crypto map outside_map 100 set transform-set ESP-3DES-SHA
crypto map outside_map 100 set nat-t-disable
crypto map outside_map interface outside
crypto ca trustpoint _SmartCallHome_ServerCA
 crl configure
crypto ca certificate chain _SmartCallHome_ServerCA
 
  quit
crypto isakmp identity hostname 
crypto isakmp enable outside
crypto isakmp policy 100
 authentication pre-share
 encryption 3des
 hash sha
 group 2
 lifetime 86400
telnet timeout 5
ssh Plant3 255.255.255.0 business
ssh timeout 60
ssh version 2
console timeout 0
management-access business
dhcpd auto_config outside
!
dhcpd address 192.168.1.5-192.168.1.254 inside
dhcpd enable inside
!
dhcpd address 192.168.48.21-192.168.48.100 business
dhcpd dns 192.168.42.207 192.168.42.201 interface business
dhcpd wins 192.168.42.207 192.168.42.201 interface business
dhcpd lease 700000 interface business
dhcpd domain ksmfg.com interface business
dhcpd enable business
!

threat-detection basic-threat
threat-detection statistics access-list
no threat-detection statistics tcp-intercept
webvpn

tunnel-group 1.1.1.1 type ipsec-l2l
tunnel-group 1.1.1.1 ipsec-attributes
 pre-shared-key *****
!
!
prompt hostname context 
service call-home
call-home reporting anonymous
call-home
 contact-email-addr jkrogh@ksplastic.com
 profile CiscoTAC-1
  destination address http https://tools.cisco.com/its/service/oddce/services/DDCEService
  destination address email callhome@cisco.com
  destination transport-method http
  subscribe-to-alert-group diagnostic
  subscribe-to-alert-group environment
  subscribe-to-alert-group inventory periodic monthly
  subscribe-to-alert-group configuration periodic monthly
  subscribe-to-alert-group telemetry periodic daily
Cryptochecksum:6a27b63eece80efacb9de581de29d1fe
: end
asdm image disk0:/asdm-715-100.bin
asdm location MOS 255.255.240.0 inside
asdm location Plant2 255.255.240.0 inside
asdm location Plant1 255.255.240.0 inside
asdm location Plant3 255.255.240.0 inside
no asdm history enable