Router#show startup-config
Using 5031 out of 131072 bytes
!
version 12.4
no service pad
service timestamps debug uptime
service timestamps log uptime
service password-encryption
!
hostname FNN01
!
boot-start-marker
boot-end-marker
!
logging buffered 10000
no logging console
enable secret 5 $1$oFDiNrre4WHZ.
!
no aaa new-model
clock timezone EST 10
clock summer-time DEST recurring last Sun Oct 2:00 last Sun Mar 2:00
!
!
ip cef
!
!
ip auth-proxy max-nodata-conns 3
ip admission max-nodata-conns 3
no ip domain lookup
!
!
!
!
!
archive
log config
hidekeys
!
!
controller DSL 0
mode atm
line-term cpe
line-mode 2-wire line-zero
dsl-mode shdsl symmetric annex B
line-rate auto
!
!
!
!
interface BRI0
no ip address
encapsulation hdlc
shutdown
!
interface ATM0
no ip address
no atm ilmi-keepalive
!
interface ATM0.1 point-to-point
description Modem Management Network
pvc 1/32
ubr 128
encapsulation aal5mux ppp dialer
dialer pool-member 1
!
!
interface ATM0.2 point-to-point
description VPN and RequestDataLink Network
shutdown
pvc 1/33
ubr 384
encapsulation aal5mux ppp dialer
dialer pool-member 2
!
!
interface ATM0.3 point-to-point
description Internet Network
pvc 1/34
ubr 1536
encapsulation aal5mux ppp dialer
dialer pool-member 3
!
!
interface ATM0.4 point-to-point
description VoIP and PowerUser Network
shutdown
pvc 1/35
ubr 384
encapsulation aal5mux ppp dialer
dialer pool-member 4
!
!
interface FastEthernet0
!
interface FastEthernet1
!
interface FastEthernet2
!
interface FastEthernet3
!
interface Vlan1
description FN29 LAN
ip address 192.168.1.1 255.255.255.0
ip access-group 110 in
ip access-group 120 out
ip nat inside
ip virtual-reassembly
!
interface Dialer1
description Modem Management Network
ip address negotiated
ip nat outside
ip virtual-reassembly
encapsulation ppp
dialer pool 1
dialer-group 1
ppp authentication chap callin
ppp chap hostname 0169A
ppp chap password 5 012131
!
interface Dialer2
description VPN and RequestDataLink Network
ip address negotiated
ip nat outside
ip virtual-reassembly
encapsulation ppp
dialer pool 2
dialer-group 1
ppp authentication chap callin
ppp chap hostname 016109B@
ppp chap password 5 073D207
!
interface Dialer3
description Internet Network
ip address negotiated
ip access-group 101 out
ip nat outside
ip virtual-reassembly
encapsulation ppp
dialer pool 3
dialer-group 1
ppp authentication chap callin
ppp chap hostname 01629C@MA01
ppp chap password 5 05393E09
!
interface Dialer4
description VoIP and PowerUser Network
ip address negotiated
ip nat outside
ip virtual-reassembly
encapsulation ppp
dialer pool 4
dialer-group 1
ppp authentication chap callin
ppp chap hostname 016C@DA01
ppp chap password 5 11F1C34
!
ip forward-protocol nd
ip route 0.0.0.0 0.0.0.0 Dialer3
ip route 202.138.192.56 255.255.255.252 Dialer1
ip route 202.138.196.56 255.255.255.252 Dialer1
ip route 202.138.200.56 255.255.255.252 Dialer1
ip route 202.138.202.56 255.255.255.252 Dialer1
ip route 202.138.204.56 255.255.255.252 Dialer1
!
no ip http server
no ip http secure-server
ip nat inside source list 11 interface Dialer3 overload
ip nat inside source static 192.168.1.50 203.111.177.242
!
access-list 11 remark *** Permit end customer address space for NAT
access-list 11 permit 192.168.1.0 0.0.0.255
access-list 70 permit 10.254.254.1
access-list 70 permit 10.224.254.1
access-list 70 permit 10.204.254.1
access-list 70 permit 10.153.254.1
access-list 70 permit 202.138.194.10
access-list 70 remark *** Modem Management
access-list 70 permit 10.71.254.1
access-list 70 permit 202.138.192.56 0.0.0.3
access-list 70 permit 202.138.196.56 0.0.0.3
access-list 70 permit 202.138.200.56 0.0.0.3
access-list 70 permit 202.138.202.56 0.0.0.3
access-list 70 permit 202.138.204.56 0.0.0.3
access-list 70 permit 172.31.241.0 0.0.0.15
access-list 70 permit 172.31.242.0 0.0.0.15
access-list 70 permit 172.31.243.0 0.0.0.15
access-list 70 permit 172.31.244.0 0.0.0.15
access-list 70 permit 172.31.245.0 0.0.0.15
access-list 101 remark Deny private RFC reserved IP addresses.
access-list 101 deny   ip any 10.0.0.0 0.255.255.255
access-list 101 deny   ip any 127.0.0.0 0.255.255.255
access-list 101 deny   ip any 172.16.0.0 0.15.255.255
access-list 101 deny   ip any 192.168.0.0 0.0.255.255
access-list 101 permit ip any any
access-list 110 remark Ethernet Inbound
access-list 110 permit ip any any
access-list 120 remark Ethernet Outbound
access-list 120 permit ip any any
dialer-list 1 protocol ip permit
snmp-server community rdsltrapcomm RO 80
snmp-server community DATCread RO
snmp-server community rdslwritecomm RW 70
snmp-server chassis-id FNN01610970829
snmp-server host 202.138.192.57 rdsltrapcomm
!
!
!
control-plane
!
!
line con 0
exec-timeout 2 0
password 5 095E5B
login
no modem enable
stopbits 1
line aux 0
line vty 0 4
exec-timeout 2 0
password 5 03165601E
login
!
scheduler max-task-time 5000
end