!
version 15.0
service config
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname K2K9Router
!
boot-start-marker
boot-end-marker
!
logging buffered 51200 warnings

!
no aaa new-model
!
no ipv6 cef
ip source-route

!
!
!
!
ip domain name yourdomain.com
multilink bundle-name authenticated

!
interface GigabitEthernet0/0
 description $ETH-LAN$$ETH-SW-LAUNCH$$INTF-INFO-GE 0/0$
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/0.1
 encapsulation dot1Q 1 native
 ip address 192.168.10.254 255.255.255.0
 ip nat inside
 ip virtual-reassembly
!
interface GigabitEthernet0/0.2
 encapsulation dot1Q 2
 ip address 192.168.4.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly
!
interface GigabitEthernet0/0.3
 encapsulation dot1Q 3
 ip address 192.168.3.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly
!
interface GigabitEthernet0/0.100
 encapsulation dot1Q 100
 ip address 10.1.1.244 255.255.255.0
!
interface GigabitEthernet0/1
 no ip address
 ip nat outside
 ip virtual-reassembly
 duplex auto
 speed auto
!
!
router eigrp 1
 network 10.0.0.0
 network 192.168.3.0
 network 192.168.4.0
 network 192.168.10.0
 redistribute static
 passive-interface GigabitEthernet0/0
!
ip forward-protocol nd
!
ip http server
ip http access-class 23
ip http authentication local
ip http secure-server
ip http timeout-policy idle 60 life 86400 requests 10000
!
ip nat inside source list 10 interface GigabitEthernet0/1 overload
ip route 10.1.10.0 255.255.255.0 10.1.1.1
!
access-list 10 permit 10.1.1.0 0.0.0.255
access-list 10 permit 10.1.10.0 0.0.0.255
access-list 10 permit 192.168.4.0 0.0.0.255
access-list 10 permit 192.168.10.0 0.0.0.255
access-list 10 permit 192.168.3.0 0.0.0.255
access-list 23 permit 10.10.10.0 0.0.0.7
!
!
!
control-plane