!
mls qos
!
mls qos map cos-dscp 0 8 16 24 32 46 48 56
mls qos srr-queue output cos-map queue 1 threshold 3  5
mls qos srr-queue output cos-map queue 2 threshold 1  2 4
mls qos srr-queue output cos-map queue 2 threshold 2  3
mls qos srr-queue output cos-map queue 2 threshold 3  6 7
mls qos srr-queue output cos-map queue 3 threshold 3  0
mls qos srr-queue output cos-map queue 4 threshold 3  1
mls qos srr-queue output dscp-map queue 1 threshold 3  46
mls qos srr-queue output dscp-map queue 1 threshold 1  40 41 42 43 44 45 47
mls qos srr-queue output dscp-map queue 2 threshold 1  1 2 3 4 5 6 7 9
mls qos srr-queue output dscp-map queue 2 threshold 1  11 13 15 16 18 20 22 25
mls qos srr-queue output dscp-map queue 2 threshold 1  32 34 36 38
mls qos srr-queue output dscp-map queue 2 threshold 2  24 26
mls qos srr-queue output dscp-map queue 2 threshold 3  48 56
mls qos srr-queue output dscp-map queue 3 threshold 1  17 19 21 23 27 28 29 30
mls qos srr-queue output dscp-map queue 3 threshold 1  31
mls qos srr-queue output dscp-map queue 3 threshold 3  0
mls qos srr-queue output dscp-map queue 4 threshold 1  8 33 35 37 39 49
mls qos srr-queue output dscp-map queue 4 threshold 1  50 51 52 53 54 55 57 58
mls qos srr-queue output dscp-map queue 4 threshold 1  59
mls qos srr-queue output dscp-map queue 4 threshold 1  60 61 62 63
mls qos srr-queue output dscp-map queue 4 threshold 3  10 12 14
mls qos queue-set output 1 threshold 2 70 80 100 100
mls qos queue-set output 1 threshold 4 40 100 100 100
!
class-map match-all Gold
  match access-group name Gold
class-map match-all Silver
  match access-group name Silver
class-map match-all Video
  match access-group name Video
class-map match-all Voice
  match access-group name Voice
class-map match-all Streaming
  match access-group name Streaming
!
!
policy-map Class
  class Voice
   set dscp ef
  class Video
   set dscp af41
  class Gold
   set dscp af31
  class Silver
   set dscp af22
  class Streaming
   set dscp cs4
!
Interface range f1/0/1 - 48
description Corp Users and IP Phones
 switchport host
 switchport access vlan 10
 switchport mode access
 switchport voice vlan 700
 srr-queue bandwidth share 1 70 25 5
 priority-queue out
 spanning-tree bpduguard enable
 service-policy input Class
 no shutdown
 exit
!
ip access-list extended Gold
 remark Signalling for Cisco IPT assumed unmarked
 permit tcp any any range 2000 2002
ip access-list extended Silver
ip access-list extended Streaming
ip access-list extended Video
 permit udp any any range 3230 3247
 permit tcp any any range 3230 3235
ip access-list extended Voice
 remark Voice traffic for Cisco IPT assumed unmarked
 permit udp any any range 16384 32767
!