SWXCA291AC00#show running 
Building configuration...

Current configuration : 15572 bytes
!
! Last configuration change at 16:12:12 EDT Tue Oct 16 2012 by nimda
! NVRAM config last updated at 14:09:41 EDT Tue Oct 16 2012 by nimda
!
version 12.2
no service pad
service tcp-keepalives-in
service tcp-keepalives-out
service timestamps debug datetime msec
service timestamps log datetime msec localtime
service password-encryption
!
hostname SWXCA291AC00
!
boot-start-marker
boot-end-marker
!
enable 
username 
username 
!
no aaa new-model
clock timezone Eastern -5
clock summer-time EDT recurring
system mtu routing 1500
authentication mac-move permit
ip routing
no ip domain-lookup
ip domain-name test.local
ip name-server 172.18.10.10
ip name-server 172.18.11.10
ip dhcp excluded-address 172.18.17.1 172.18.17.100
ip dhcp excluded-address 172.18.17.151 172.18.17.254
!
ip dhcp pool VLAN_317-POOL
   network 172.18.17.0 255.255.255.0
   default-router 172.18.17.1 
   domain-name test.local
   dns-server 172.18.10.10 172.18.11.10 
   lease 8
!
!
!
mls qos map cos-dscp 0 8 16 24 32 46 48 56
mls qos srr-queue input bandwidth 70 30
mls qos srr-queue input threshold 1 80 90
mls qos srr-queue input priority-queue 2 bandwidth 30
mls qos srr-queue input cos-map queue 1 threshold 2 3
mls qos srr-queue input cos-map queue 1 threshold 3 6 7
mls qos srr-queue input cos-map queue 2 threshold 1 4
mls qos srr-queue input dscp-map queue 1 threshold 2 24
mls qos srr-queue input dscp-map queue 1 threshold 3 48 49 50 51 52 53 54 55
mls qos srr-queue input dscp-map queue 1 threshold 3 56 57 58 59 60 61 62 63
mls qos srr-queue input dscp-map queue 2 threshold 3 32 33 40 41 42 43 44 45
mls qos srr-queue input dscp-map queue 2 threshold 3 46 47
mls qos srr-queue output cos-map queue 1 threshold 3 4 5
mls qos srr-queue output cos-map queue 2 threshold 1 2
mls qos srr-queue output cos-map queue 2 threshold 2 3
mls qos srr-queue output cos-map queue 2 threshold 3 6 7
mls qos srr-queue output cos-map queue 3 threshold 3 0
mls qos srr-queue output cos-map queue 4 threshold 3 1
mls qos srr-queue output dscp-map queue 1 threshold 3 32 33 40 41 42 43 44 45
mls qos srr-queue output dscp-map queue 1 threshold 3 46 47
mls qos srr-queue output dscp-map queue 2 threshold 1 16 17 18 19 20 21 22 23
mls qos srr-queue output dscp-map queue 2 threshold 1 26 27 28 29 30 31 34 35
mls qos srr-queue output dscp-map queue 2 threshold 1 36 37 38 39
mls qos srr-queue output dscp-map queue 2 threshold 2 24
mls qos srr-queue output dscp-map queue 2 threshold 3 48 49 50 51 52 53 54 55
mls qos srr-queue output dscp-map queue 2 threshold 3 56 57 58 59 60 61 62 63
mls qos srr-queue output dscp-map queue 3 threshold 3 0 1 2 3 4 5 6 7
mls qos srr-queue output dscp-map queue 4 threshold 1 8 9 11 13 15
mls qos srr-queue output dscp-map queue 4 threshold 2 10 12 14
mls qos queue-set output 1 threshold 1 100 100 50 200
mls qos queue-set output 1 threshold 2 125 125 100 400
mls qos queue-set output 1 threshold 3 100 100 100 400
mls qos queue-set output 1 threshold 4 60 150 50 200
mls qos queue-set output 1 buffers 15 25 40 20
mls qos
password encryption aes
!
crypto pki trustpoint TP-self-signed-664610048
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-664610048
 revocation-check none
 rsakeypair TP-self-signed-664610048
!
!
crypto pki certificate chain TP-self-signed-664610048
 certificate self-signed 01
  ajdlfa;jdlkfjalsdjfksaldjfalksdjf
  quit
auto qos srnd4
!
!
!
port-channel load-balance src-dst-ip
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
spanning-tree vlan 317,700 priority 24576
!
vlan internal allocation policy ascending
!
ip ssh version 2
!
class-map match-all AUTOQOS_VOIP_DATA_CLASS
 match ip dscp ef 
class-map match-all AUTOQOS_DEFAULT_CLASS
 match access-group name AUTOQOS-ACL-DEFAULT
class-map match-all AUTOQOS_VOIP_SIGNAL_CLASS
 match ip dscp cs3 
!
!
policy-map AUTOQOS-SRND4-CISCOPHONE-POLICY
 class AUTOQOS_VOIP_DATA_CLASS
  set dscp ef
  police 128000 8000 exceed-action policed-dscp-transmit
 class AUTOQOS_VOIP_SIGNAL_CLASS
  set dscp cs3
  police 32000 8000 exceed-action policed-dscp-transmit
 class AUTOQOS_DEFAULT_CLASS
  set dscp default
  police 10000000 8000 exceed-action policed-dscp-transmit
!
!
!
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
 switchport access vlan 312
 switchport mode access
!
interface GigabitEthernet0/3
 shutdown
!
interface GigabitEthernet0/4
 switchport access vlan 312
 switchport mode access
!
interface GigabitEthernet0/5
 shutdown
!         
interface GigabitEthernet0/6
 shutdown
!
interface GigabitEthernet0/7
!
interface GigabitEthernet0/8
!
interface GigabitEthernet0/9
!
interface GigabitEthernet0/10
!
interface GigabitEthernet0/11
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust cos
 macro description cisco-switch
 spanning-tree link-type point-to-point
!
interface GigabitEthernet0/12
!
interface GigabitEthernet0/13
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/14
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/15
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/16
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/17
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!         
interface GigabitEthernet0/18
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface GigabitEthernet0/19
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/20
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/21
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/22
 description [VLAN_312]
 switchport access vlan 312
 switchport mode access
 switchport voice vlan 305
 switchport port-security maximum 2
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/23
 description [VLAN_312] PRINTER Dell 1710n
 switchport access vlan 312
 switchport mode access
 switchport port-security
 switchport port-security aging time 2
 switchport port-security violation restrict
 switchport port-security aging type inactivity
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust device cisco-phone
 mls qos trust cos
 auto qos voip cisco-phone 
 macro description cisco-desktop
 spanning-tree portfast
 spanning-tree bpduguard enable
 service-policy input AUTOQOS-SRND4-CISCOPHONE-POLICY
!
interface GigabitEthernet0/24
 description [VLAN_312]
!
interface GigabitEthernet0/25
 description INC SWITCH
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust dscp
 auto qos trust dscp
 macro description cisco-switch
 spanning-tree link-type point-to-point
!
interface GigabitEthernet0/26
 description INC ROUTER
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 16
 switchport trunk allowed vlan 16
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust dscp
 auto qos trust dscp
 macro description cisco-router
 spanning-tree portfast trunk
 spanning-tree bpduguard enable
!
interface GigabitEthernet0/27
 description SWITCH
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust dscp
 auto qos trust dscp
 macro description cisco-switch
 spanning-tree link-type point-to-point
!
interface GigabitEthernet0/28
 description INC SWXCA264AC00 GI0-23
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust dscp
 auto qos trust 
 macro description cisco-switch
 spanning-tree link-type point-to-point
!
interface Vlan1
 no ip address
!
interface Vlan300
 ip address 172.18.0.18 255.255.255.0
 no ip mroute-cache
 ip ospf message-digest-key 1 md5 7 
!
interface Vlan317
 ip address 172.18.17.1 255.255.255.0
 ip ospf message-digest-key 1 md5 7 
!
interface Vlan700
 ip address 172.19.0.1 255.255.255.0
 ip ospf message-digest-key 1 md5 7
!
router ospf 1
 router-id 172.18.0.18
 log-adjacency-changes
 area 0 authentication message-digest
 area 7 authentication message-digest
 network 172.18.0.0 0.0.0.255 area 0
 network 172.18.17.0 0.0.0.255 area 0
 network 172.19.0.0 0.0.255.255 area 7
!
ip classless
ip route 172.18.35.0 255.255.255.128 172.18.0.132
no ip http server
ip http authentication local
ip http secure-server
ip http timeout-policy idle 60 life 86400 requests 10000
!
!
ip access-list extended AUTOQOS-ACL-DEFAULT
 permit ip any any
ip access-list extended VLAN-300-IN
 permit ospf 172.18.0.0 0.0.0.255 any
 permit ip any host 172.18.0.5
 permit ip 172.18.12.0 0.0.0.255 172.19.0.0 0.0.255.255
!
ip sla enable reaction-alerts
logging 172.18.15.10
!
snmp-server community 
snmp-server community 
snmp-server location 
snmp-server contact 
snmp ifmib ifindex persist
!
banner motd ^C
######################################################################
Unauthorized access prohibited!
Logout NOW!
######################################################################
^C
!
line con 0
 logging synchronous
line vty 0 4
 session-timeout 60 
 logging synchronous
 login local
 length 0
 transport input ssh
line vty 5 15
 session-timeout 60 
 logging synchronous
 login local
 transport input ssh
!
ntp clock-period 36028931
ntp server 
ntp server 
end