SWXMAWC1VC00#show running-config 
Building configuration...

Current configuration : 8108 bytes
!
version 12.2
no service pad
service tcp-keepalives-in
service tcp-keepalives-out
service timestamps debug datetime msec
service timestamps log datetime msec localtime
service password-encryption
!
hostname SWXMAWC1VC00
!
boot-start-marker
boot-end-marker
!
enable secret 5 
!
username
username 
username 
!
!
no aaa new-model
clock timezone Eastern -5
clock summer-time EDT recurring
switch 1 provision ws-c3750x-24p
system mtu routing 1500
authentication mac-move permit
ip routing
!
!
no ip domain-lookup
ip domain-name test.local
ip name-server 172.18.10.10
ip name-server 172.18.11.10
!
mls qos map cos-dscp 0 8 16 24 32 46 48 56
mls qos srr-queue input bandwidth 70 30
mls qos srr-queue input threshold 1 80 90
mls qos srr-queue input priority-queue 2 bandwidth 30
mls qos srr-queue input cos-map queue 1 threshold 2 3
mls qos srr-queue input cos-map queue 1 threshold 3 6 7
mls qos srr-queue input cos-map queue 2 threshold 1 4
mls qos srr-queue input dscp-map queue 1 threshold 2 24
mls qos srr-queue input dscp-map queue 1 threshold 3 48 49 50 51 52 53 54 55
mls qos srr-queue input dscp-map queue 1 threshold 3 56 57 58 59 60 61 62 63
mls qos srr-queue input dscp-map queue 2 threshold 3 32 33 40 41 42 43 44 45
mls qos srr-queue input dscp-map queue 2 threshold 3 46 47
mls qos srr-queue output cos-map queue 1 threshold 3 4 5
mls qos srr-queue output cos-map queue 2 threshold 1 2
mls qos srr-queue output cos-map queue 2 threshold 2 3
mls qos srr-queue output cos-map queue 2 threshold 3 6 7
mls qos srr-queue output cos-map queue 3 threshold 3 0
mls qos srr-queue output cos-map queue 4 threshold 3 1
mls qos srr-queue output dscp-map queue 1 threshold 3 32 33 40 41 42 43 44 45
mls qos srr-queue output dscp-map queue 1 threshold 3 46 47
mls qos srr-queue output dscp-map queue 2 threshold 1 16 17 18 19 20 21 22 23
mls qos srr-queue output dscp-map queue 2 threshold 1 26 27 28 29 30 31 34 35
mls qos srr-queue output dscp-map queue 2 threshold 1 36 37 38 39
mls qos srr-queue output dscp-map queue 2 threshold 2 24
mls qos srr-queue output dscp-map queue 2 threshold 3 48 49 50 51 52 53 54 55
mls qos srr-queue output dscp-map queue 2 threshold 3 56 57 58 59 60 61 62 63
mls qos srr-queue output dscp-map queue 3 threshold 3 0 1 2 3 4 5 6 7
mls qos srr-queue output dscp-map queue 4 threshold 1 8 9 11 13 15
mls qos srr-queue output dscp-map queue 4 threshold 2 10 12 14
mls qos queue-set output 1 threshold 1 100 100 50 200
mls qos queue-set output 1 threshold 2 125 125 100 400
mls qos queue-set output 1 threshold 3 100 100 100 400
mls qos queue-set output 1 threshold 4 60 150 50 200
mls qos queue-set output 1 buffers 15 25 40 20
mls qos
password encryption aes
!
crypto pki trustpoint TP-self-signed-3858294144
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3858294144
 revocation-check none
 rsakeypair TP-self-signed-3858294144
!
!
crypto pki certificate chain TP-self-signed-3858294144
 certificate self-signed 01

  quit
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
auto qos srnd4
!
!
!
!
vlan internal allocation policy ascending
!
ip ssh version 2
!
!         
interface FastEthernet0
 no ip address
 no ip route-cache cef
 no ip route-cache
 no ip mroute-cache
!
interface GigabitEthernet1/0/1
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust cos
 macro description cisco-switch
 auto qos trust 
 spanning-tree link-type point-to-point
!
interface GigabitEthernet1/0/2
 switchport access vlan 335
 switchport mode access
!
interface GigabitEthernet1/0/3
 switchport access vlan 335
 switchport mode access
!
interface GigabitEthernet1/0/4
 shutdown
!
interface GigabitEthernet1/0/5
 shutdown
!
interface GigabitEthernet1/0/6
 shutdown
!
interface GigabitEthernet1/0/7
 shutdown
!
interface GigabitEthernet1/0/8
 shutdown
!
interface GigabitEthernet1/0/9
 shutdown
!
interface GigabitEthernet1/0/10
 shutdown
!         
interface GigabitEthernet1/0/11
 shutdown
!
interface GigabitEthernet1/0/12
 shutdown
!
interface GigabitEthernet1/0/13
 shutdown
!
interface GigabitEthernet1/0/14
 shutdown
!
interface GigabitEthernet1/0/15
 shutdown
!
interface GigabitEthernet1/0/16
 shutdown
!
interface GigabitEthernet1/0/17
 shutdown
!
interface GigabitEthernet1/0/18
 shutdown 
!
interface GigabitEthernet1/0/19
 shutdown
!
interface GigabitEthernet1/0/20
 shutdown
!
interface GigabitEthernet1/0/21
 shutdown
!
interface GigabitEthernet1/0/22
 shutdown
!
interface GigabitEthernet1/0/23
 shutdown
!
interface GigabitEthernet1/0/24
 shutdown
!
interface GigabitEthernet1/1/1
 switchport trunk encapsulation dot1q
 switchport mode trunk
 srr-queue bandwidth share 1 30 35 5
 queue-set 2
 priority-queue out 
 mls qos trust cos
 macro description cisco-switch
 auto qos trust 
 spanning-tree link-type point-to-point
!
interface GigabitEthernet1/1/2
 shutdown
!
interface GigabitEthernet1/1/3
 shutdown
!
interface GigabitEthernet1/1/4
 shutdown
!
interface TenGigabitEthernet1/1/1
!
interface TenGigabitEthernet1/1/2
!
interface Vlan1
 no ip address
!         
interface Vlan300
 ip address 172.18.0.132 255.255.255.0
 ip helper-address 172.18.10.10
 no ip route-cache cef
 no ip route-cache
 no ip mroute-cache
!
interface Vlan308
 ip address 172.18.8.1 255.255.255.128
 no ip route-cache cef
 no ip route-cache
 no ip mroute-cache
!
interface Vlan335
 ip address 172.18.35.1 255.255.255.128
 ip helper-address 172.18.10.10
 no ip route-cache cef
 no ip route-cache
 no ip mroute-cache
!
router ospf 1
 router-id 172.18.0.132
 log-adjacency-changes
 area 0 authentication message-digest
 area 7 authentication message-digest
 network 172.18.0.0 0.0.0.255 area 0
 network 172.18.17.0 0.0.0.255 area 0
 network 172.19.0.0 0.0.255.255 area 7
!
ip classless
no ip http server
ip http authentication local
ip http secure-server
ip http timeout-policy idle 60 life 86400 requests 10000
ip ospf name-lookup
!
ip sla enable reaction-alerts
logging 172.18.15.10
snmp-server 
snmp-server 
snmp-server 
snmp ifmib ifindex persist
!
banner motd ^C ######################################################################
Unauthorized access prohibited!
Logout NOW!
###################################################################### 
^C
!
line con 0
 logging synchronous
line vty 0 4
 login local
 length 0
 transport input ssh
line vty 5 15
 login local
 transport input ssh
!
ntp server 
ntp server 
end

SWXMAWC1VC00#