GigabitEthernet0/1 is up, line protocol is up 
  Hardware is BCM1125 Internal MAC, address is 0023.ebb3.fcf1 (bia 0023.ebb3.fcf1)
  MTU 1500 bytes, BW 10000 Kbit, DLY 1000 usec, 
     reliability 255/255, txload 1/255, rxload 1/255
  Encapsulation ARPA, loopback not set
  Keepalive set (10 sec)
  Full-duplex, 10Mb/s, media type is RJ45
  output flow-control is XON, input flow-control is XON
  ARP type: ARPA, ARP Timeout 04:00:00
  Last input 00:00:08, output 00:00:02, output hang never
  Last clearing of "show interface" counters 3d07h
  Input queue: 0/75/0/0 (size/max/drops/flushes); Total output drops: 0
  Queueing strategy: Class-based queueing
  Output queue: 0/1000/64/0 (size/max total/threshold/drops) 
     Conversations  0/1/256 (active/max active/max total)
     Reserved Conversations 7/7 (allocated/max allocated)
     Available Bandwidth 2500 kilobits/sec
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec

policy-map FULL-EGRESS-QUEUING
 class CLASS-VOICE
  priority percent 50
  police rate percent 50
 class CLASS-NETWORK-CONTROL
  bandwidth remaining percent 5
 class CLASS-VIDEO
  bandwidth remaining percent 20
 class CLASS-SIGNALLING
  bandwidth remaining percent 15
 class CLASS-MISSION-CRITICAL
  bandwidth remaining percent 30
  random-detect dscp-based
 class CLASS-BULK-DATA
  bandwidth remaining percent 9
  random-detect dscp-based
 class CLASS-SCAVENGER
  bandwidth remaining percent 1
  random-detect dscp-based
 class class-default
  bandwidth remaining percent 20
  random-detect dscp-based
!