Switch configuration
Current configuration : 6407 bytes
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname Reno-Switch
!
boot-start-marker
boot-end-marker
!
!
!
!
no aaa new-model
switch 1 provision ws-c2960s-24ps-l
!
!
vtp domain data&Voice
vtp mode transparent
nterface Loopback1
 ip address 10.2.20.1 255.255.255.0
!
interface FastEthernet0
 no ip address
!
interface GigabitEthernet1/0/1
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/6
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/7
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/8
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/9
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
interface GigabitEthernet1/0/10
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/11
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/12
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface GigabitEthernet1/0/13
 switchport access vlan 10
 switchport mode access
 switchport nonegotiate
 switchport voice vlan 47
 duplex full
 mls qos trust cos
 spanning-tree portfast