1900 Router Commands

Reno-Router#show ip interface br | ex una
Interface                  IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0         192.168.88.2    YES NVRAM  up                    up      
GigabitEthernet0/1.10      10.3.3.1        YES NVRAM  up                    up      
GigabitEthernet0/1.47      10.41.10.1      YES NVRAM  up                    up      
Loopback0                  10.2.30.1       YES NVRAM  up                    up      

Reno-Router#show run intr gig 
Reno-Router#show run intr eth
Reno-Router#show run intr fa 
Reno-Router#show run intr fast0/1
                        ^
% Invalid input detected at '^' marker.

Reno-Router#show run inter gi    
Reno-Router#show run inter gigabitEthernet0/1
Building configuration...

Current configuration : 125 bytes
!
interface GigabitEthernet0/1
 description "configuring the Virtual interface"
 no ip address
 duplex auto
 speed auto
end

Reno-Router#show run inter gigabitEthernet0/0
Building configuration...

Current configuration : 100 bytes
!
interface GigabitEthernet0/0
 ip address 192.168.88.2 255.255.255.0
 duplex auto
 speed auto
end

Reno-Router#show run inter gigabitEthernet0/0.10
                            ^
% Invalid input detected at '^' marker.

Reno-Router#show ent                            
Reno-Router#show enter 
Reno-Router#show interface gig
Reno-Router#show interface gigabitEthernet0/0.19
                           ^
% Invalid input detected at '^' marker.

Reno-Router#show interface gigabitEthernet0/0.10
                           ^
% Invalid input detected at '^' marker.

Reno-Router#show ip route                       
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area 
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route, H - NHRP, l - LISP
       + - replicated route, % - next hop override

Gateway of last resort is 192.168.88.1 to network 0.0.0.0

S*    0.0.0.0/0 [1/0] via 192.168.88.1
      10.0.0.0/8 is variably subnetted, 6 subnets, 2 masks
C        10.2.30.0/24 is directly connected, Loopback0
L        10.2.30.1/32 is directly connected, Loopback0
C        10.3.3.0/24 is directly connected, GigabitEthernet0/1.10
L        10.3.3.1/32 is directly connected, GigabitEthernet0/1.10
C        10.41.10.0/24 is directly connected, GigabitEthernet0/1.47
L        10.41.10.1/32 is directly connected, GigabitEthernet0/1.47
      192.168.88.0/24 is variably subnetted, 2 subnets, 2 masks
C        192.168.88.0/24 is directly connected, GigabitEthernet0/0
L        192.168.88.2/32 is directly connected, GigabitEthernet0/0
Reno-Router#

ASA COMMANDS BELOW

RENO# show route

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area 
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is 65.255.80.1 to network 0.0.0.0

C    192.168.88.0 255.255.255.0 is directly connected, inside
C    65.255.80.0 255.255.255.0 is directly connected, outside
S    10.3.3.0 255.255.255.0 [1/0] via 192.168.88.2, inside
S    10.41.10.0 255.255.255.0 [1/0] via 192.168.88.2, inside
S*   0.0.0.0 0.0.0.0 [1/0] via 65.255.80.1, outside
RENO# show run route
route outside 0.0.0.0 0.0.0.0 65.255.80.1 1
route inside 10.3.3.0 255.255.255.0 192.168.88.2 1
route inside 10.41.10.0 255.255.255.0 192.168.88.2 1
RENO# show inter ip br
Interface                  IP-Address      OK? Method Status                Protocol
Ethernet0/0                unassigned      YES unset  up                    up  
Ethernet0/1                unassigned      YES unset  down                  down
Ethernet0/2                unassigned      YES unset  up                    up  
Ethernet0/3                unassigned      YES unset  up                    up  
Ethernet0/4                unassigned      YES unset  down                  down
Ethernet0/5                unassigned      YES unset  down                  down
Ethernet0/6                unassigned      YES unset  down                  down
Ethernet0/7                unassigned      YES unset  down                  down
Internal-Data0/0           unassigned      YES unset  up                    up  
Internal-Data0/1           unassigned      YES unset  up                    up  
Vlan1                      192.168.88.1    YES CONFIG up                    up  
Vlan2                      65.255.80.227   YES CONFIG up                    up  
Virtual0                   127.0.0.1       YES unset  up                    up  
RENO# show run inter gig0/3
                     ^
ERROR: % Invalid input detected at '^' marker.
RENO# show run inter eth0/3
!
interface Ethernet0/3
RENO# show run inter eth0/0
!
interface Ethernet0/0
 switchport access vlan 2
RENO# show run inter eth0/1
!
interface Ethernet0/1
 switchport access vlan 2
RENO# show run inter eth0/4
!
interface Ethernet0/4
RENO#