Author: Jeffrey CTR Harned
Company: Federal Aviation Administration

cisco4#show ip mroute
IP Multicast Routing Table
Flags: D - Dense, S - Sparse, B - Bidir Group, s - SSM Group, C - Connected,
       L - Local, P - Pruned, R - RP-bit set, F - Register flag,
       T - SPT-bit set, J - Join SPT, M - MSDP created entry, E - Extranet,
       X - Proxy Join Timer Running, A - Candidate for MSDP Advertisement,
       U - URD, I - Received Source Specific Host Report,
       Z - Multicast Tunnel, z - MDT-data group sender,
       Y - Joined MDT-data group, y - Sending to MDT-data group,
       V - RD & Vector, v - Vector
Outgoing interface flags: H - Hardware switched, A - Assert winner
 Timers: Uptime/Expires
 Interface state: Interface, Next-Hop or VCD, State/Mode

(*, 239.1.1.3), 00:09:41/stopped, RP 0.0.0.0, flags: DC
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan10, Forward/Sparse-Dense, 00:01:39/stopped

(172.26.71.53, 239.1.1.3), 00:00:41/00:02:18, flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan10, Forward/Sparse-Dense, 00:00:41/stopped

(*, 239.1.1.2), 00:09:40/00:02:57, RP 0.0.0.0, flags: DC
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan5, Forward/Sparse-Dense, 00:02:14/stopped

(*, 239.1.1.5), 00:09:41/stopped, RP 0.0.0.0, flags: DC
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan10, Forward/Sparse-Dense, 00:01:41/stopped

(172.26.71.57, 239.1.1.5), 00:00:41/00:02:18, flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan10, Forward/Sparse-Dense, 00:00:41/stopped

(*, 239.1.1.4), 00:09:41/stopped, RP 0.0.0.0, flags: DC
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan15, Forward/Sparse-Dense, 00:01:34/stopped

(172.26.71.54, 239.1.1.4), 00:00:41/00:02:18, flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan15, Forward/Sparse-Dense, 00:00:41/stopped

(*, 239.1.1.6), 00:09:41/stopped, RP 0.0.0.0, flags: DC
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan15, Forward/Sparse-Dense, 00:01:34/stopped

(172.26.71.61, 239.1.1.6), 00:00:41/00:02:18, flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan15, Forward/Sparse-Dense, 00:00:41/stopped

(*, 224.0.1.40), 00:09:41/00:02:57, RP 0.0.0.0, flags: DCL
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    Vlan5, Forward/Sparse-Dense, 00:02:14/stopped

cisco4#