interface GigabitEthernet4/1
 description ***Mikrotik SFP3***
 no ip address
 speed nonegotiate
 flowcontrol send on
 switchport
 switchport trunk encapsulation dot1q
 switchport mode trunk
 no cdp enable
 spanning-tree guard root
 channel-protocol lacp
 channel-group 14 mode active
----------------------
interface GigabitEthernet4/3
 description ***Mikrotik SFP2***
 no ip address
 speed nonegotiate
 flowcontrol send on
 switchport
 switchport trunk encapsulation dot1q
 switchport mode trunk
 no cdp enable
 channel-protocol lacp
 channel-group 14 mode active
==================
interface Port-channel14
 description ** To Mikrotik Bundle **
 no ip address
 speed nonegotiate
 switchport
 switchport trunk encapsulation dot1q
 switchport mode trunk
 lacp max-bundle 2
===============================
Port-channel14 is up, line protocol is up (connected)
  Hardware is EtherChannel, address is 0013.1a9d.5f82 (bia 0013.1a9d.5f82)
  Description: ** To Mikrotik Bundle **
  MTU 1500 bytes, BW 1000000 Kbit, DLY 10 usec,
     reliability 255/255, txload 29/255, rxload 145/255
  Encapsulation ARPA, loopback not set
  Full-duplex, 1000Mb/s
  input flow-control is off, output flow-control is unsupported
  Members in this channel: Gi4/1
  ARP type: ARPA, ARP Timeout 04:00:00
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/2000/0/0 (size/max/drops/flushes); Total output drops: 51891
  Queueing strategy: fifo
  Output queue: 0/40 (size/max)
  5 minute input rate 570523000 bits/sec, 55147 packets/sec
  5 minute output rate 115228000 bits/sec, 44248 packets/sec
     31786129014 packets input, 41106048924446 bytes, 0 no buffer
     Received 592116 broadcasts (246489 multicast)
     0 runts, 0 giants, 0 throttles
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored
     0 watchdog, 0 multicast, 0 pause input
     0 input packets with dribble condition detected
     25212805666 packets output, 7446370146075 bytes, 0 underruns
     0 output errors, 0 collisions, 1 interface resets
     0 babbles, 0 late collision, 0 deferred
     0 lost carrier, 0 no carrier, 0 PAUSE output
     0 output buffer failures, 0 output buffers swapped out