version 12.2
clock timezone CST -6
clock summer-time CDT recurring
switch 1 provision ws-c3750-24p
system mtu routing 1500
ip subnet-zero
!
no file verify auto
!
spanning-tree mode pvst
spanning-tree extend system-id
spanning-tree vlan 1-4094 priority 61440
!
vlan internal allocation policy ascending
!
interface Port-channel1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface GigabitEthernet1/0/1
 description Uplink to 6509
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 254
 switchport mode trunk
!
interface GigabitEthernet2/0/1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan254
 ip address 172.16.254.67 255.255.255.0
!
ip default-gateway 172.16.254.1
ip classless
ip http server
!
control-plane
!
ntp clock-period 36029500
ntp server 172.16.254.1
end
--------------------------------------------------------
Switch Stack Config Below
--------------------------------------------------------
version 12.2
clock timezone CST -6
clock summer-time CDT recurring
switch 1 provision ws-c3750-24p
system mtu routing 1500
!
crypto pki trustpoint TP-self-signed-1491237888
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1491237888
 revocation-check none
 rsakeypair TP-self-signed-1491237888
!
crypto pki certificate chain TP-self-signed-1491237888
 certificate self-signed 01
  3082023F 308201A8 A0030201 02020101 300D0609 2A864886 F70D0101 04050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 31343931 32333738 3838301E 170D3933 30333031 30303039 
  30385A17 0D323030 31303130 30303030 305A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 34393132 
  33373838 3830819F 300D0609 2A864886 F70D0101 01050003 818D0030 81890281 
  8100E0BF F1DF3014 25443449 8893BC3E 35A85407 861A00EA 62CC4922 4E91F1A4 
  2BC31D33 D25186D3 1E46685C 21EB5222 C288F915 3CFB9E5A E80D5D64 ECEC2CB5 
  96508D21 01B7FFDA A4F22127 E6E2B607 7E879343 5D86ED94 0C90D07C 9CF8FB18 
  8451E8C3 1E8E674E E6364C16 2A25C78B FE36E5B0 8D575EB3 FBCF76A7 83C9F175 
  E45D0203 010001A3 67306530 0F060355 1D130101 FF040530 030101FF 30120603 
  551D1104 0B300982 07537769 7463682E 301F0603 551D2304 18301680 14F84C9C 
  8EEDA7B6 12667837 EABBF1E2 D5AA0CA0 6E301D06 03551D0E 04160414 F84C9C8E 
  EDA7B612 667837EA BBF1E2D5 AA0CA06E 300D0609 2A864886 F70D0101 04050003 
  81810082 DC45EE74 C7A9066C 80174B00 22FDE22E DB4979D4 C40ECE4F 8DFEDC0E 
  D6EA6930 9F348D00 C1B8EE8A C05A01ED 694C72DE 061170F0 5A3B4B25 96974DE6 
  2BE3DD4E 0404E9B0 49B6E483 94BD1450 506BA868 EEE48B4E DB44DC32 414BD527 
  AC653960 9F2B4E90 15B7252A 0073FC3A EE648D19 1F1C25D7 851C2AA4 F3309D89 8D41F6
  quit
!
spanning-tree mode pvst
spanning-tree extend system-id
spanning-tree vlan 1-4094 priority 61440
!
vlan internal allocation policy ascending
!
interface Port-channel1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface FastEthernet1/0/15
 description UnityInnWifi AP Ubiquity
 switchport access vlan 254
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 254
 switchport mode trunk
!
interface GigabitEthernet1/0/1
 description Uplink to Inn
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface GigabitEthernet1/0/2
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan254
 ip address 172.16.254.76 255.255.255.0
!
ip default-gateway 172.16.254.67
ip classless
ip http server
ip http secure-server
!
ntp clock-period 36029500
ntp server 172.16.254.1