sho run int gig
vtp3#sho run int gigabitEthernet 5/3
Building configuration...

Current configuration : 171 bytes
!
interface GigabitEthernet5/3
 switchport
 switchport trunk encapsulation dot1q
 switchport trunk allowed vlan 1-1024
 switchport mode trunk
 switchport nonegotiate
end

vtp3#sho int trunk

Port                Mode         Encapsulation  Status        Native vlan
Gi5/3               on           802.1q         trunking      1

Port                Vlans allowed on trunk
Gi5/3               1-1024

Port                Vlans allowed and active in management domain
Gi5/3               1-2,10-12,31,48,64,96,112,192

Port                Vlans in spanning tree forwarding state and not pruned
Gi5/3               1-2,10-12,31,48,64,96,112,192
vtp3#sho vtp stat
VTP Version                     : 3 (capable)
Configuration Revision          : 3
Maximum VLANs supported locally : 1005
Number of existing VLANs        : 15
VTP Operating Mode              : Server
VTP Domain Name                 : SRSnet
VTP Pruning Mode                : Disabled
VTP V2 Mode                     : Enabled
VTP Traps Generation            : Disabled
MD5 digest                      : 0xF6 0xCA 0xD9 0x07 0xEA 0x03 0x17 0x11 
Configuration last modified by 172.25.24.8 at 2-4-09 21:42:25
Local updater ID is 172.25.2.132 on interface Vl2 (lowest numbered VLAN interface found)
VTP version running             : 2
vtp3#conf t
Enter configuration commands, one per line.  End with CNTL/Z.

Added new vlan 3

vtp3(config)#vlan 3
vtp3(config-vlan)#name vlan3
vtp3(config-vlan)#exit
% Applying VLAN changes may take few minutes.  Please wait...

vtp3#wr mem
Building configuration...

*Feb  5 16:58:57.173 EST: %SYS-5-CONFIG_I: Configured from console by console[OK]
vtp3#
vtp3#sho int trunk

Port                Mode         Encapsulation  Status        Native vlan
Gi5/3               on           802.1q         trunking      1

Port                Vlans allowed on trunk
Gi5/3               1-1024

Port                Vlans allowed and active in management domain
Gi5/3               1-3,10-12,31,48,64,96,112,192

Port                Vlans in spanning tree forwarding state and not pruned
Gi5/3               1-3,10-12,31,48,64,96,112,192
vtp3#sho vtp statu
VTP Version                     : 3 (capable)
Configuration Revision          : 4
Maximum VLANs supported locally : 1005
Number of existing VLANs        : 16
VTP Operating Mode              : Server
VTP Domain Name                 : SRSnet
VTP Pruning Mode                : Disabled
VTP V2 Mode                     : Enabled
VTP Traps Generation            : Disabled
MD5 digest                      : 0x5D 0xFE 0xF6 0xF7 0xC9 0xBC 0xE4 0x72 
Configuration last modified by 172.25.2.132 at 2-5-09 21:58:54
Local updater ID is 172.25.2.132 on interface Vl2 (lowest numbered VLAN interface found)
VTP version running             : 2
vtp3#
vtp2#
vtp2#
vtp2#sho int trunk

Port                Mode         Encapsulation  Status        Native vlan
Gi5/2               on           802.1q         trunking      1

Port                Vlans allowed on trunk
Gi5/2               1-1024

Port                Vlans allowed and active in management domain
Gi5/2               1-2,10-12,31,48

Port                Vlans in spanning tree forwarding state and not pruned
Gi5/2               1-2,10-12,31,48
vtp2#sho run int gig
vtp2#sho run int gigabitEthernet 5/2
Building configuration...

Current configuration : 188 bytes
!
interface GigabitEthernet5/2
 switchport
 switchport trunk encapsulation dot1q
 switchport trunk allowed vlan 1-1024
 switchport mode trunk
 switchport nonegotiate
 media-type rj45
end

vtp2#sho vtp stat
VTP Version                     : 2
Configuration Revision          : 0
Maximum VLANs supported locally : 1005
Number of existing VLANs        : 11
VTP Operating Mode              : Client
VTP Domain Name                 : SRSnet
VTP Pruning Mode                : Disabled
VTP V2 Mode                     : Enabled
VTP Traps Generation            : Disabled
MD5 digest                      : 0x01 0xBD 0x12 0x9B 0x60 0xEE 0xD7 0xE8 
Configuration last modified by 127.0.0.51 at 0-0-00 00:00:00
vtp2#sho int trunk

Port                Mode         Encapsulation  Status        Native vlan
Gi5/2               on           802.1q         trunking      1

Port                Vlans allowed on trunk
Gi5/2               1-1024

Port                Vlans allowed and active in management domain
Gi5/2               1-2,10-12,31,48

Port                Vlans in spanning tree forwarding state and not pruned
Gi5/2               1-2,10-12,31,48
vtp2#