!

hostname <hostname>

!

enable secret 5 <password>

!

clock timezone EST -5 0

clock summer-time EDT recurring

!

no ip domain lookup

ip domain name <domain>

ip name-server <DNS\_Server\_IP>

!

stcapp ccm-group 1

stcapp

!

stcapp feature access-code

stcapp feature speed-dial

!

voice-card 0

!

voice call send-alert

voice rtp send-recv

!

voice service voip

 fax protocol pass-through g711ulaw

 modem passthrough nse codec g711ulaw

!

application

 global

 service alternate Default

 !

username admin privilege 15 password <password>

!

ip ssh version 2

!

interface Fastethernet0/0

ip address <IP\_Address>

 duplex auto

 speed auto

!

ip route <static\_route>

!

voice-port 0/0/0

 timeouts initial 60

 timeouts interdigit 60

 timeouts ringing infinity

 caller-id enable

!

voice-port 0/0/1

 timeouts initial 60

 timeouts interdigit 60

 timeouts ringing infinity

!

voice-port 0/0/2

 timeouts initial 60

 timeouts interdigit 60

 timeouts ringing infinity

!

voice-port 0/0/3

 timeouts initial 60

 timeouts interdigit 60

 timeouts ringing infinity

!

sccp local fastethernet0/0

sccp ccm <CUCM\_Publisher\_IP> identifier 1 priority 1 version 7.0

sccp ccm <CUCM\_Subscriber\_IP> identifier 2 priority 2 version 7.0

sccp

!

sccp ccm group 1

 bind interface fastethernet0/0

 associate ccm 1 priority 1

 associate ccm 2 priority 2

 switchback method graceful

!

ccm-manager music-on-hold

!

ccm-manager redundant-host <CUCM\_Subscriber\_IP>

ccm-manager config

ccm-manager sccp local fastethernet0/0

!

dial-peer voice 1000 pots

 service stcapp

 port 0/0/0

!

dial-peer voice 1001 pots

 service stcapp

 port 0/0/1

!

dial-peer voice 1002 pots

 service stcapp

 port 0/0/2

!

dial-peer voice 1003 pots

 service stcapp

 port 0/0/3

!

line vty 0 4

 exec-timeout 0 0

 login local

 transport input ssh

!

ntp server <IP\_Address>

!

end