AP0015.fa05.b7f8#sh crypto ca certificate

CA Certificate

Status: Available

Certificate Serial Number: 00

Certificate Usage: General Purpose

Issuer:

ea=support@airespace.com

cn=ca

ou=none

o=airespace Inc

l=San Jose

st=California

c=US

Subject:

ea=support@airespace.com

cn=ca

ou=none

o=airespace Inc

l=San Jose

st=California

c=US

Validity Date:

start date: 23:38:55 UTC Feb 12 2003

end date: 23:38:55 UTC Nov 11 2012

Associated Trustpoints: airespace-old-root-cert

CA Certificate

Status: Available

Certificate Serial Number: 00

Certificate Usage: Not Set

Issuer:

ea=support@airespace.com

cn=Airespace Root CA

ou=Engineering

o=Airespace Inc.

l=San Jose

--More--

\*Mar 1 00:01:04.313: %CDP\_PD-4-POWER\_OK: Full power - NEGOTIATED inline po st=California

c=US

--More--

\*Mar 1 00:01:04.350: %LINK-3-UPDOWN: Interface Dot11Radio1, changed state to up

\*Mar 1 00:01:04.385: %LINK-3-UPDOWN: Interface Dot11Radio0, changed state to up

\*Mar 1 00:01:05.315: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio1, changed state to up

\*Mar 1 00:01:05.350: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio0, changed s Subject:

ea=support@airespace.com

cn=Airespace Root CA

ou=Engineering

o=Airespace Inc.

l=San Jose

st=California

c=US

Validity Date:

start date: 13:41:22 UTC Jul 31 2003

end date: 13:41:22 UTC Apr 29 2013

--More--

\*Mar 1 00:01:09.586: %DOT11-6-FREQ\_USED: Interface Dot11Radio0, frequency 2432 selected

\*Mar 1 00:01:09.593: %DOT11-6-FREQ\_USED: Interface Dot11Radio1, frequency 526 Associated Trustpoints: airespace-new-root-cert

CA Certificate

Status: Available

Certificate Serial Number: 03

Certificate Usage: General Purpose

Issuer:

ea=support@airespace.com

cn=Airespace Root CA

ou=Engineering

o=Airespace Inc.

l=San Jose

st=California

c=US

Subject:

ea=support@airespace.com

cn=Airespace Device CA

ou=Engineering

o=Airespace Inc.

l=San Jose

st=California

c=US

Validity Date:

start date: 22:37:13 UTC Apr 28 2005

end date: 22:37:13 UTC Jan 26 2015

Associated Trustpoints: airespace-device-root-cert

CA Certificate

Status: Available

Certificate Serial Number: 5FF87B282B54DC8D42A315B568C9ADFF

Certificate Usage: Signature

Issuer:

cn=Cisco Root CA 2048

o=Cisco Systems

--More--

\*Mar 1 00:01:19.602: %DOT11-6-FREQ\_USED: Interface Dot11Radio0, frequency 2437 selected

\*Mar 1 00:01:19.609: %DOT11-6-FREQ\_USED: Interface Dot11Radio1, frequency 528 Subject:

cn=Cisco Root CA 2048

o=Cisco Systems

Validity Date:

start date: 20:17:12 UTC May 14 2004

end date: 20:25:42 UTC May 14 2029

Associated Trustpoints: cisco-root-cert

Certificate

Status: Available

Certificate Serial Number: 19D0271600000005DE0D

Certificate Usage: General Purpose

Issuer:

cn=Cisco Manufacturing CA

o=Cisco Systems

Subject:

--More--

\*Mar 1 00:01:29.617: %DOT11-6-FREQ\_USED: Interface Dot11Radio0, frequency 2442 selected

\*Mar 1 00:01:29.624: %DOT11-6-FREQ\_USED: Interface Dot11Radio1, frequency 530 Name: C1240-0015fa05b7f8

ea=support@cisco.com

cn=C1240-0015fa05b7f8

o=Cisco Systems

l=San Jose

st=California

c=US

CRL Distribution Point:

http://www.cisco.com/security/pki/crl/cmca.crl

Validity Date:

start date: 18:29:39 UTC Dec 12 2005

end date: 18:39:39 UTC Dec 12 2015

renew date: 00:00:00 UTC Jan 1 1970

Associated Trustpoints: Cisco\_IOS\_MIC\_cert

CA Certificate

Status: Available

--More--

\*Mar 1 00:01:39.633: %DOT11-6-FREQ\_USED: Interface Dot11Radio0, frequency 2447 selected

\*Mar 1 00:01:39.639: %DOT11-6-FREQ\_USED: Interface Dot11Radio1, frequency 532 Certificate Serial Number: 6A6967B3000000000003

Certificate Usage: Signature

Issuer:

cn=Cisco Root CA 2048

o=Cisco Systems

Subject:

cn=Cisco Manufacturing CA

o=Cisco Systems

CRL Distribution Point:

http://www.cisco.com/security/pki/crl/crca2048.crl

Validity Date:

start date: 22:16:01 UTC Jun 10 2005

end date: 20:25:42 UTC May 14 2029

Associated Trustpoints: Cisco\_IOS\_MIC\_cert

AP0015.fa05.b7f8#

AP0015.fa05.b7f8#

AP0015.fa05.b7f8#

AP0015.fa05.b7f8#sh crypto ca certificat

\*Mar 1 00:01:49.648: %DOT11-6-FREQ\_USED: Interface Dot11Radio0, frequency 2452 selected

\*Mar 1 00:01:49.655: %DOT11-6-FREQ\_USED: Interface Dot11Radio1, fresh crypto ca certificate