AP70F0.96ED.AFC0#
AP70F0.96ED.AFC0#show capwap client config
AdminState                         : ADMIN_ENABLED(1)
Name                               : AP70F0.96ED.AFC0
Location                           : default location
Primary controller name            :
Secondary controller name          :
Tertiary controller name           :
ssh status                         : Disabled
ApMode                             : Local
ApSubMode                          : Not Configured
Link-Encryption                    : Disabled
OfficeExtend AP                    : Disabled
Discovery Timer                    : 10
Heartbeat Timer                    : 30
Syslog server                      : 255.255.255.255
Syslog Facility                    : 0
Syslog level                       : errors
AP join priority                   : 1
IP Prefer-mode                     : Unconfigured
CAPWAP UDP-Lite                    : Unconfigured
AP retransmit count                : 5
AP retransmit timer                : 3
AP lsc enable                      : 0
AP Policy Tag                      : UNKNOWN
AP RF Tag                          : UNKNOWN
AP Site Tag                        : UNKNOWN
AP Tag Source                      : 0
AP lsc reboot cnt                  : 0
AP lsc max num of retry            : 1
SwVer                              : 8.10.105.0
spamStatTimer                      : 30
Led State Enabled                  : 1
Led Brightness Level               : 8
Primed Interval                    : 0
AP ILP Pre-Standard Switch Support : Disabled
IPv4 TCP MSS Adjust                : Disabled
IPv6 TCP MSS Adjust                : Disabled
LinkFailure                        : 0
SpamReboots                        : 6
ApCrashes                          : 0
AP VLAN Tag status                 : Disabled 0
AP Power Injector                  : Disabled
Indoor Deployment                  : 0
Slot 0 Config:
    Radio Type                : RADIO_TYPE_XOR
    Radio Mode                : Local
    Country code              : GB
    Country ISO Code          : GB
    CleanAir Enable State     : Disabled
    Channel                   : 1
    Automatic Config          : 1
    Current Band              : 2.4GHz
    Channel Width             : 20
    Current Transmit Power    : 1
    Automatic Config          : 1
    DiversitySelection        : Diversity Enabled
   HT Rx Antenna Selection   : 15
    HT Tx Antenna Selection   : 15
    Antenna Band Mode         : Antenna Sector B
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Load Profile
      RF Busy Threshold       : 10
      Clients Threshold       : 12
      Bytes/Second Threshold  : 1000000
    Interference Profile
      Interference  Threshold : 30
    Noise Profile
      NoiseThreshold          : 80
    Coverage Profile
      SNR Threshold           : 70
      Exception Threshold     : 25
      Min Clients Threshold   : 3
       RTS threshold          : 2347
    HE Capable               : true
    HE Info
    HE SuBFCapable           : 1
    HE MuBFCapable           : 1
    HE MbssidCapable         : 0
    HE AmpduTidBmap          : 0
    HE BSS_COLOR_DISABLED    : 0
    HE PARTIAL_BSS_COLOR     : 0
    HE BSS_Color             : 1
    HE DEFAULT_PE_DUR        : 4
    HE RTS_THRESHOLD         : 1023
    HE VHT_OPINFO_PRESENT    : 0
    HE CO_LOCATED_BSS        : 0
    HE ER_SU_DISABLE         : 0
    HE 80_80_CHANNEL_SUPPORT : 0
    HE TWT Capable           : Yes
    HE TWT Config            : Disabled
    HE TWT Broadcast Support : Disabled
    HE MCS Rates             :  AA  FF  AA  FF  FF  FF  FF  FF  FF  FF  FF  FF
 
Slot 1 Config:
    Radio Type                : RADIO_TYPE_80211a
    Radio Mode                : Local
    Country code              : GB
    Country ISO Code          : GB
    CleanAir Enable State     : Disabled
    Channel                   : 36
    Automatic Config          : 1
    Channel Width             : 20
    Current Transmit Power    : 1
    Automatic Config          : 1
    DiversitySelection        : Diversity Enabled
    HT Rx Antenna Selection   : 15
    HT Tx Antenna Selection   : 15
    Antenna Band Mode         : Antenna Sector B
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Antenna Selection         : Internal Antenna
    Load Profile
      RF Busy Threshold       : 10
      Clients Threshold       : 12
      Bytes/Second Threshold  : 1000000
    Interference Profile
      Interference  Threshold : 30
    Noise Profile
      NoiseThreshold          : 80
    Coverage Profile
      SNR Threshold           : 70
      Exception Threshold     : 25
      Min Clients Threshold   : 3
       RTS threshold          : 2347
    VHT Capable               : true
    VHT Info
      numRxAnt                : 4
      numRxChains             : 4
      numTxAnt                : 4
      numTxChains             : 4
      NSS                     : 4
      OperInfo                : 255 255 1
      BasicMcsSet             : 65532
    VHT Config
      DFS Channel             : 0
      Radar Scan Mode         : 1
    VhtEnable                 : 1
      VHTDynBWRes             : 0
      VHTSounding             : 0
      VHTGroupId              : 0
      Flash Commit            : 1
    VHT Capability
    VHT Capability Info       : 866119606
    VHT MCS Rates             : 0 0 0 0 0 0 0 255
    HE Capable               : true
    HE Info
    HE SuBFCapable           : 1
    HE MuBFCapable           : 1
    HE MbssidCapable         : 0
    HE AmpduTidBmap          : 0
    HE BSS_COLOR_DISABLED    : 0
    HE PARTIAL_BSS_COLOR     : 0
    HE BSS_Color             : 1
    HE DEFAULT_PE_DUR        : 4
    HE RTS_THRESHOLD         : 1023
    HE VHT_OPINFO_PRESENT    : 0
    HE CO_LOCATED_BSS        : 0
    HE ER_SU_DISABLE         : 0
    HE 80_80_CHANNEL_SUPPORT : 0
    HE TWT Capable           : Yes
    HE TWT Config            : Disabled
    HE TWT Broadcast Support : Disabled
    HE MCS Rates             :  AA  FF  AA  FF  FF  FF  FF  FF  FF  FF  FF  FF