Predownload COMPLETE!! Trigerring the REBOOT in 5secs.

Writing reload timestamp (Tue Dec  1 18:29:00 UTC 2020) to disk

failed to unmount /storage; waiting 1s and trying again.

[12/01/2020 18:29:04.3896] reboot: Restarting system

BootROM - 1.78
Booting from SPI flash, Secure mode
BootROM: RSA Public key verification PASSED
BootROM: CSK block signature verification PASSED
BootROM: Boot header signature verification PASSED
BootROM: Box ID verification PASSED
BootROM: JTAG is disabled

General initialization - Version: 1.0.0
Detected Device ID 6920
Master bootloder version 1.34
High speed PHY - Version: 2.0
BoardId = 0x25board SerDes lanes topology details:
 | Lane # | Speed|    Type     |
 ------------------------------|
 |   1    |  0   |  SGMII1     |
 |   2    |  5   |  PCIe1      |
 |   4    |  5   |  PCIe2      |
 |   5    |  0   |  SGMII2     |
 -------------------------------
:** Link is Gen1, check the EP capability
PCIe, Idx 1: Link upgraded to Gen2 based on client cpabilities
:** Link is Gen1, check the EP capability
PCIe, Idx 2: Link upgraded to Gen2 based on client cpabilities
High speed PHY - Ended Successfully
DDR4 Training Sequence - Ver TIP-0.23.(Sublib 0.8)0
DDR4 Training Sequence - Switching XBAR Window to FastPath Window
DDR4 Training Sequence - Ended Successfully
BootROM: Image checksum verification PASSED
BootROM: Boot image signature verification PASSED

  ____  _
 / ___|(_) ___   ___  ___
| |    | |/ __| / __|/ _ \
| |___ | |\__ \| (__| (_) |
 \____||_||___/ \___|\___/
         _   _     ____              _
        | | | |   | __ )  ___   ___ | |_
        | | | |___|  _ \ / _ \ / _ \| __|
        | |_| |___| |_) | (_) | (_) | |_
         \___/    |____/ \___/ \___/ \__|
 ** LOADER **

U-Boot 2013.01-gacaad15 (Aug 18 2019 - 20:12:19) SDK version: 2015_T2.0p10

Board: Barbados-3KVE
SoC:   MV88F6920 Rev A1
       running 2 CPUs
CPU:   ARM Cortex A9 MPCore (Rev 1) LE
       CPU 0
       CPU    @ 1800 [MHz]
       L2     @ 900 [MHz]
       TClock @ 250 [MHz]
       DDR4    @ 900 [MHz]
       DDR4 32 Bit Width,FastPath Memory Access, DLB Enabled, ECC Disabled
DRAM:  1 GiB

RST I2C0
NAND:  256 MiB
SF: Detected MX25L3205D with page size 64 KiB, total 4 MiB
PCI-e 1 (IF 0 - bus 0) Root Complex Interface, Detected Link X1, GEN 2.0
PCI-e 2 (IF 1 - bus 1) Root Complex Interface, Detected Link X1, GEN 2.0

Map:   Code:                    0x3fed9000:0x3ffadc40
       BSS:                     0x3ffef704
       Stack:                   0x3f9c8f20
       Heap:                    0x3f9c9000:0x3fed9000
       U-Boot Environment:      0x00100000:0x00110000 (SPI)

Board configuration:
|  port  | Interface  | PHY address  |
|--------|------------|--------------|
| egiga1 |   SGMII    |     0x01     |
| egiga2 |   SGMII    |     In-Band  |
Net:   , egiga1, egiga2 [PRIME]
Hit ESC key to stop autoboot:  0
Creating 1 MTD partitions on "nand0":
0x000000200000-0x000010000000 : "mtd=2"
UBI: attaching mtd1 to ubi0
UBIFS: mounted UBI device 0, volume 1, name "part2"
Loading file 'part2/part.bin' to addr 0x02000000 with size 81920 (0x00014000)...
Done
SF: Detected MX25L3205D with page size 64 KiB, total 4 MiB

Checking image signing.
Image signing verification failure(-2), not allowed to run...
Trying alternate partition part1
UBIFS: mounted UBI device 0, volume 0, name "part1"
Loading file 'part1/part.bin' to addr 0x02000000 with size 55558977 (0x034fc341)...
Done

Checking image signing.
Image signing verification success, continue to run...
Loading Marvel PHY firmware...
Ethernet transceiver PHY firmware download started:
Downloading to PHY's RAM...................... 180192 of 180192 Bytes transferred. [Done]
Ethernet transceiver PHY firmware download succeeded.
Automatic Voltage setting value: 05
## Booting kernel from Legacy Image at 02000000 ...
   Image Name:   Barbados Firmware Image
   Created:      2018-06-05  15:21:43 UTC
   Image Type:   ARM Linux Multi-File Image (uncompressed)
   Data Size:    55557969 Bytes = 53 MiB
   Load Address: 00008000
   Entry Point:  00008000
   Contents:
      Image 0: 4021504 Bytes = 3.8 MiB
      Image 1: 51520684 Bytes = 49.1 MiB
      Image 2: 15765 Bytes = 15.4 KiB
   Verifying Checksum ... OK
## Loading init Ramdisk from multi component Legacy Image at 02000000 ...
## Flattened Device Tree from multi component Image at 02000000
   Booting using the fdt at 0x054f81fc
   Loading Multi-File Image ... OK
OK
   reserving fdt memory region: addr=0 size=4000
   Loading Device Tree to 01ff9000, end 01fffd94 ... OK

   Starting Device Tree update ('fdt_skip_update' = no)

Limit DDR size at 3GB due to power of 2 requirement of Address decoding
Updating device tree successful

Starting kernel ...

[01/01/1970 00:00:00.0000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 260096
[01/01/1970 00:00:00.0000] Memory: 977924K/1048576K available (5460K kernel code, 398K rwdata, 2444K rodata, 351K init, 465K bss, 70652K reserved)
[01/01/1970 00:00:00.1200] CPU1: Booted secondary processor
[01/01/1970 00:00:12.4700] buginf tty flushing thread started, ttyport=bf13bc00
[01/01/1970 00:00:12.5900] m25p80 spi1.0: found mx25l3206, expected n25q032
[*01/01/1970 00:00:13.6664] buginf() enabled.
[*01/01/1970 00:00:13.6751] Made it into bootsh: Jun  5 2018 07:26:40
[*01/01/1970 00:00:13.6752] bootsh build T-eb8875394ad25c6d61b54b35d0937f2f9ded3dd6-geb887539-vipendya
[*01/01/1970 00:00:13.6752] bootsh mini ramfs booted
[*01/01/1970 00:00:24.5419] 397219 blocks

Welcome to Cisco.

Usage of this device is governed by Cisco's End User License Agreement,
available at:
http://www.cisco.com/c/en/us/td/docs/general/warranty/English/EU1KEN_.html.

             Restricted Rights Legend

Use, duplication, or disclosure by the Government is subject to
restrictions as set forth in subparagraph (c) of the Commercial
Computer Software - Restricted Rights clause at FAR sec. 52.227-19 and
subparagraph (c) (1) (ii) of the Rights in Technical Data and Computer
Software clause at DFARS sec. 252.227-7013.

            Cisco Systems, Inc.
            170 West Tasman Drive
            San Jose, California 95134-1706

This product contains cryptographic features and is subject to United
States and local country laws governing import, export, transfer and
use. Delivery of Cisco cryptographic products does not imply
third-party authority to import, export, distribute or use encryption.
Importers, exporters, distributors and users are responsible for
compliance with U.S. and local country laws. By using this product you
agree to comply with applicable laws and regulations. If you are unable
to comply with U.S. and local laws, return this product immediately.

A summary of U.S. laws governing Cisco cryptographic products may be found at:
http://www.cisco.com/wwl/export/crypto/tool/stqrg.html

If you require further assistance please contact us by sending email to
export@cisco.com.

This product contains some software licensed under the
"GNU General Public License, version 2" provided with
ABSOLUTELY NO WARRANTY under the terms of
"GNU General Public License, version 2", available here:
http://www.gnu.org/licenses/old-licenses/gpl-2.0.html

This product contains some software licensed under the
"GNU Library General Public License, version 2" provided
with ABSOLUTELY NO WARRANTY under the terms of "GNU Library
General Public License, version 2", available here:
http://www.gnu.org/licenses/old-licenses/lgpl-2.0.html

This product contains some software licensed under the
"GNU Lesser General Public License, version 2.1" provided
with ABSOLUTELY NO WARRANTY under the terms of "GNU Lesser
General Public License, version 2.1", available here:
http://www.gnu.org/licenses/old-licenses/lgpl-2.1.html

This product contains some software licensed under the
"GNU General Public License, version 3" provided with
ABSOLUTELY NO WARRANTY under the terms of
"GNU General Public License, Version 3", available here:
http://www.gnu.org/licenses/gpl.html.

This product contains some software licensed under the
"GNU Affero General Public License, version 3" provided
with ABSOLUTELY NO WARRANTY under the terms of
"GNU Affero General Public License, version 3", available here:
http://www.gnu.org/licenses/agpl-3.0.html.

init started: BusyBox v1.23.2 (2018-06-05 06:58:59 PDT)
Jan  1 00:00:28 FIPS[1261]: *** shell: FIPS Mode = disabled ***

User Access Verification
Username: [*01/01/1970 00:00:29.8511]
[*01/01/1970 00:00:29.8512]
[*01/01/1970 00:00:29.8512]
[*01/01/1970 00:00:29.8512]
[*01/01/1970 00:00:29.8512] Authenticating ACT2 ID:AP3800
[*01/01/1970 00:00:29.8512] Authenticating SN:FOC224637ZR
[*01/01/1970 00:00:29.8516]
[*01/01/1970 00:00:29.8516] (ACT2Boot) Hardware is Cisco (c) authentic :-)
[*01/01/1970 00:00:29.8516]
[*01/01/1970 00:00:29.8549] Seeding /dev/urandom from ACT2
[*01/01/1970 00:00:30.5038] Reading ACT2 SUDI certificates
[*12/01/2018 23:59:59.0066] Last reload time: Dec 1 18:29:00 2020
[*12/01/2020 18:29:00.0001] Setting system time Tue Dec  1 18:29:00 UTC 2020
[*12/01/2020 18:29:00.1150] Loading kernel crypto modules
[*12/01/2020 18:29:00.2397] GCM-128 POST passed
[*12/01/2020 18:29:00.2398] GCM-256 POST passed
[*12/01/2020 18:29:00.8639] MGIG Bundeled version 201, Tarball version 201
[*12/01/2020 18:29:00.8859] Identified Ethernet mGig PHY: mv2010
[*12/01/2020 18:29:07.6775] Active version: 8.5.131.0
[*12/01/2020 18:29:07.6788] Backup version: 0.0.0.0
[*12/01/2020 18:[12/01/2020 18:29:07.8500] PCI: enabling device 0000:00:02.0 (0140 -> 0143)
29:07.8482] devi[12/01/2020 18:29:07.9300] PCI: enabling device 0000:02:00.0 (0140 -> 0142)
ce wired0 entered promiscuous mode
[*12/01/2020 18:29:09.3765] 0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;
[*12/01/2020 18:29:14.4781] Firmware download complete
[*12/01/2020 18:29:14.4789] FIPS enc aes-ccmp Verified
[*12/01/2020 18:29:14.4790] FIPS dec aes-ccmp [12/01/2020 18:29:14.6200] PCI: enabling device 0000:00:03.0 (0140 -> 0143)
Verified
[*12/0[12/01/2020 18:29:14.7200] PCI: enabling device 0000:03:00.0 (0140 -> 0142)
1/2020 18:29:14.4791] FIPS enc aes-ccmp-256 Verified
[*12/01/2020 18:29:14.4792] FIPS dec aes-ccmp-256 Verified
[*12/01/2020 18:29:14.4793] FIPS enc aes-gcmp Verified
[*12/01/2020 18:29:14.4794] FIPS dec aes-gcmp Verified
[*12/01/2020 18:29:14.4796] FIPS enc aes-gcmp-256 Verified
[*12/01/2020 18:29:14.4797] FIPS dec aes-gcmp-256 Verified
[*12/01/2020 18:29:16.1566] 0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;
[*12/01/2020 18:29:20.5664] Firmware download complete
[*12/01/2020 18:29:20.5671] FIPS enc aes-ccmp Verified
[*12/01/2020 18:29:20.5673] FIPS dec aes-ccmp Verified
[*12/01/2020 18:29:20.5674] FIPS enc aes-ccmp-256 Verified
[*12/01/2020 18:29:20.5675] FIPS dec aes-ccmp-256 Verified
[*12/01/2020 18:29:20.5676] FIPS enc aes-gcmp Verified
[*12/01/2020 18:29:20.5677] FIPS dec aes-gcmp Verified
[*12/01/2020 18:29:20.5678] FIPS enc aes-gcmp-256 Verified
[*12/01/2020 18:29:20.5679] FIPS dec aes-gcmp-256 Verified
[*12/01/2020 18:29:21.0476] ifconfig: SIOCGIFFLAGS: No such device
[*12/01/2020 18:29:21.1659] Initializing NSS Firmware
[12/01/2020 18:29:24.3100] Disabling lock debugging due to kernel taint
[*12/01/2020 18:29:24.4113] stile module dp init successfully
[*12/01/2020 18:29:24.4114] NBAR Label:BLD_MCP_DEV_LATEST_20150424_123021 NBAR VERSION:module build date: Jun  5 2018 at 07:22:48
[*12/01/2020 18:29:26.1220]
[*12/01/2020 18:29:26.1258] boot 9 build T-eb8875394ad25c6d61b54b35d0937f2f9ded3dd6-geb887539-vipendya board barbados mac 70:B3:17:F6:17:18
[*12/01/2020 18:29:26.1289] Module: act2_driver  .text=0x7f000000        data=0x7f000770        bss=0x7f000a04
[*12/01/2020 18:29:26.1289] Module: aes_generic  .text=0x7f004000        data=0x7f00a460        bss=
[*12/01/2020 18:29:26.1289] Module: sha256_generic  .text=0x7f00e000        data=0x7f00fbdc        bss=
[*12/01/2020 18:29:26.1289] Module: sha512_generic  .text=0x7f014000        data=0x7f0158c8        bss=
[*12/01/2020 18:29:26.1289] Module: hmac  .text=0x7f019000        data=0x7f0195e8        bss=
[*12/01/2020 18:29:26.1290] Module: sha1_generic  .text=0x7f01d000        data=0x7f01d2cc        bss=
[*12/01/2020 18:29:26.1290] Module: sha1_arm  .text=0x7f021000        data=0x7f021850        bss=
[*12/01/2020 18:29:26.1290] Module: gf128mul  .text=0x7f025000        data=        bss=
[*12/01/2020 18:29:26.1290] Module: cbc  .text=0x7f02a000        data=0x7f02a4f4        bss=
[*12/01/2020 18:29:26.1290] Module: ctr  .text=0x7f02e000        data=0x7f02e7c8        bss=
[*12/01/2020 18:29:26.1290] Module: ghash_generic  .text=0x7f032000        data=0x7f032268        bss=
[*12/01/2020 18:29:26.1290] Module: seqiv  .text=0x7f036000        data=0x7f036654        bss=
[*12/01/2020 18:29:26.1290] Module: mbedtls  .text=0x7f03a000        data=0x7f0415e0        bss=0x7f041850
[*12/01/2020 18:29:26.1290] Module: a390_mii_xsmi  .text=0x7f046000        data=0x7f046b8c        bss=0x7f046d50
[*12/01/2020 18:29:26.1290] Module: a390_port_switch  .text=0x7f04b000        data=0x7f0ae078        bss=0x7f0b1898
[*12/01/2020 18:29:26.1290] Module: aptrace  .text=0x7f0c9000        data=0x7f0d4f84        bss=0x7f0d5470
[*12/01/2020 18:29:26.1290] Module: ap8x  .text=0x7f0dd000        data=0x7f18f0c0        bss=0x7f196ad8
[*12/01/2020 18:29:26.1290] Module: mv_nss_api  .text=0x7f387000        data=0x7f3d9680        bss=0x7f3dab08
[*12/01/2020 18:29:26.1290] Module: proclikefs  .text=0x7f3ec000        data=        bss=0x7f3ecb80
[*12/01/2020 18:29:26.1290] Module: stile_lm_ft  .text=        data=        bss=
[*12/01/2020 18:29:26.1290] Module: stile_lm_dp  .text=        data=        bss=
[*12/01/2020 18:29:26.1290] Module: mtdoops  .text=0x7fefc000        data=0x7fefce34        bss=0x7fefcfa8
[*12/01/2020 18:29:26.1290] Module: ipv6  .text=0x7ff01000        data=0x7ff36a40        bss=0x7ff38600
[*12/01/2020 18:29:26.1290] Module: llc  .text=0x7ff5f000        data=0x7ff5f84c        bss=0x7ff5f9e8
[*12/01/2020 18:29:26.1290] Module: stp  .text=0x7ff64000        data=0x7f[12/01/2020 18:29:28.9200] wired0 emac 0: link up
f64280        bs[12/01/2020 18:29:28.9900] wired0: link up
s=0x7ff6443c
[*12/01/2020 18:29:26.1291] Module: crc_itu_t  .text=0x7ff68000        data=        bss=
[*12/01/2020 18:29:26.1291] Module: lowmemorykiller  .text=0x7ff6c000        data=0x7ff6c2f4        bss=0x7ff6c4a0
[*12/01/2020 18:29:26.1291] Module: p8022  .text=0x7ff70000        data=        bss=
[*12/01/2020 18:29:26.1291] Module: psnap  .text=0x7ff74000        data=0x7ff74344        bss=0x7ff744c4
[*12/01/2020 18:29:26.1291] Module: rng_core  .text=0x7ff78000        data=0x7ff78818        bss=0x7ff789d8
[*12/01/2020 18:29:26.1291] Module: udf  .text=0x7ff7c000        data=0x7ff8c018        bss=0x7ff8c194
[*12/01/2020 18:29:26.1495] barbados /tmp/SC4_1dbm.txt
[*12/01/2020 18:29:26.2693] Last reload reason : 1: reload command
[*12/01/2020 18:29:34.3063]
[*12/01/2020 18:29:34.3063] Click sched monitor: schedulers = 1
[*12/01/2020 18:29:38.3260] click-config/io-real.click:131: While configuring 'todev_wired0 :: ToDevice':
[*12/01/2020 18:29:38.3260]   warning: device 'wired0' is down
[*12/01/2020 18:29:38.3505] click-config/io-real.click:131: While configuring 'fromdev_wired0 :: FromDevice':
[*12/01/2020 18:29:38.3505]   warning: device 'wired0' is down
[*12/01/2020 18:29:38.8266] click-config/io-real[12/01/2020 18:29:38.8500] wired0 emac 0: link up
.click:131: Whil[12/01/2020 18:29:38.9200] wired0: link up
e initializing 'tohost_wired0 :: ToHost':
[*12/01/2020 18:29:38.8266]   warning: device 'wired0' is down
[*12/01/2020 18:29:38.9927] aptrace_register_sysproc_fn: duplicate registeration for 'wired'
[*12/01/2020 18:29:39.8515] chatter: tohost_srcr6 :: ToHost: device 'srcr6' went down
[*12/01/2020 18:29:39.8632] chatter: tohost_srcr6 :: ToHost: device 'srcr6' came up
[*12/01/2020 18:29:39.8639] ip6_port srcr6, ip6local fe80::72b3:17ff:fef6:1718, ip6 ::, plen 0, gw6 ::, gw6_mac 00:00:00:00:00:00, mtu 1500, vid 0, mode6 3(slaac)
[*12/01/2020 18:29:40.1403] SYS-COND: AP is in fair condition
[*12/01/2020 18:29:40.1408] ethernet_port wired0, ip 192.168.1.4, netmask 255.255.255.0, gw 192.168.1.1, mtu 1500, bcast 192.168.1.255, dns1 0.0.0.0, is_static true, vid 0, static_ip_failover false, dhcp_vlan_failover false
[*12/01/2020 18:29:48.7955]  Create symlink /dev/mic_cert result 0
[*12/01/2020 18:29:48.7955] Loading certificates from storage...
[*12/01/2020 18:29:48.8096] SKU to radio FW
[*12/01/2020 18:29:49.1100] Generating key, this may take a while...
[*12/01/2020 18:29:51.3263] Public key portion is:
[*12/01/2020 18:29:51.3263] ssh-rsa AAAAB3NzaC1yc2EAAAADAQABAAABAQDSasDV23O/JzsPvUKJb8OFN8witWhgtvU+y8QYEhRCsp066oH2tS+hmmQiGyg/4CMAtVq2vccyz7ZFJnSXZJk7PBRhsR3pnsHL7YbRr/YM+ILKhjh1Y0Qli0DTuc9go0BuJk4xc+AmKUP2kAVjGY258yFge90JB/I4TRVlzz7mnH+7mFI6JyIl2V2FTbAEzGX/9zKVaCGf0D5uyKd0IepSaQzdihIOe9lXls8ltrds/sax3nQdcSzjHJbcIloosh6hMHSYLBzf8Nq6bkffU76lyNcTNh0I7Wl9usqH3wBKkbayVYvvKzLs9IOia+CdNQWm64Uj0jOIziv3BtzZh1bt root@m70B317F61718
[*12/01/2020 18:29:51.3263] Fingerprint: md5 05:ac:f8:21:21:a5:a1:53:ed:d9:e1:36:c2:cd:e0:70
[*12/01/2020 18:29:51.3378] Starting monit
[*12/01/2020 18:29:51.6049]  New Monit id: d83a9930e5a00104d83f84868a0f4c4b
[*12/01/2020 18:29:51.6049]  Stored in '/var/.monit.id'
[*12/01/2020 18:29:51.6051] Starting Monit 5.18 daemon with http interface at [*]:2812
[*12/01/2020 18:29:54.5004] starting tam services using ACT2...
[*12/01/2020 18:29:54.9702] Password for 'admin' changed
[*12/01/2020 18:29:55.2746] gzip -dc /etc/wcp.usermodule.template.gz | sed -e 's/__TX_POWER_XOR_5G_FILE__/\/radio_fw\/X5.csv/g' -e 's/__EVM_POWER_XOR_5G_FILE__/\/radio_fw\/EVM_X5.csv/g' -e 's/__TX_POWER_2G_FILE__/\/radio_fw\/R2.csv/g' -e 's/__TX_POWER_5G_FILE__/\/radio_fw\/R5.csv/g' -e 's/__EVM_POWER_2G_FILE__/\/radio_fw\/EVM_2.csv/g' -e 's/__EVM_POWER_5G_FILE__/\/radio_fw\/EVM_5.csv/g' -e 's/__DOMAIN_2G__/1/g' -e 's/__DOMAIN_5G__/12/g' -e 's/__PWR_TABLE_49G__/0/g' -e 's/__PRODUCT_ID__/AIR-AP3802E-E-K9/g' -e 's/__AP_TYPE__/51/g' -e 's/__WIRELESS_MAC__/70:B3:17:D8:73:60/g' -e 's/__WIRED_MAC__/70:B3:17:F6:17:18/g' -e 's/__WIRED1_MAC__/70:B3:17:F6:17:18/g' | DMALLOC_OPTIONS=debug=0x400003,inter=1000,log=/tmp/wcp.dmalloc.log,limit=40000000 wcpd &
[*12/01/2020 18:29:56.9831] Stopped Radio 0
[*12/01/2020 18:29:56.9970] DOT11_DRV[0]: set_channel Channel set to 6
[*12/01/2020 18:29:57.5717] Stopped Radio 1
[*12/01/2020 18:29:57.5846] DOT11_DRV[1]: set_channel Channel set to 36
[*12/01/2020 18:29:57.8350] CRIT-MeshControl:
[*12/01/2020 18:29:57.8350] Mesh Control: skipped adding wired1 backhaul
[*12/01/2020 18:29:57.8362] WCP: Opening /tmp/wcpstate failed!
[*12/01/2020 18:29:58.3618] DOT11_CFG[0] Radio Mode is changed from Local to FlexConnect
[*12/01/2020 18:29:58.4981] Started Radio 0
[*12/01/2020 18:29:58.4986] DOT11_CFG[1] Radio Mode is changed from Local to FlexConnect
[*12/01/2020 18:29:58.6238] Started Radio 1
[*12/01/2020 18:29:59.0884] Stopped Radio 0
[*12/01/2020 18:29:59.1010] DOT11_DRV[0]: set_channel Channel set to 1
[*12/01/2020 18:29:59.2300] Started Radio 0
[*12/01/2020 18:29:59.9427] Stopped Radio 0
[*12/01/2020 18:29:59.9554] DOT11_DRV[0]: set_channel Channel set to 1
[*12/01/2020 18:30:00.0786] Started Radio 0
[*12/01/2020 18:30:00.0857] Stopped Radio 0
[*12/01/2020 18:30:00.0984] DOT11_DRV[0]: set_channel Channel set to 1
[*12/01/2020 18:30:00.2225] Started Radio 0
[*12/01/2020 18:30:01.1008] bftype is 6
[*12/01/2020 18:30:01.2294] Stopped Radio 0
[*12/01/2020 18:30:01.2416] DOT11_DRV[0]: set_channel Channel set to 1
[*12/01/2020 18:30:01.4194] Started Radio 0
[*12/01/2020 18:30:02.1470] Stopped Radio 0
[*12/01/2020 18:30:02.1595] DOT11_DRV[0]: set_channel Channel set to 1
[*12/01/2020 18:30:02.3302] Started Radio 0
[*12/01/2020 18:30:02.5828] WCP: Opening /tmp/wcpstate failed!
[*12/01/2020 18:30:03.0264] Stopped Radio 1
[*12/01/2020 18:30:03.0404] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:03.1260] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:03.1818] Started Radio 1
[*12/01/2020 18:30:03.3311] reset DFS SM before last CAC expired
[*12/01/2020 18:30:03.8542] Stopped Radio 1
[*12/01/2020 18:30:03.8678] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:03.9478] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:04.0037] Started Radio 1
[*12/01/2020 18:30:04.1574] reset DFS SM before last CAC expired
[*12/01/2020 18:30:04.6781] Stopped Radio 1
[*12/01/2020 18:30:04.6902] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:04.7703] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:04.8264] Started Radio 1
[*12/01/2020 18:30:04.8337] Stopped Radio 1
[*12/01/2020 18:30:04.8373] deinit DFS SM since radio is stopped before last CAC expired
[*12/01/2020 18:30:04.8467] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:04.9278] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:04.9833] Started Radio 1
[*12/01/2020 18:30:05.1369] reset DFS SM before last CAC expired
[*12/01/2020 18:30:05.8154] bftype is 6
[*12/01/2020 18:30:05.9470] Stopped Radio 1
[*12/01/2020 18:30:05.9599] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:06.1205] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:06.1771] Started Radio 1
[*12/01/2020 18:30:06.3311] reset DFS SM before last CAC expired
[*12/01/2020 18:30:06.8623] Stopped Radio 1
[*12/01/2020 18:30:06.8754] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:07.0322] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:07.0900] Started Radio 1
[*12/01/2020 18:30:07.2455] reset DFS SM before last CAC expired
[*12/01/2020 18:30:07.7748] Stopped Radio 1
[*12/01/2020 18:30:07.7869] DOT11_DRV[1]: set_channel Channel set to 100
[*12/01/2020 18:30:07.9445] 1:change to DFS channel 100, CAC for 60 seconds.
[*12/01/2020 18:30:08.0011] Started Radio 1
[*12/01/2020 18:30:08.0148] reset DFS SM before last CAC expired
[*12/01/2020 18:30:08.2314] WCP: Opening /tmp/wcpstate failed!
[*12/01/2020 18:30:08.3534] DOT11_CFG[0] Radio Mode is changed from FlexConnect to FlexConnect
[*12/01/2020 18:30:08.3551] DOT11_CFG[1] Radio Mode is changed from FlexConnect to FlexConnect
[*12/01/2020 18:30:08.3758] AP IPv4 Address updated from 0.0.0.0 to 192.168.1.4
[*12/01/2020 18:31:28.2356] DOT11_DRV[1]: DFS CAC timer might have stopped, resume beacon stuck detection
[*12/01/2020 18:32:46.9986] chatter: tohost_virtual :: ToHost: device 'virtual' went down
[*12/01/2020 18:32:47.0386] chatter: tohost_vlan0 :: ToHost: device 'vlan0' went down
[*12/01/2020 18:32:47.0686] chatter: tohost_vlan1 :: ToHost: device 'vlan1' went down
[*12/01/2020 18:32:47.0986] chatter: tohost_vlan2 :: ToHost: device 'vlan2' went down
[*12/01/2020 18:32:47.1386] chatter: tohost_vlan3 :: ToHost: device 'vlan3' went down
[*12/01/2020 18:32:47.1687] chatter: tohost_vlan4 :: ToHost: device 'vlan4' went down
[*12/01/2020 18:32:47.2092] chatter: tohost_vlan5 :: ToHost: device 'vlan5' went down
[*12/01/2020 18:32:47.2485] chatter: tohost_vlan6 :: ToHost: device 'vlan6' went down
[*12/01/2020 18:32:47.2886] chatter: tohost_vlan7 :: ToHost: device 'vlan7' went down
[*12/01/2020 18:32:47.3390] chatter: tohost_vlan8 :: ToHost: device 'vlan8' went down
[*12/01/2020 18:32:47.3785] chatter: tohost_vlan9 :: ToHost: device 'vlan9' went down
[*12/01/2020 18
Cryptographic library self-test....
Testing SHA1 Short Message 1
Testing SHA256 Short Message 1
Testing SHA384 Short Message 1
SHA1 POST PASSED
Testing HMAC SHA1 Short Message 1
Testing HMAC SHA2 Short Message 1
Testing HMAC SHA384 Short Message 1
passed!

XML config selected
/bin/sh: /usr/bin/iptables: not found
/bin/sh: /usr/bin/iptables: not found
Validating XML configuration
Cisco is a trademark of Cisco Systems, Inc.
Software Copyright Cisco Systems, Inc. All rights reserved.

Cisco AireOS Version 8.5.131.0
Initializing OS Services: ok
Initializing Serial Services: ok
Initializing Network Services: ok
Starting SSHD: ok
Starting Statistics Service: ok
Starting ARP Services: ok
Starting Trap Manager: ok
Starting Network Interface Management Services: ok
Starting System Services: ok
Starting SNMP services: ok
Starting Fastpath Hardware Acceleration: Starting Switching Services: ok
Starting QoS Services: ok
Starting Policy Manager: ok
Starting Data Transport Link Layer: ok
Starting Access Control List Services: ok
Starting System Interfaces:
As the Mgmt Address is updated, all the DHCP scopes with Central NAT enabled will be disabled and enabled
As the Mgmt Address is updated, all the WLANs associated with central NAT enabled scopes will be enabled and disabled
ok
Starting Client Troubleshooting Service: ok
Starting Certificate Database: Initializing Curl Globally..
ok
Starting VPN Services: ok
Starting Management Frame Protection: ok
Starting DNS Services: ok
ok
Starting LWAPP: ok
Starting CAPWAP: ok
Starting LOCP: ok
Starting Security Services: ok
Starting Policy Manager: ok
Starting Authentication Engine: ok
Starting Mobility Management: ok
Starting Capwap Ping Component: ok
Starting AVC Services: ok
Starting AVC Flex Services: ok
Starting Virtual AP Services: ok
Starting AireWave Director: ok
Starting Network Time Services: ok
Starting Cisco Discovery Protocol: ok
Starting Broadcast Services: ok
Starting Logging Services: ok
Starting DHCP Server: ok
Starting IDS Signature Manager: ok
Starting RFID Tag Tracking: ok
Starting RF Profiles: ok
Starting Mesh Services:  ok
Starting TSM: ok
Starting CIDS Services: ok
Starting Ethernet-over-IP: ok
Starting DTLS server:  enabled in CAPWAP
Starting CleanAir: ok
Starting WIPS: ok
Starting SSHPM LSC PROV LIST: ok
Starting RRC Services: ok
Starting SXP Services: ok
Starting Alarm Services: ok
Starting FMC HS: ok
Starting FLEXEXPRESS ConfigSync Task: ok
Starting Hotspot Services: ok
Starting HTTP Image Download Task: ok
Starting Tunnel Services New: ok
Starting Portal Server Services: ok
Starting Management Services:
Starting IPSec Profiles component: ok
Starting CPU ACL Logging services: ok
   Web Server:    CLI:    Secure Web: ok

(Cisco Controller)