Mar 13 16:53:50 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:53:50 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:54:21 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:54:21 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1962429915^M
Mar 13 16:54:21 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:54:21 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:54:21 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:54:21 syslog[337]: CSeq: 1150 REGISTER^M
Mar 13 16:54:21 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:54:21 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:54:21 syslog[337]: Max-Forwards: 70^M
Mar 13 16:54:21 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:54:21 syslog[337]: Expires: 60^M
Mar 13 16:54:21 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:54:21 syslog[337]: Line: 1^M
Mar 13 16:54:21 syslog[337]: Content-Length: 0^M
Mar 13 16:54:21 syslog[337]: ^M
Mar 13 16:54:21 syslog[337]: 
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:54:21 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:54:21 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:54:21 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:54:21 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:54:21 syslog[337]: CSeq: 1150 REGISTER^M
Mar 13 16:54:21 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1962429915^M
Mar 13 16:54:21 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:54:21 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:54:21 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:54:21 syslog[337]: Content-Length: 0^M
Mar 13 16:54:21 syslog[337]: Date: Sat, 13 Mar 2010 11:54:23 PST^M
Mar 13 16:54:21 syslog[337]: ^M
Mar 13 16:54:21 syslog[337]: 
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:54:21 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:54:52 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:54:52 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1177493093^M
Mar 13 16:54:52 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:54:52 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:54:52 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:54:52 syslog[337]: CSeq: 1151 REGISTER^M
Mar 13 16:54:52 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:54:52 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:54:52 syslog[337]: Max-Forwards: 70^M
Mar 13 16:54:52 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:54:52 syslog[337]: Expires: 60^M
Mar 13 16:54:52 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:54:52 syslog[337]: Line: 1^M
Mar 13 16:54:52 syslog[337]: Content-Length: 0^M
Mar 13 16:54:52 syslog[337]: ^M
Mar 13 16:54:52 syslog[337]: 
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:54:52 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:54:52 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:54:52 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:54:52 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:54:52 syslog[337]: CSeq: 1151 REGISTER^M
Mar 13 16:54:52 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1177493093^M
Mar 13 16:54:52 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:54:52 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:54:52 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:54:52 syslog[337]: Content-Length: 0^M
Mar 13 16:54:52 syslog[337]: Date: Sat, 13 Mar 2010 11:54:54 PST^M
Mar 13 16:54:52 syslog[337]: ^M
Mar 13 16:54:52 syslog[337]: 
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:54:52 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:55:23 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:55:23 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1936032978^M
Mar 13 16:55:23 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:55:23 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:55:23 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:55:23 syslog[337]: CSeq: 1152 REGISTER^M
Mar 13 16:55:23 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:55:23 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:55:23 syslog[337]: Max-Forwards: 70^M
Mar 13 16:55:23 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:55:23 syslog[337]: Expires: 60^M
Mar 13 16:55:23 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:55:23 syslog[337]: Line: 1^M
Mar 13 16:55:23 syslog[337]: Content-Length: 0^M
Mar 13 16:55:23 syslog[337]: ^M
Mar 13 16:55:23 syslog[337]: 
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:55:23 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:55:23 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:55:23 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:55:23 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:55:23 syslog[337]: CSeq: 1152 REGISTER^M
Mar 13 16:55:23 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1936032978^M
Mar 13 16:55:23 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:55:23 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:55:23 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:55:23 syslog[337]: Content-Length: 0^M
Mar 13 16:55:23 syslog[337]: Date: Sat, 13 Mar 2010 11:55:25 PST^M
Mar 13 16:55:23 syslog[337]: ^M
Mar 13 16:55:23 syslog[337]: 
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:55:23 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:55:54 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:55:54 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK968043456^M
Mar 13 16:55:54 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:55:54 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:55:54 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:55:54 syslog[337]: CSeq: 1153 REGISTER^M
Mar 13 16:55:54 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:55:54 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:55:54 syslog[337]: Max-Forwards: 70^M
Mar 13 16:55:54 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:55:54 syslog[337]: Expires: 60^M
Mar 13 16:55:54 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:55:54 syslog[337]: Line: 1^M
Mar 13 16:55:54 syslog[337]: Content-Length: 0^M
Mar 13 16:55:54 syslog[337]: ^M
Mar 13 16:55:54 syslog[337]: 
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:55:54 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:55:54 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:55:54 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:55:54 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:55:54 syslog[337]: CSeq: 1153 REGISTER^M
Mar 13 16:55:54 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK968043456^M
Mar 13 16:55:54 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:55:54 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:55:54 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:55:54 syslog[337]: Content-Length: 0^M
Mar 13 16:55:54 syslog[337]: Date: Sat, 13 Mar 2010 11:55:56 PST^M
Mar 13 16:55:54 syslog[337]: ^M
Mar 13 16:55:54 syslog[337]: 
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:55:54 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:56:03 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:56:03 syslog[337]: INVITE sip:101@192.168.1.100:6060 SIP/2.0^M
Mar 13 16:56:03 syslog[337]: Via: SIP/2.0/UDP 192.168.1.100:6060;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-__0^M
Mar 13 16:56:04 syslog[337]: Via: SIP/2.0/UDP 192.168.1.5:6054;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-;rport^M
Mar 13 16:56:04 syslog[337]: Max-Forwards: 70^M
Mar 13 16:56:04 syslog[337]: Contact: <sip:108@192.168.1.5:6054>^M
Mar 13 16:56:04 syslog[337]: To: <sip:101@192.168.1.100:6060>^M
Mar 13 16:56:04 syslog[337]: From: "108"<sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:04 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:04 syslog[337]: CSeq: 1 INVITE^M
Mar 13 16:56:04 syslog[337]: Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, NOTIFY, MESSAGE, SUBSCRIBE, INFO^M
Mar 13 16:56:04 syslog[337]: Content-Type: application/sdp^M
Mar 13 16:56:04 syslog[337]: Supported: eventlist^M
Mar 13 16:56:04 syslog[337]: User-Agent: eyeBeam release 3010n stamp 19039^M
Mar 13 16:56:04 syslog[337]: Content-Length: 264^M
Mar 13 16:56:04 syslog[337]: ^M
Mar 13 16:56:04 syslog[337]: v=0^M
Mar 13 16:56:04 syslog[337]: o=- 98272635 98273419 IN IP4 192.168.1.5^M
Mar 13 16:56:04 syslog[337]: s=eyeBeam^M
Mar 13 16:56:04 syslog[337]: c=IN IP4 192.168.1.5^M
Mar 13 16:56:04 syslog[337]: t=0 0^M
Mar 13 16:56:04 syslog[337]: m=audio 6056 RTP/AVP 100 0 8 18 5 101^M
Mar 13 16:56:04 syslog[337]: a=alt:1 1 : B420ABE1 00000014 192.168.1.5 6056^M
Mar 13 16:56:04 syslog[337]: a=fmtp:101 0-15^M
Mar 13 16:56:04 syslog[337]: a=rtpmap:100 speex/16000^M
Mar 13 16:56:04 syslog[337]: a=rtpmap:101 telephone-event/8000^M
Mar 13 16:56:04 syslog[337]: a=sendrecv^M
Mar 13 16:56:04 syslog[337]: 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | This is a request
Mar 13 16:56:04 syslog[337]: <0> | ERROR | *** Call id set to 115 *** 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:04 syslog[337]: SIP/2.0 100 Trying^M
Mar 13 16:56:04 syslog[337]: Via: SIP/2.0/UDP 192.168.1.100:6060;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-__0^M
Mar 13 16:56:04 syslog[337]: Via: SIP/2.0/UDP 192.168.1.5:6054;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-;rport^M
Mar 13 16:56:04 syslog[337]: From: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:04 syslog[337]: To: <sip:101@192.168.1.100:6060>^M
Mar 13 16:56:04 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:04 syslog[337]: CSeq: 1 INVITE^M
Mar 13 16:56:04 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:04 syslog[337]: Content-Length: 0^M
Mar 13 16:56:04 syslog[337]: ^M
Mar 13 16:56:04 syslog[337]: 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [New call received!] 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | New Incoming Call here (115) 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Get ext user info  auto-answer = [] video = [0] referred_by = []
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Get ext user info  ringtone = [] ringtone_ext_flag = [] ringtone_info = [] ringtone_url = [] 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Message sent: [(PHONE_MSG_CALL_INCOME) -- (0xa000d)  wParam(0x73)-lParam(0x0)] 
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:04 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:04 syslog[337]: SIP/2.0 180 Ringing^M
Mar 13 16:56:04 syslog[337]: Via: SIP/2.0/UDP 192.168.1.100:6060;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-__0^M
Mar 13 16:56:04 syslog[337]: Via: SIP/2.0/UDP 192.168.1.5:6054;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-;rport^M
Mar 13 16:56:04 syslog[337]: From: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:04 syslog[337]: To: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:04 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:04 syslog[337]: CSeq: 1 INVITE^M
Mar 13 16:56:04 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:56:04 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:04 syslog[337]: Allow-Events: talk,hold,conference,refer,check-sync^M
Mar 13 16:56:04 syslog[337]: Content-Length: 0^M
Mar 13 16:56:04 syslog[337]: ^M
Mar 13 16:56:04 syslog[337]: 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Message received: [(SIP_MSG_ANSWER_CALL) -- (0x40007)  wParam(0x73)-lParam(0x0)] 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Answer: SRTP disabled
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Last DTMF Payload is 101 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Bandwidth is zero, unset the b= field
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Bandwidth is zero, unset the b= field
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Session-Expires Header Not found!
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Local IP Address is (192.168.1.101)
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Message sent: [(PHONE_MSG_CALL_ESTABLISHED) -- (0xa0006)  wParam(0x73)-lParam(0x0)] 
Mar 13 16:56:05 syslog[337]: ^[[1m<0> | LEVEL4 | $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Audio [0-PCMU (), Port local 11796, remote: 6056, dtmf payload 101, sendrecv 0, ptime 20] 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Video [0- (), Port local 0, remote: 0] audip:192.168.1.5-vidip, sendrecv 0
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Bandwidth Audio [0-0], Video (0, 0)]
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | audio srtp option decode [], encode []
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | video srtp option decode [], encode []
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
Mar 13 16:56:05 syslog[337]: ^[[0m<0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:05 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:56:05 syslog[337]: Via: SIP/2.0/UDP 192.168.1.100:6060;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-__0^M
Mar 13 16:56:05 syslog[337]: Via: SIP/2.0/UDP 192.168.1.5:6054;branch=z9hG4bK-d87543-25653879ab08dd12-1--d87543-;rport^M
Mar 13 16:56:05 syslog[337]: From: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:05 syslog[337]: To: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:05 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:05 syslog[337]: CSeq: 1 INVITE^M
Mar 13 16:56:05 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:56:05 syslog[337]: Content-Type: application/sdp^M
Mar 13 16:56:05 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:56:05 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:05 syslog[337]: Content-Length: 201^M
Mar 13 16:56:05 syslog[337]: ^M
Mar 13 16:56:05 syslog[337]: v=0^M
Mar 13 16:56:05 syslog[337]: o=- 20015 20015 IN IP4 192.168.1.101^M
Mar 13 16:56:05 syslog[337]: s=SDP data^M
Mar 13 16:56:05 syslog[337]: c=IN IP4 192.168.1.101^M
Mar 13 16:56:05 syslog[337]: t=0 0^M
Mar 13 16:56:05 syslog[337]: m=audio 11796 RTP/AVP 0 101^M
Mar 13 16:56:05 syslog[337]: a=rtpmap:0 PCMU/8000^M
Mar 13 16:56:05 syslog[337]: a=sendrecv^M
Mar 13 16:56:05 syslog[337]: a=fmtp:101 0-15^M
Mar 13 16:56:05 syslog[337]: a=rtpmap:101 telephone-event/8000^M
Mar 13 16:56:05 syslog[337]: 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:56:05 syslog[337]: ACK sip:101@192.168.1.101:5062 SIP/2.0^M
Mar 13 16:56:05 syslog[337]: Via: SIP/2.0/UDP 192.168.1.5:6054;branch=z9hG4bK-d87543-e934b648d809db6d-1--d87543-;rport^M
Mar 13 16:56:05 syslog[337]: Max-Forwards: 70^M
Mar 13 16:56:05 syslog[337]: Contact: <sip:108@192.168.1.5:6054>^M
Mar 13 16:56:05 syslog[337]: To: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:05 syslog[337]: From: "108"<sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:05 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:05 syslog[337]: CSeq: 1 ACK^M
Mar 13 16:56:05 syslog[337]: User-Agent: eyeBeam release 3010n stamp 19039^M
Mar 13 16:56:05 syslog[337]: Content-Length: 0^M
Mar 13 16:56:05 syslog[337]: ^M
Mar 13 16:56:05 syslog[337]: 
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.5:6054
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | This is a request
Mar 13 16:56:05 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [ACK received!] 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Message received: [(SIP_MSG_CALL_HOLD) -- (0x40006)  wParam(0x73)-lParam(0x1)] 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | sipua_call_build_reinvite by callid = [115] 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Bandwidth is zero, unset the b= field
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Offer: SRTP disabled
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Last DTMF Payload is 101 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Bandwidth is zero, unset the b= field
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:08 syslog[337]: INVITE sip:108@192.168.1.5:6054 SIP/2.0^M
Mar 13 16:56:08 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK343690854^M
Mar 13 16:56:08 syslog[337]: From: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:08 syslog[337]: To: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:08 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:08 syslog[337]: CSeq: 2 INVITE^M
Mar 13 16:56:08 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:56:08 syslog[337]: Content-Type: application/sdp^M
Mar 13 16:56:08 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:56:08 syslog[337]: Max-Forwards: 70^M
Mar 13 16:56:08 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:08 syslog[337]: Allow-Events: talk,hold,conference,refer,check-sync^M
Mar 13 16:56:08 syslog[337]: Content-Length: 296^M
Mar 13 16:56:08 syslog[337]: ^M
Mar 13 16:56:08 syslog[337]: v=0^M
Mar 13 16:56:08 syslog[337]: o=- 20015 20016 IN IP4 192.168.1.101^M
Mar 13 16:56:08 syslog[337]: s=SDP data^M
Mar 13 16:56:08 syslog[337]: c=IN IP4 192.168.1.101^M
Mar 13 16:56:08 syslog[337]: t=0 0^M
Mar 13 16:56:08 syslog[337]: m=audio 11796 RTP/AVP 0 8 18 9 101^M
Mar 13 16:56:08 syslog[337]: a=rtpmap:0 PCMU/8000^M
Mar 13 16:56:08 syslog[337]: a=rtpmap:8 PCMA/8000^M
Mar 13 16:56:08 syslog[337]: a=rtpmap:18 G729/8000^M
Mar 13 16:56:08 syslog[337]: a=fmtp:18 annexb=no^M
Mar 13 16:56:08 syslog[337]: a=rtpmap:9 G722/8000^M
Mar 13 16:56:08 syslog[337]: a=fmtp:101 0-15^M
Mar 13 16:56:08 syslog[337]: a=rtpmap:101 telephone-event/8000^M
Mar 13 16:56:08 syslog[337]: a=sendonly^M
Mar 13 16:56:08 syslog[337]: 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:56:08 syslog[337]: SIP/2.0 404 Not Found^M
Mar 13 16:56:08 syslog[337]: To: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:08 syslog[337]: From: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:08 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:08 syslog[337]: CSeq: 2 INVITE^M
Mar 13 16:56:08 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK343690854^M
Mar 13 16:56:08 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:56:08 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:56:08 syslog[337]: Content-Length: 0^M
Mar 13 16:56:08 syslog[337]: ^M
Mar 13 16:56:08 syslog[337]: 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:08 syslog[337]: ACK sip:108@192.168.1.5:6054 SIP/2.0^M
Mar 13 16:56:08 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK343690854^M
Mar 13 16:56:08 syslog[337]: From: <sip:101@192.168.1.100:6060>;tag=939905824^M
Mar 13 16:56:08 syslog[337]: To: "108" <sip:108@192.168.1.100:6060>;tag=1c004040^M
Mar 13 16:56:08 syslog[337]: Call-ID: e45f3163a3132b0e@aW5nZW5pZXJpYQ..^M
Mar 13 16:56:08 syslog[337]: CSeq: 2 ACK^M
Mar 13 16:56:08 syslog[337]: Content-Length: 0^M
Mar 13 16:56:08 syslog[337]: ^M
Mar 13 16:56:08 syslog[337]: 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [4xx received for Call!] 
Mar 13 16:56:08 syslog[337]: <0> | LEVEL4 | Message sent: [(PHONE_MSG_CALL_FAIL) -- (0xa0009)  wParam(0x73)-lParam(0x194)] 
Mar 13 16:56:25 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:25 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:25 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:56:25 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1623076193^M
Mar 13 16:56:25 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:56:25 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:56:25 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:56:25 syslog[337]: CSeq: 1154 REGISTER^M
Mar 13 16:56:25 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:56:25 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:56:25 syslog[337]: Max-Forwards: 70^M
Mar 13 16:56:25 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:25 syslog[337]: Expires: 60^M
Mar 13 16:56:26 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:56:26 syslog[337]: Line: 1^M
Mar 13 16:56:26 syslog[337]: Content-Length: 0^M
Mar 13 16:56:26 syslog[337]: ^M
Mar 13 16:56:26 syslog[337]: 
Mar 13 16:56:26 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:56:26 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:56:26 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:56:26 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:56:26 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:56:26 syslog[337]: CSeq: 1154 REGISTER^M
Mar 13 16:56:26 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1623076193^M
Mar 13 16:56:26 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:56:26 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:56:26 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:56:26 syslog[337]: Content-Length: 0^M
Mar 13 16:56:26 syslog[337]: Date: Sat, 13 Mar 2010 11:56:27 PST^M
Mar 13 16:56:26 syslog[337]: ^M
Mar 13 16:56:26 syslog[337]: 
Mar 13 16:56:26 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:56:26 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:56:26 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:56:40 mini_httpd[1776]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=8
Mar 13 16:56:41 mini_httpd[404]: mini_httpd.c(918):child process 1776 exit!
Mar 13 16:56:41 mini_httpd[1778]: mini_httpd.c(1378):path:/language/Spanish.js,query:
Mar 13 16:56:41 mini_httpd[404]: mini_httpd.c(918):child process 1778 exit!
Mar 13 16:56:41 mini_httpd[1779]: mini_httpd.c(1378):path:/style.css,query:
Mar 13 16:56:41 mini_httpd[404]: mini_httpd.c(918):child process 1779 exit!
Mar 13 16:56:41 mini_httpd[1780]: mini_httpd.c(1378):path:/utility.js,query:
Mar 13 16:56:41 mini_httpd[404]: mini_httpd.c(918):child process 1780 exit!
Mar 13 16:56:45 mini_httpd[1781]: mini_httpd.c(1378):path:/image02/bg.gif,query:
Mar 13 16:56:45 mini_httpd[404]: mini_httpd.c(918):child process 1781 exit!
Mar 13 16:56:45 mini_httpd[1782]: mini_httpd.c(1378):path:/image02/top01.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1782 exit!
Mar 13 16:56:46 mini_httpd[1783]: mini_httpd.c(1378):path:/image02/top02.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1783 exit!
Mar 13 16:56:46 mini_httpd[1784]: mini_httpd.c(1378):path:/image02/top03.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1784 exit!
Mar 13 16:56:46 mini_httpd[1785]: mini_httpd.c(1378):path:/image02/top05.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1785 exit!
Mar 13 16:56:46 mini_httpd[1786]: mini_httpd.c(1378):path:/image02/button04.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1786 exit!
Mar 13 16:56:46 mini_httpd[1787]: mini_httpd.c(1378):path:/image02/button05.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1787 exit!
Mar 13 16:56:46 mini_httpd[1788]: mini_httpd.c(1378):path:/image02/top04.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1788 exit!
Mar 13 16:56:46 mini_httpd[1789]: mini_httpd.c(1378):path:/image02/button06.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1789 exit!
Mar 13 16:56:46 mini_httpd[1790]: mini_httpd.c(1378):path:/image02/button02.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1790 exit!
Mar 13 16:56:46 mini_httpd[1791]: mini_httpd.c(1378):path:/image02/button03.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1791 exit!
Mar 13 16:56:46 mini_httpd[1792]: mini_httpd.c(1378):path:/image02/button01.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1792 exit!
Mar 13 16:56:46 mini_httpd[1793]: mini_httpd.c(1378):path:/image02/longline.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1793 exit!
Mar 13 16:56:46 mini_httpd[1794]: mini_httpd.c(1378):path:/image02/note.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1794 exit!
Mar 13 16:56:46 mini_httpd[1795]: mini_httpd.c(1378):path:/image02/end.gif,query:
Mar 13 16:56:46 mini_httpd[404]: mini_httpd.c(918):child process 1795 exit!
Mar 13 16:56:48 mini_httpd[1796]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=33
Mar 13 16:56:49 syslog: https.c(1592): error
Mar 13 16:56:49 mini_httpd[404]: mini_httpd.c(918):child process 1796 exit!
Mar 13 16:56:51 mini_httpd[1798]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=32
Mar 13 16:56:52 syslog: https.c(1660): mkdir /yealink/config/certs
Mar 13 16:56:52 mini_httpd[404]: mini_httpd.c(918):child process 1798 exit!
Mar 13 16:56:54 mini_httpd[1802]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=8
Mar 13 16:56:54 mini_httpd[404]: mini_httpd.c(918):child process 1802 exit!
Mar 13 16:56:56 mini_httpd[1804]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=7
Mar 13 16:56:56 mini_httpd[404]: mini_httpd.c(918):child process 1804 exit!
Mar 13 16:56:56 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:56:56 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:56:56 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:56:56 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1497119717^M
Mar 13 16:56:56 mini_httpd[1806]: mini_httpd.c(1378):path:/image02/button07.gif,query:
Mar 13 16:56:56 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:56:56 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:56:56 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:56:56 syslog[337]: CSeq: 1155 REGISTER^M
Mar 13 16:56:56 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:56:56 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:56:56 syslog[337]: Max-Forwards: 70^M
Mar 13 16:56:56 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:56:56 syslog[337]: Expires: 60^M
Mar 13 16:56:56 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:56:56 syslog[337]: Line: 1^M
Mar 13 16:56:56 syslog[337]: Content-Length: 0^M
Mar 13 16:56:56 syslog[337]: ^M
Mar 13 16:56:56 syslog[337]: 
Mar 13 16:56:56 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:56:56 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:56:56 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:56:56 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:56:56 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:56:57 syslog[337]: CSeq: 1155 REGISTER^M
Mar 13 16:56:57 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK1497119717^M
Mar 13 16:56:57 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:56:57 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:56:57 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:56:57 syslog[337]: Content-Length: 0^M
Mar 13 16:56:57 syslog[337]: Date: Sat, 13 Mar 2010 11:56:58 PST^M
Mar 13 16:56:57 syslog[337]: ^M
Mar 13 16:56:57 syslog[337]: 
Mar 13 16:56:57 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:56:57 mini_httpd[404]: mini_httpd.c(918):child process 1806 exit!
Mar 13 16:56:57 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:56:57 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:56:59 mini_httpd[1807]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=16
Mar 13 16:57:00 mini_httpd[404]: mini_httpd.c(918):child process 1807 exit!
Mar 13 16:57:00 mini_httpd[1809]: mini_httpd.c(1378):path:/baseXHR.js,query:
Mar 13 16:57:00 mini_httpd[404]: mini_httpd.c(918):child process 1809 exit!
Mar 13 16:57:12 mini_httpd[1810]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=7
Mar 13 16:57:12 mini_httpd[404]: mini_httpd.c(918):child process 1810 exit!
Mar 13 16:57:16 mini_httpd[1812]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=16
Mar 13 16:57:17 mini_httpd[404]: mini_httpd.c(918):child process 1812 exit!
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | Set Option: dns cache used:192.168.1.100 -> 192.168.1.100
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | Message sent: (to dest=192.168.1.100:6060)
Mar 13 16:57:27 syslog[337]: REGISTER sip:192.168.1.100:6060 SIP/2.0^M
Mar 13 16:57:27 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK777697078^M
Mar 13 16:57:27 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:57:27 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>^M
Mar 13 16:57:27 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:57:27 syslog[337]: CSeq: 1156 REGISTER^M
Mar 13 16:57:27 syslog[337]: Contact: <sip:101@192.168.1.101:5062>^M
Mar 13 16:57:27 syslog[337]: Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE^M
Mar 13 16:57:27 syslog[337]: Max-Forwards: 70^M
Mar 13 16:57:27 syslog[337]: User-Agent: Yealink SIP-T20P 9.43.0.21 00:15:65:14:5a:e1^M
Mar 13 16:57:27 syslog[337]: Expires: 60^M
Mar 13 16:57:27 syslog[337]: Mac: 001565145ae1^M
Mar 13 16:57:27 syslog[337]: Line: 1^M
Mar 13 16:57:27 syslog[337]: Content-Length: 0^M
Mar 13 16:57:27 syslog[337]: ^M
Mar 13 16:57:27 syslog[337]: 
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | Received message: 
Mar 13 16:57:27 syslog[337]: SIP/2.0 200 OK^M
Mar 13 16:57:27 syslog[337]: To: "TEST101" <sip:101@192.168.1.100:6060>;tag=60b7acd9-0^M
Mar 13 16:57:27 syslog[337]: From: "TEST101" <sip:101@192.168.1.100:6060>;tag=1478954625^M
Mar 13 16:57:27 syslog[337]: Call-ID: 1190409395@192.168.1.101^M
Mar 13 16:57:27 syslog[337]: CSeq: 1156 REGISTER^M
Mar 13 16:57:27 syslog[337]: Via: SIP/2.0/UDP 192.168.1.101:5062;branch=z9hG4bK777697078^M
Mar 13 16:57:27 syslog[337]: Contact: sip:101@192.168.1.101:5062;expires=60^M
Mar 13 16:57:27 syslog[337]: Server: Linksys/SPA9000-6.1.5^M
Mar 13 16:57:27 syslog[337]: Allow-Events: talk, hold, conference^M
Mar 13 16:57:27 syslog[337]: Content-Length: 0^M
Mar 13 16:57:27 syslog[337]: Date: Sat, 13 Mar 2010 11:57:29 PST^M
Mar 13 16:57:27 syslog[337]: ^M
Mar 13 16:57:27 syslog[337]: 
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | Message received from: 192.168.1.100:6060
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | STATE MACHINE MSG: [User is successfully registred!] 
Mar 13 16:57:27 syslog[337]: <0> | LEVEL4 | Register expire time updated to (60)
Mar 13 16:57:44 mini_httpd[1814]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=27
Mar 13 16:57:44 mini_httpd[404]: mini_httpd.c(918):child process 1814 exit!
Mar 13 16:57:44 mini_httpd[1815]: mini_httpd.c(1378):path:/cgi-bin/ConfigManApp.com,query:Id=27
  PID  Uid        VSZ Stat Command
    1 root       2784 SW  init       
    2 root            SW  [ksoftirqd/0]
    3 root            SW< [desched/0]
    4 root            SW< [events/0]
    5 root            SW< [khelper]
   10 root            SW< [kthread]
   13 root            SW< [kblockd/0]
   39 root            SW  [pdflush]
   40 root            SW  [pdflush]
   42 root            SW< [aio/0]
   41 root            SW  [kswapd0]
   59 root            SW  [mtdblockd]
   48 root            SW  [kseriod]
   85 root            SW< [IRQ 8]
   88 root            SW< [IRQ 15]
  133 root            SWN [jffs2_gcd_mtd4]
  178 root       2228 SW  /sbin/syslogd -S -O /tmp/Messages -s 100 -b5 
  210 root            SW< [IRQ 35]
  237 root       6404 SW  acd esw0 192.168.1.101  
  245 root       2784 SWN /bin/sh /yealink/scripts/NTPClient.sh 
  289 root       6100 SW  /yealink/bin/pcap.exx 
  292 root       2784 SW  /bin/sh /yealink/scripts/SipApp.sh 
  293 root       7788 SW  /yealink/bin/autop.exe all 
  294 root       2784 SW  /bin/sh /yealink/scripts/VpmApp.sh 
  296 root       2784 SW  init       
  300 root       2784 SW  /bin/sh /yealink/scripts/TalkLogicApp.sh 
  301 root       2784 SW  /bin/sh /yealink/scripts/FrameApp.sh 
  302 root       6196 SW  /yealink/bin/ContactList.exe 
  303 root       2448 SW  syslog 
  304 root       6176 SW  /yealink/bin/CallList.exe 
  305 root       2448 SW  syslog 
  306 root       5408 SW  /yealink/bin/Screen.exe 
  318 root       2448 SW  syslog 
  319 root       6140 SW  /yealink/bin/Test.exe 
  330 root            SW< [IRQ 13]
  336 root       9604 SW  /yealink/bin/sipServer.exx 
  337 root       2448 SW  syslog 
  338 root       9604 SW  /yealink/bin/sipServer.exx 
  339 root       9604 SWN /yealink/bin/sipServer.exx 
  340 root       8860 SW  /yealink/bin/TalkLogic.exe 
  342 root       6604 SW  /yealink/bin/Frame.exe 
  343 root       8860 SW  /yealink/bin/TalkLogic.exe 
  344 root       8860 SW  /yealink/bin/TalkLogic.exe 
  345 root       9604 SWN /yealink/bin/sipServer.exx 
  355 root       5408 SW  /yealink/bin/Screen.exe 
  356 root            SW< [IRQ 29]
  359 root       5408 SW  /yealink/bin/Screen.exe 
  360 root       5408 DW  /yealink/bin/Screen.exe 
  361 root            SW< [IRQ 45]
  372 root       9604 SW  /yealink/bin/sipServer.exx 
  374 root       8660 SW  /yealink/bin/ggsvca_ipp 
  375 root       8660 SW  /yealink/bin/ggsvca_ipp 
  376 root       8660 SW  /yealink/bin/ggsvca_ipp 
  377 root       8660 SW  /yealink/bin/ggsvca_ipp 
  378 root       8660 SW  /yealink/bin/ggsvca_ipp 
  380 root       8660 SW  /yealink/bin/ggsvca_ipp 
  381 root       8660 SW  /yealink/bin/ggsvca_ipp 
  382 root       8660 SW  /yealink/bin/ggsvca_ipp 
  383 root       8660 SW  /yealink/bin/ggsvca_ipp 
  384 root       8660 SW  /yealink/bin/ggsvca_ipp 
  385 root       8660 SW  /yealink/bin/ggsvca_ipp 
  386 root       8660 SW  /yealink/bin/ggsvca_ipp 
  387 root       8660 SW  /yealink/bin/ggsvca_ipp 
  388 root       8660 SW  /yealink/bin/ggsvca_ipp 
  401 root       4248 SW  /bin/mini_httpds -p 443 -S -d /yealink/html -c cgi-bi
  404 root       4248 SW  /bin/mini_httpd -p 80 -d /yealink/html -c cgi-bin/** 
  418 root       2784 SW  /usr/sbin/inetd 
  422 root       4448 SWN /yealink/bin/macd 
  577 root       9604 SW  /yealink/bin/sipServer.exx 
 1775 root       1760 SWN sleep 1000 
 1815 root       9012 SWN ConfigManApp.com 
 1816 root       4248 SW  /bin/mini_httpd -p 80 -d /yealink/html -c cgi-bin/** 
 1817 root       2784 SWN sh -c cd /tmp;ifconfig >> Messages;ps >> Messages;tar
 1818 root       2784 RWN ps