ccme#
ccme#sh voice reg
ccme#sh voice register all
VOICE REGISTER GLOBAL
=====================
CONFIG [Version=4.1(0)]
========================
  Version 4.1(0)
  Mode is cme
  Max-pool is 20
  Max-dn is 25
  Source-address is 192.168.1.12 port 5060
  Authenticate register
  Authenticate realm mydomain.com
  Time-format is 24
  Date-format is D/M/Y
  Time-zone is 5
  Hold-alert is disabled
  Mwi stutter is disabled
  Mwi registration for full E.164 is disabled
  Forwarding local is enabled
  Dst auto adjust is enabled
    start at Apr week 1 day Sun time 02:00
    stop  at Oct week 8 day Sun time 02:00
  Max redirect number is 5
  Telnet Level: 0
  Tftp path is flash:
  Generate text file is disabled
  Tftp files are created, current syncinfo 0015020029507155
  OS79XX.TXT is not created
  timeout interdigit 10
  network-locale[0] US    (This is the default network locale for this box)
  network-locale[1] US 
  network-locale[2] US 
  network-locale[3] US 
  network-locale[4] US 
  user-locale[0] US    (This is the default user locale for this box)
  user-locale[1] US 
  user-locale[2] US 
  user-locale[3] US 
  user-locale[4] US 

VOICE REGISTER DN
=================
Dn Tag 1
Config:
  Number is 561
  Preference is 0
  Huntstop is disabled
  Allow watch is enabled
  Auto answer is disabled
Dn Tag 2
Config:
  Number is 564
  Preference is 0
  Huntstop is disabled
  Name XLITE MAC
  Allow watch is enabled
  Auto answer is disabled
  Label is 564
Dn Tag 3
Config:
  Number is 560
  Preference is 0
  Huntstop is disabled
  Name EYEBEAM PC
  Allow watch is enabled
  Auto answer is disabled
  Label is 560

VOICE REGISTER TEMPLATE
=======================

VOICE REGISTER DIALPLAN
=======================

VOICE REGISTER POOL
===================
Pool Tag 1
Config:
  Mac address is 0026.BB56.7FE0
  Type is 7970
  Number list 1 : DN 1
  Proxy Ip address is 0.0.0.0
  DTMF Relay is enabled, sip-notify
  Call Waiting is enabled
  DnD is disabled
  keep-conference is enabled
  username 561 password veerd003
  kpml signal is enabled
  service-control mechanism is not supported

Dialpeers created:

Statistics:
  Active registrations  : 0

  Total Registration Statistics
    Registration requests  : 0
    Registration success   : 0
    Registration failed    : 0
    unRegister requests    : 0
    unRegister success     : 0
    unRegister failed      : 0

Pool Tag 2
Config:
  Mac address is 0000.0000.0000
  Number list 1 : DN 2
  Proxy Ip address is 0.0.0.0
  DTMF Relay is enabled, sip-notify
  Call Waiting is enabled
  DnD is disabled
  keep-conference is enabled
  username 564 password veerd003
  service-control mechanism is not supported
  registration Call ID is N2VhOGQwMWYyMzdiOGEzODMxODIwODJhMGM0ZWMzMDI. 
  active primary line is: 564

  contact IP address: 192.168.1.106 port 47928

Dialpeers created:

dial-peer voice 40001 voip
 destination-pattern 564
 session target ipv4:192.168.1.106:47928
 session protocol sipv2
 dtmf-relay sip-notify
 voice-class codec 1
  after-hours-exempt   FALSE          

Statistics:
  Active registrations  : 1

  Total Registration Statistics
    Registration requests  : 1
    Registration success   : 1
    Registration failed    : 0
    unRegister requests    : 0
    unRegister success     : 0
    unRegister failed      : 0

Pool Tag 3
Config:
  Mac address is 0000.0000.0000
  Number list 1 : DN 3
  Proxy Ip address is 0.0.0.0
  DTMF Relay is enabled, sip-notify
  Call Waiting is enabled
  DnD is disabled
  keep-conference is enabled
  username 560 password veerd003
  service-control mechanism is not supported
  registration Call ID is 6d1cdf77206d066dOGU3MTM1ZWNhNzVmNzgxMDQzMTEzZTE4MTBiYTYzNTA. 
  active primary line is: 560

  contact IP address: 192.168.1.108 port 15664

Dialpeers created:

dial-peer voice 40002 voip
 destination-pattern 560
 session target ipv4:192.168.1.108:15664
 session protocol sipv2
 dtmf-relay sip-notify
 voice-class codec 1
  after-hours-exempt   FALSE          

Statistics:
  Active registrations  : 1

  Total Registration Statistics
    Registration requests  : 1
    Registration success   : 1
    Registration failed    : 0
    unRegister requests    : 0
    unRegister success     : 0
    unRegister failed      : 0

ccme#
ccme#show sip-ua regi
ccme#show sip-ua register status
Line          peer           expires(sec)  registered 
============  =============  ============  ===========
ccme#