dial-peer voice 10 voip
 description Inbound CUCM to CUBE
 huntstop
 session protocol sipv2
 session target ipv4:10.1.1.135
 incoming called-number .
 voice-class codec 1  
 dtmf-relay rtp-nte
dial-peer voice 20 voip
 description Outbound CUCM to CUBE
 huntstop
 destination-pattern 2..
 session protocol sipv2
 session target ipv4:10.1.1.135
 voice-class codec 1  
 dtmf-relay rtp-nte
dial-peer voice 100 voip
 description Inbound ITSP to CUBE
 translation-profile incoming Extensions
 huntstop
 session protocol sipv2
 session target sip-server
 incoming called-number 08627027..
 voice-class codec 1  
 voice-class sip profiles 3
 dtmf-relay rtp-nte
dial-peer voice 200 voip
 description Outbound CUBE to ITSP
 huntstop
 destination-pattern .T
 session protocol sipv2
 session target sip-server
 voice-class codec 1  
 voice-class sip profiles 3
 dtmf-relay rtp-nte