CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000065: *Oct 22 20:01:21: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK74f02ab8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:20 GMT
CSeq: 101 INVITE
User-Agent: Cisco-CP9971/9.2.1
Contact: <sip:2001@192.168.3.3:5060;transport=udp>
Expires: 180
Accept: application/sdp
Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Supported: replaces,join,sdp-anat,norefersub,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-5.1.0,X-cisco-xsi-8.0.1
Allow-Events: kpml,dialog
Content-Length: 573
Content-Type: application/sdp
Content-Disposition: session;handling=optional

v=0
o=Cisco-SIPUA 18280 0 IN IP4 192.168.3.3
s=SIP Call
t=0 0
m=audio 20310 RTP/AVP 8 0 18 102 116 101
c=IN IP4 192.168.3.3
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:102 L16/16000
a=rtpmap:116 iLBC/8000
a=fmtp:116 mode=20
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
m=video 29254 RTP/AVP 97
c=IN IP4 192.168.3.3
b=TIAS:1000000
a=rtpmap:97 H264/90000
a=fmtp:97 profile-level-id=42801E;packetization-mode=0;level-asymmetry-allowed=1
a=imageattr:* recv [x=640,y=480,q=0.50]
a=sendrecv

000066: *Oct 22 20:01:21: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK74f02ab8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>
Date: Mon, 22 Oct 2018 20:01:21 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 101 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000067: *Oct 22 20:01:21: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 

CME_2801#
CME_2801#
CME_2801#SIP/2.0 180 Ringing
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK74f02ab8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:21 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 101 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000068: *Oct 22 20:01:24: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK74f02ab8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:21 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 101 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Disposition: session;handling=required
Content-Length: 228

v=0
o=CiscoSystemsSIP-GW-UserAgent 7206 3851 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17670 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
m=video 0 RTP/AVP 97
c=IN IP4 192.168.3.254

000069: *Oct 22 20:01:24: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK0f917f1d
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:23 GMT
CSeq: 101 ACK
User-Agent: Cisco-CP9971/9.2.1
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#hold now————————————————————————Press HOLD button————————————————————————
          ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000070: *Oct 22 20:01:32: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK5f5558d1
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:31 GMT
CSeq: 102 INVITE
User-Agent: Cisco-CP9971/9.2.1
Contact: <sip:2001@192.168.3.3:5060;transport=udp>
Accept: application/sdp
Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Call-Info: <urn:x-cisco-remotecc:hold>
Supported: replaces,join,sdp-anat,norefersub,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-5.1.0,X-cisco-xsi-8.0.1
Allow-Events: kpml,dialog
Content-Length: 573
Content-Type: application/sdp
Content-Disposition: session;handling=optional

v=0
o=Cisco-SIPUA 18280 1 IN IP4 192.168.3.3
s=SIP Call
t=0 0
m=audio 20310 RTP/AVP 8 0 18 102 116 101
c=IN IP4 192.168.3.3
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:102 L16/16000
a=rtpmap:116 iLBC/8000
a=fmtp:116 mode=20
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendonly
m=video 25466 RTP/AVP 97
c=IN IP4 192.168.3.3
b=TIAS:1000000
a=rtpmap:97 H264/90000
a=fmtp:97 profile-level-id=42801E;packetization-mode=0;level-asymmetry-allowed=1
a=imageattr:* recv [x=640,y=480,q=0.50]
a=sendonly

000071: *Oct 22 20:01:32: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK5f5558d1
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:32 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 102 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000072: *Oct 22 20:01:32: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK5f5558d1
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:32 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 102 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 240

v=0
o=CiscoSystemsSIP-GW-UserAgent 7206 3852 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17670 RTP/AVP 8
c=IN IP4 192.168.3.254
a=recvonly
a=rtpmap:8 PCMA/8000
m=video 0 RTP/AVP 97
c=IN IP4 192.168.3.254

000073: *Oct 22 20:01:32: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK5900ab11
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:31 GMT
CSeq: 102 ACK
User-Agent: Cisco-CP9971/9.2.1
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#un-hold now———————————————————Press Resume the call to un-hold—————————————————————
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
000074: *Oct 22 20:01:48: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
INVITE sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK4b0f9acf
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:47 GMT
CSeq: 103 INVITE
User-Agent: Cisco-CP9971/9.2.1
Contact: <sip:2001@192.168.3.3:5060;transport=udp>
Accept: application/sdp
Allow: ACK,BYE,CANCEL,INVITE,NOTIFY,OPTIONS,REFER,REGISTER,UPDATE,SUBSCRIBE,INFO
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Call-Info: <urn:x-cisco-remotecc:resume>
Supported: replaces,join,sdp-anat,norefersub,extended-refer,X-cisco-callinfo,X-cisco-serviceuri,X-cisco-escapecodes,X-cisco-service-control,X-cisco-srtp-fallback,X-cisco-monrec,X-cisco-config,X-cisco-sis-5.1.0,X-cisco-xsi-8.0.1
Allow-Events: kpml,dialog
Content-Length: 572
Content-Type: application/sdp
Content-Disposition: session;handling=optional

v=0
o=Cisco-SIPUA 5137 2 IN IP4 192.168.3.3
s=SIP Call
t=0 0
m=audio 20310 RTP/AVP 8 0 18 102 116 101
c=IN IP4 192.168.3.3
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:102 L16/16000
a=rtpmap:116 iLBC/8000
a=fmtp:116 mode=20
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=sendrecv
m=video 25466 RTP/AVP 97
c=IN IP4 192.168.3.3
b=TIAS:1000000
a=rtpmap:97 H264/90000
a=fmtp:97 profile-level-id=42801E;packetization-mode=0;level-asymmetry-allowed=1
a=imageattr:* recv [x=640,y=480,q=0.50]
a=sendrecv

000075: *Oct 22 20:01:48: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK4b0f9acf
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:48 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 103 INVITE
Allow-Events: telephone-event
Server: Cisco-SIPGateway/IOS-12.x
Content-Length: 0

000076: *Oct 22 20:01:48: //14/1476E1708010/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK4b0f9acf
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:01:48 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
CSeq: 103 INVITE
Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER
Allow-Events: telephone-event
Remote-Party-ID: "SCCP7941" <sip:2002@192.168.3.254>;party=called;screen=no;privacy=off
Contact: <sip:2002@192.168.3.254:5060>
Supported: replaces
Server: Cisco-SIPGateway/IOS-12.x
Supported: timer
Content-Type: application/sdp
Content-Length: 228

v=0
o=CiscoSystemsSIP-GW-UserAgent 7206 3852 IN IP4 192.168.3.254
s=SIP Call
c=IN IP4 192.168.3.254
t=0 0
m=audio 17670 RTP/AVP 8
c=IN IP4 192.168.3.254
a=rtpmap:8 PCMA/8000
m=video 0 RTP/AVP 97
c=IN IP4 192.168.3.254

000077: *Oct 22 20:01:48: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
ACK sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK637ca012
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:47 GMT
CSeq: 103 ACK
User-Agent: Cisco-CP9971/9.2.1
Remote-Party-ID: "SIP9971" <sip:2001@192.168.3.254>;party=calling;id-type=subscriber;privacy=off;screen=yes
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#end call now——————————————————————End the call now———————————————
           ^
% Invalid input detected at '^' marker.

CME_2801#
CME_2801#
CME_2801#
000078: *Oct 22 20:02:00: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Received: 
BYE sip:2002@192.168.3.254:5060 SIP/2.0
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK79dc82a8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Max-Forwards: 70
Date: Mon, 22 Oct 2018 20:01:59 GMT
CSeq: 104 BYE
User-Agent: Cisco-CP9971/9.2.1
Content-Length: 0

000079: *Oct 22 20:02:00: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:
Sent: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 192.168.3.3:5060;branch=z9hG4bK79dc82a8
From: "SIP9971" <sip:2001@192.168.3.254>;tag=18339d14d67300097762fd18-75fe34c5
To: <sip:2002@192.168.3.254>;tag=559F0-1155
Date: Mon, 22 Oct 2018 20:02:00 GMT
Call-ID: 18339d14-d6730005-623a23fb-00278e48@192.168.3.3
Server: Cisco-SIPGateway/IOS-12.x
CSeq: 104 BYE
Reason: Q.850;cause=16
P-RTP-Stat: PS=954,OS=152640,PR=340,OR=53128,PL=0,JI=0,LA=0,DU=35
Content-Length: 0

CME_2801#
CME_2801#
CME_2801#
CME_2801#
CME_2801#undebug all
All possible debugging has been turned off
CME_2801#
CME_2801#
CME_2801#
CME_2801#