Apr 14 2022 07:36:22.811 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

INVITE sip:9011525550802000@10.9.8.5:5060 SIP/2.0

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cca2e18e8fa

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

Supported: timer,resource-priority,replaces

Min-SE: 1800

User-Agent: Cisco-CUCM11.5

Allow: INVITE, OPTIONS, INFO, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY

CSeq: 101 INVITE

Expires: 180

Allow-Events: presence

Supported: X-cisco-srtp-fallback,X-cisco-original-called

Call-Info: <urn:x-cisco-remotecc:callinfo>;x-cisco-video-traffic-class=DESKTOP

Session-ID: 52380aab00105000a000285261c00ef8;remote=00000000000000000000000000000000

Cisco-Guid: 2086333568-0000065536-0000003169-0161629194

Session-Expires: 7200

P-Asserted-Identity: <sip:7791234567@10.9.8.9>

Remote-Party-ID: <sip:7791234567@10.9.8.9>;party=calling;screen=yes;privacy=off

Contact: <sip:7791234567@10.9.8.9:5060;transport=tcp>;+u.sip!devicename.ccm.cisco.com="SEP285261C00EF8"

Max-Forwards: 69

Content-Length: 0

Apr 14 2022 07:36:22.815 CDT: //-1/7C5AEC800000/CCAPI/cc\_api\_display\_ie\_subfields:

 cc\_api\_call\_setup\_ind\_common:

 cisco-username=7791234567

 ----- ccCallInfo IE subfields -----

 cisco-ani=7791234567

 cisco-anitype=0

 cisco-aniplan=0

 cisco-anipi=0

 cisco-anisi=1

 dest=9011525550802000

 cisco-desttype=0

 cisco-destplan=0

 cisco-rdie=FFFFFFFF

 cisco-rdn=

 cisco-rdntype=0

 cisco-rdnplan=0

 cisco-rdnpi=-1

 cisco-rdnsi=-1

 cisco-redirectreason=-1 fwd\_final\_type =0

 final\_redirectNumber =

 hunt\_group\_timeout =0

Apr 14 2022 07:36:22.815 CDT: //-1/7C5AEC800000/CCAPI/cc\_api\_call\_setup\_ind\_common:

 Interface=0x3E806604, Call Info(

 Calling Number=7791234567,(Calling Name=)(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed),

 Called Number=9011525550802000(TON=Unknown, NPI=Unknown),

 Calling Translated=FALSE, Subscriber Type Str=Unknown, FinalDestinationFlag=TRUE,

 Incoming Dial-peer=2, Progress Indication=NULL(0), Calling IE Present=TRUE,

 Source Trkgrp Route Label=, Target Trkgrp Route Label=, CLID Transparent=FALSE), Call Id=5611483

Apr 14 2022 07:36:22.815 CDT: //-1/7C5AEC800000/CCAPI/ccCheckClipClir:

 In: Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed)

Apr 14 2022 07:36:22.815 CDT: //-1/7C5AEC800000/CCAPI/ccCheckClipClir:

 Out: Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed)

Apr 14 2022 07:36:22.815 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.815 CDT: :cc\_get\_feature\_vsa malloc success

Apr 14 2022 07:36:22.815 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.815 CDT: cc\_get\_feature\_vsa count is 1

Apr 14 2022 07:36:22.815 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.815 CDT: :FEATURE\_VSA attributes are: feature\_name:0,feature\_time:1042264936,feature\_id:422899

Apr 14 2022 07:36:22.815 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_call\_setup\_ind\_common:

 Set Up Event Sent;

 Call Info(Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed),

 Called Number=9011525550802000(TON=Unknown, NPI=Unknown))

Apr 14 2022 07:36:22.815 CDT: //5611483/7C5AEC800000/CCAPI/cc\_process\_call\_setup\_ind:

 Event=0x22C31278

Apr 14 2022 07:36:22.815 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_setupind\_match\_search:

 Try with the demoted called number 9011525550802000

Apr 14 2022 07:36:22.815 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetContext:

 Context=0x3F645CD8

Apr 14 2022 07:36:22.815 CDT: //5611483/7C5AEC800000/CCAPI/cc\_process\_call\_setup\_ind:

 >>>>CCAPI handed cid 5611483 with tag 2 to app "\_ManagedAppProcess\_Default"

Apr 14 2022 07:36:22.815 CDT: //5611483/7C5AEC800000/CCAPI/ccCallProceeding:

 Progress Indication=NULL(0)

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetupRequest:

 Destination=, Calling IE Present=TRUE, Mode=0,

 Outgoing Dial-peer=60, Params=0x3F639A40, Progress Indication=NULL(0)

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/cc\_set\_post\_tagdata:

 CALL\_ERROR; Avlist Removal Is Failed

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/cc\_set\_post\_tagdata:

 CALL\_ERROR; Avlist Removal Is Failed

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/cc\_fill\_tg\_params:

 Not a cic call

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetupRequest:

 Trunk Group Select Interface Success;

 Interface=0x2311DA28, Selected Interface=1, Selected DSL=0

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCheckClipClir:

 In: Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed)

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCheckClipClir:

 Out: Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed)

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetupRequest:

 Destination Pattern=9011T, Called Number=011525550802000, Digit Strip=TRUE

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetupRequest:

 Calling Number=7791234567(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed),

 Called Number=011525550802000(TON=Unknown, NPI=Unknown),

 Redirect Number=, Display Info=

 Account Number=7791234567, Final Destination Flag=TRUE,

 Guid=7C5AEC80-0001-0000-0000-0C6109A2440A, Outgoing Dial-peer=60

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_display\_ie\_subfields:

 ccCallSetupRequest:

 cisco-username=7791234567

 ----- ccCallInfo IE subfields -----

 cisco-ani=7791234567

 cisco-anitype=0

 cisco-aniplan=0

 cisco-anipi=0

 cisco-anisi=1

 dest=011525550802000

 cisco-desttype=0

 cisco-destplan=0

 cisco-rdie=FFFFFFFF

 cisco-rdn=

 cisco-rdntype=0

 cisco-rdnplan=0

 cisco-rdnpi=-1

 cisco-rdnsi=-1

 cisco-redirectreason=-1 fwd\_final\_type =0

 final\_redirectNumber =

 hunt\_group\_timeout =0

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccIFCallSetupRequestPrivate:

 Interface=0x2311DA28, Interface Type=6, Destination=, Mode=0x0,

 Call Params(Calling Number=7791234567,(Calling Name=)(TON=Unknown, NPI=Unknown, Screening=User, Passed, Presentation=Allowed),

 Called Number=011525550802000(TON=Unknown, NPI=Unknown), Calling Translated=FALSE,

 Subscriber Type Str=Unknown, FinalDestinationFlag=TRUE, Outgoing Dial-peer=60, Call Count On=FALSE,

 Source Trkgrp Route Label=, Target Trkgrp Route Label=ALL\_PSTN, tg\_label\_flag=2, Application Call Id=)

Apr 14 2022 07:36:22.819 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.819 CDT: :cc\_get\_feature\_vsa malloc success

Apr 14 2022 07:36:22.819 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.819 CDT: cc\_get\_feature\_vsa count is 2

Apr 14 2022 07:36:22.819 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_get\_feature\_vsa:

Apr 14 2022 07:36:22.819 CDT: :FEATURE\_VSA attributes are: feature\_name:0,feature\_time:1042268072,feature\_id:422900

Apr 14 2022 07:36:22.819 CDT: //5611484/7C5AEC800000/CCAPI/ccIFCallSetupRequestPrivate:

 SPI Call Setup Request Is Success; Interface Type=6, FlowMode=1

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccCallSetupRequest:

 Trunk Group Call Setting;

 Call Entry(Retry Count=0, Voice Class Cause Code=0)

Apr 14 2022 07:36:22.819 CDT: //5611484/7C5AEC800000/CCAPI/ccCallSetContext:

 Context=0x3F6399F0

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/ccSaveDialpeerTag:

 Outgoing Dial-peer=60

Apr 14 2022 07:36:22.819 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_modify\_tgt\_cid\_call\_active\_record:

 Target Trkgrp Route Label=ALL\_PSTN, tg\_label\_flag=TRUE, Call Id=0x559FDB

Apr 14 2022 07:36:22.823 CDT: ISDN Se0/0/0:23 Q931: Applying typeplan for sw-type 0xD is 0x2 0x1, Calling num 7791234567

Apr 14 2022 07:36:22.823 CDT: ISDN Se0/0/0:23 Q931: Sending SETUP callref = 0x2A75 callID = 0xA979 switch = primary-ni interface = User

Apr 14 2022 07:36:22.827 CDT: //5611483/7C5AEC800000/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 100 Trying

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cca2e18e8fa

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

CSeq: 101 INVITE

Allow-Events: kpml, telephone-event

Server: Cisco-SIPGateway/IOS-15.4.3.M3

Content-Length: 0

Apr 14 2022 07:36:22.843 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_proceeding:

 Interface=0x2311DA28, Progress Indication=NULL(0)

Apr 14 2022 07:36:23.095 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_alert:

 Interface=0x2311DA28, Progress Indication=INBAND(8), Signal Indication=SIGNAL RINGBACK(1)

Apr 14 2022 07:36:23.095 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_alert:

 Call Entry(Retry Count=0, Responsed=TRUE)

Apr 14 2022 07:36:23.095 CDT: //5611483/7C5AEC800000/CCAPI/ccCallAlert:

 Progress Indication=INBAND(8), Signal Indication=SIGNAL RINGBACK(1)

Apr 14 2022 07:36:23.095 CDT: //5611483/7C5AEC800000/CCAPI/ccCallAlert:

 Call Entry(Responsed=TRUE, Alert Sent=TRUE)

Apr 14 2022 07:36:23.095 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceCreate:

 (confID=0xFFFFFFFF, callID1=0x559FDB, gcid=53A58A53-BB2611EC-AD27AE7F-6F8F82E1, tag=0x0)

Apr 14 2022 07:36:23.095 CDT: //5611484/7C5AEC800000/CCAPI/ccConferenceCreate:

 (confID=0xFFFFFFFF, callID2=0x559FDC, gcid=53A58A53-BB2611EC-AD27AE7F-6F8F82E1, tag=0x0)

Apr 14 2022 07:36:23.095 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceCreate:

 Conference Id=0xFFFFFFFF, Call Id1=5611483, Call Id2=5611484, Tag=0x0

Apr 14 2022 07:36:23.095 CDT: //5611483/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:23.099 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:23.099 CDT: //5611483/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:23.099 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_bridge\_done:

 Conference Id=0x1800C, Source Interface=0x3E806604, Source Call Id=5611483,

 Destination Call Id=5611484, Disposition=0x0, Tag=0x0

Apr 14 2022 07:36:23.099 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_bridge\_done:

 Conference Id=0x1800C, Source Interface=0x2311DA28, Source Call Id=5611484,

 Destination Call Id=5611483, Disposition=0x0, Tag=0xFFFFFFFF

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/cc\_generic\_bridge\_done:

 Conference Id=0x1800C, Source Interface=0x2311DA28, Source Call Id=5611484,

 Destination Call Id=5611483, Disposition=0x0, Tag=0xFFFFFFFF

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceCreate:

 Call Entry(Conference Id=0x1800C, Destination Call Id=5611484)

Apr 14 2022 07:36:23.099 CDT: //5611484/7C5AEC800000/CCAPI/ccConferenceCreate:

 Call Entry(Conference Id=0x1800C, Destination Call Id=5611483)

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceCreate:

Apr 14 2022 07:36:23.099 CDT: confID:0x1800C; callEntry1 callID1:0x559FDB, type:3; callEntry2 callID2:0x559FDC, type:6

Apr 14 2022 07:36:23.099 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Destination Interface=0x3E806604, Destination Call Id=5611483, Source Call Id=5611484,

 Caps(Codec=0x1, Fax Rate=0x1, Fax Version:=0, Vad=0x1,

 Modem=0x2, Codec Bytes=20, Signal Type=3)

Apr 14 2022 07:36:23.099 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Caps(Playout Mode=1, Playout Initial=60(ms), Playout Min=40(ms),

 Playout Max=1000(ms), Fax Nom=300(ms))

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Destination Interface=0x2311DA28, Destination Call Id=5611484, Source Call Id=5611483,

 Caps(Codec=0x1, Fax Rate=0x2, Fax Version:=0, Vad=0x1,

 Modem=0x0, Codec Bytes=160, Signal Type=2)

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Caps(Playout Mode=1, Playout Initial=60(ms), Playout Min=40(ms),

 Playout Max=1000(ms), Fax Nom=300(ms))

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ack:

 Destination Interface=0x2311DA28, Destination Call Id=5611484, Source Call Id=5611483,

 Caps(Codec=g711ulaw(0x1), Fax Rate=FAX\_RATE\_VOICE(0x2), Fax Version:=0, Vad=OFF(0x1),

 Modem=OFF(0x0), Codec Bytes=160, Signal Type=2, Seq Num Start=3028)

Apr 14 2022 07:36:23.099 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_caps\_ack:

 Destination Interface=0x3E806604, Destination Call Id=5611483, Source Call Id=5611484,

 Caps(Codec=g711ulaw(0x1), Fax Rate=FAX\_RATE\_VOICE(0x2), Fax Version:=0, Vad=OFF(0x1),

 Modem=OFF(0x0), Codec Bytes=160, Signal Type=2, Seq Num Start=3028)

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/ccCallNotify:

 Data Bitmask=0x7, Call Id=5611483

Apr 14 2022 07:36:23.099 CDT: //5611483/7C5AEC800000/CCAPI/ccCallNotify:

 Data Bitmask=0x7, Call Id=5611483

Apr 14 2022 07:36:23.103 CDT: //5611483/7C5AEC800000/CCAPI/cc\_process\_notify\_bridge\_done:

 Conference Id=0x1800C, Call Id1=5611483, Call Id2=5611484

Apr 14 2022 07:36:23.103 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_voice\_mode\_event:

 Call Id=5611484

Apr 14 2022 07:36:23.103 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_voice\_mode\_event:

 Call Entry(Context=0x3F6399F0)

Apr 14 2022 07:36:23.103 CDT: //5611483/7C5AEC800000/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 183 Session Progress

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cca2e18e8fa

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>;tag=E3B4CF34-2CE

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

CSeq: 101 INVITE

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

Allow-Events: kpml, telephone-event

Remote-Party-ID: <sip:011525550802000@10.9.8.5>;party=called;screen=no;privacy=off

Contact: <sip:9011525550802000@10.9.8.5:5060;transport=tcp>

Call-Info: <sip:10.9.8.5:5060>;method="NOTIFY;Event=telephone-event;Duration=2000"

Supported: sdp-anat

Server: Cisco-SIPGateway/IOS-15.4.3.M3

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 378

v=0

o=CiscoSystemsSIP-GW-UserAgent 8185 8833 IN IP4 10.9.8.5

s=SIP Call

c=IN IP4 10.9.8.5

t=0 0

m=audio 27910 RTP/AVP 0 18 8 116 101

c=IN IP4 10.9.8.5

a=rtpmap:0 PCMU/8000

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

a=maxptime:20

Apr 14 2022 07:36:23.187 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_connected:

 Interface=0x2311DA28, Data Bitmask=0x1, Progress Indication=NULL(0),

 Connection Handle=0

Apr 14 2022 07:36:23.187 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_connected:

 Call Entry(Connected=TRUE, Responsed=TRUE, Retry Count=0)

Apr 14 2022 07:36:23.187 CDT: //5611483/7C5AEC800000/CCAPI/ccCallConnect:

 Progress Indication=NULL(0), Data Bitmask=0x1

Apr 14 2022 07:36:23.187 CDT: //5611483/7C5AEC800000/CCAPI/ccCallConnect:

 Call Entry(Connected=TRUE, Responsed=TRUE)

Apr 14 2022 07:36:23.187 CDT: //5611483/7C5AEC800000/CCAPI/ccCallNotify:

 Data Bitmask=0x7, Call Id=5611483

Apr 14 2022 07:36:23.191 CDT: //5611483/7C5AEC800000/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cca2e18e8fa

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>;tag=E3B4CF34-2CE

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

CSeq: 101 INVITE

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

Allow-Events: kpml, telephone-event

Remote-Party-ID: <sip:011525550802000@10.9.8.5>;party=called;screen=no;privacy=off

Contact: <sip:9011525550802000@10.9.8.5:5060;transport=tcp>

Supported: replaces

Call-Info: <sip:10.9.8.5:5060>;method="NOTIFY;Event=telephone-event;Duration=2000"

Supported: sdp-anat

Server: Cisco-SIPGateway/IOS-15.4.3.M3

Require: timer

Session-Expires: 7200;refresher=uac

Supported: timer

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 378

v=0

o=CiscoSystemsSIP-GW-UserAgent 8185 8833 IN IP4 10.9.8.5

s=SIP Call

c=IN IP4 10.9.8.5

t=0 0

m=audio 27910 RTP/AVP 0 18 8 116 101

c=IN IP4 10.9.8.5

a=rtpmap:0 PCMU/8000

a=rtpmap:18 G729/8000

a=fmtp:18 annexb=no

a=rtpmap:8 PCMA/8000

a=rtpmap:116 iLBC/8000

a=fmtp:116 mode=20

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

a=maxptime:20

Apr 14 2022 07:36:23.199 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

ACK sip:9011525550802000@10.9.8.5:5060;transport=tcp SIP/2.0

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81ccb3895f833

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>;tag=E3B4CF34-2CE

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

User-Agent: Cisco-CUCM11.5

Max-Forwards: 70

CSeq: 101 ACK

Allow-Events: presence

Session-ID: 52380aab00105000a000285261c00ef8;remote=e0d2c66d5577b66dfec376fab2668512

Content-Type: application/sdp

Content-Length: 237

v=0

o=CiscoSystemsCCM-SIP 2668512 1 IN IP4 10.9.8.9

s=SIP Call

c=IN IP4 10.9.8.13

b=TIAS:64000

b=AS:64

t=0 0

m=audio 27986 RTP/AVP 0 101

a=ptime:20

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

Apr 14 2022 07:36:23.203 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Destination Interface=0x2311DA28, Destination Call Id=5611484, Source Call Id=5611483,

 Caps(Codec=0x1, Fax Rate=0x2, Fax Version:=0, Vad=0x1,

 Modem=0x0, Codec Bytes=160, Signal Type=2)

Apr 14 2022 07:36:23.203 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ind:

 Caps(Playout Mode=1, Playout Initial=60(ms), Playout Min=40(ms),

 Playout Max=1000(ms), Fax Nom=300(ms))

Apr 14 2022 07:36:23.203 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_caps\_ack:

 Destination Interface=0x2311DA28, Destination Call Id=5611484, Source Call Id=5611483,

 Caps(Codec=g711ulaw(0x1), Fax Rate=FAX\_RATE\_VOICE(0x2), Fax Version:=0, Vad=OFF(0x1),

 Modem=OFF(0x0), Codec Bytes=160, Signal Type=2, Seq Num Start=6092)

Apr 14 2022 07:36:23.203 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_caps\_ack:

 Destination Interface=0x3E806604, Destination Call Id=5611483, Source Call Id=5611484,

 Caps(Codec=g711ulaw(0x1), Fax Rate=FAX\_RATE\_VOICE(0x2), Fax Version:=0, Vad=OFF(0x1),

 Modem=OFF(0x0), Codec Bytes=160, Signal Type=2, Seq Num Start=6092)

Apr 14 2022 07:36:23.203 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_voice\_mode\_event:

 Call Id=5611484

Apr 14 2022 07:36:23.203 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_voice\_mode\_event:

 Call Entry(Context=0x3F6399F0)

Apr 14 2022 07:36:30.915 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

BYE sip:9011525550802000@10.9.8.5:5060;transport=tcp SIP/2.0

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81ccf13f8c5ea

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>;tag=E3B4CF34-2CE

Date: Thu, 14 Apr 2022 12:36:22 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

User-Agent: Cisco-CUCM11.5

Max-Forwards: 70

P-Asserted-Identity: <sip:7791234567@10.9.8.9>

CSeq: 102 BYE

Reason: Q.850;cause=16

Session-ID: 52380aab00105000a000285261c00ef8;remote=e0d2c66d5577b66dfec376fab2668512

Content-Length: 0

Apr 14 2022 07:36:30.915 CDT: //5611484/7C5AEC800000/CCAPI/ccGenerateToneInfo:

 Stop Tone On Digit=FALSE, Tone=Null,

 Tone Direction=Sum Network, Params=0x0, Call Id=5611484

Apr 14 2022 07:36:30.915 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_call\_disconnected:

 Cause Value=16, Interface=0x3E806604, Call Id=5611483

Apr 14 2022 07:36:30.915 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_call\_disconnected:

 Call Entry(Responsed=TRUE, Cause Value=16, Retry Count=0)

Apr 14 2022 07:36:30.915 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceDestroy:

 Conference Id=0x1800C, Tag=0x0

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/ccConferenceDestroy:

Apr 14 2022 07:36:30.919 CDT: confID:0x1800C; callEntry1 callID1:0x559FDB, type:3; callEntry2 callID2:0x559FDC, type:6

Apr 14 2022 07:36:30.919 CDT: //5611483/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:30.919 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:30.919 CDT: //5611484/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:30.919 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:30.919 CDT: //5611483/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:30.919 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:30.919 CDT: //5611483/xxxxxxxxxxxx/CCAPI/cc\_api\_get\_xcode\_stream:

Apr 14 2022 07:36:30.919 CDT: cc\_api\_get\_xcode\_stream : 4982

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/cc\_set\_post\_tagdata:

 CALL\_ERROR; Avlist Removal Is Failed

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/cc\_set\_post\_tagdata:

 CALL\_ERROR; Avlist Removal Is Failed

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_bridge\_drop\_done:

 Conference Id=0x1800C, Source Interface=0x3E806604, Source Call Id=5611483,

 Destination Call Id=5611484, Disposition=0x0, Tag=0x0

Apr 14 2022 07:36:30.919 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_bridge\_drop\_done:

 Conference Id=0x1800C, Source Interface=0x2311DA28, Source Call Id=5611484,

 Destination Call Id=5611483, Disposition=0x0, Tag=0x0

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/cc\_generic\_bridge\_done:

 Conference Id=0x1800C, Source Interface=0x2311DA28, Source Call Id=5611484,

 Destination Call Id=5611483, Disposition=0x0, Tag=0x0

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/ccCallDisconnect:

 Cause Value=16, Tag=0x0, Call Entry(Previous Disconnect Cause=0, Disconnect Cause=16)

Apr 14 2022 07:36:30.919 CDT: //5611483/7C5AEC800000/CCAPI/ccCallDisconnect:

 Cause Value=16, Call Entry(Responsed=TRUE, Cause Value=16)

Apr 14 2022 07:36:30.919 CDT: //5611484/7C5AEC800000/CCAPI/ccCallDisconnect:

 Cause Value=16, Tag=0x0, Call Entry(Previous Disconnect Cause=0, Disconnect Cause=0)

Apr 14 2022 07:36:30.919 CDT: //5611484/7C5AEC800000/CCAPI/ccCallDisconnect:

 Cause Value=16, Call Entry(Responsed=TRUE, Cause Value=16)

Apr 14 2022 07:36:30.919 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_get\_transfer\_info:

 Transfer Number=NULL

Apr 14 2022 07:36:30.927 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_call\_disconnect\_done:

 Disposition=0, Interface=0x3E806604, Tag=0x0, Call Id=5611483,

 Call Entry(Disconnect Cause=16, Voice Class Cause Code=0, Retry Count=0)

Apr 14 2022 07:36:30.931 CDT: //5611483/7C5AEC800000/CCAPI/cc\_api\_call\_disconnect\_done:

 Call Disconnect Event Sent

Apr 14 2022 07:36:30.931 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_free\_feature\_vsa:

Apr 14 2022 07:36:30.931 CDT: :cc\_free\_feature\_vsa freeing 3E1FB360

Apr 14 2022 07:36:30.931 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_free\_feature\_vsa:

Apr 14 2022 07:36:30.931 CDT: vsacount in free is 1

Apr 14 2022 07:36:30.931 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81ccf13f8c5ea

From: <sip:7791234567@10.9.8.9>;tag=2668512~822a1999-125e-4057-b862-622bb2f3d3da-38246533

To: <sip:9011525550802000@10.9.8.5>;tag=E3B4CF34-2CE

Date: Thu, 14 Apr 2022 12:36:30 GMT

Call-ID: 7c5aec80-25811546-7cde2-9a2440a@10.9.8.9

Server: Cisco-SIPGateway/IOS-15.4.3.M3

CSeq: 102 BYE

Reason: Q.850;cause=16

P-RTP-Stat: PS=384,OS=61440,PR=377,OR=60320,PL=0,JI=0,LA=2,DU=7

Content-Length: 0

Apr 14 2022 07:36:30.931 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

OPTIONS sip:10.9.8.5:5060 SIP/2.0

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cd15d5f9de7

From: <sip:10.9.8.9>;tag=550611267

To: <sip:10.9.8.5>

Date: Thu, 14 Apr 2022 12:36:30 GMT

Call-ID: 811fa080-2581154e-7cde5-9a2440a@10.9.8.9

User-Agent: Cisco-CUCM11.5

CSeq: 101 OPTIONS

Contact: <sip:10.9.8.9:5060;transport=tcp>

Max-Forwards: 0

Content-Length: 0

Apr 14 2022 07:36:30.935 CDT: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

SIP/2.0 200 OK

Via: SIP/2.0/TCP 10.9.8.9:5060;branch=z9hG4bK81cd15d5f9de7

From: <sip:10.9.8.9>;tag=550611267

To: <sip:10.9.8.5>;tag=E3B4EDCC-5EF

Date: Thu, 14 Apr 2022 12:36:30 GMT

Call-ID: 811fa080-2581154e-7cde5-9a2440a@10.9.8.9

Server: Cisco-SIPGateway/IOS-15.4.3.M3

CSeq: 101 OPTIONS

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

Allow-Events: telephone-event

Accept: application/sdp

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Content-Type: application/sdp

Content-Length: 366

v=0

o=CiscoSystemsSIP-GW-UserAgent 581 6421 IN IP4 10.9.8.5

s=SIP Call

c=IN IP4 10.9.8.5

t=0 0

m=audio 0 RTP/AVP 18 0 8 9 4 2 15

c=IN IP4 10.9.8.5

m=image 0 udptl t38

c=IN IP4 10.9.8.5

a=T38FaxVersion:0

a=T38MaxBitRate:9600

a=T38FaxRateManagement:transferredTCF

a=T38FaxMaxBuffer:200

a=T38FaxMaxDatagram:320

a=T38FaxUdpEC:t38UDPRedundancy

Apr 14 2022 07:36:30.959 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_disconnect\_done:

 Disposition=0, Interface=0x2311DA28, Tag=0x0, Call Id=5611484,

 Call Entry(Disconnect Cause=16, Voice Class Cause Code=0, Retry Count=0)

Apr 14 2022 07:36:30.959 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_disconnect\_done:

 tg for this call is ALL\_PSTN success/fail is 1

Apr 14 2022 07:36:30.959 CDT: //5611484/7C5AEC800000/CCAPI/cc\_api\_call\_disconnect\_done:

 Call Disconnect Event Sent

Apr 14 2022 07:36:30.959 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_free\_feature\_vsa:

Apr 14 2022 07:36:30.959 CDT: :cc\_free\_feature\_vsa freeing 3E1FBFA0

Apr 14 2022 07:36:30.959 CDT: //-1/xxxxxxxxxxxx/CCAPI/cc\_free\_feature\_vsa:

Apr 14 2022 07:36:30.959 CDT: vsacount in free is 0