version 4.2(1)SV1(5.2b)
no feature telnet

username admin password 5 $1$8/7b.I/H$TUT2occn1HkUzebiUxtvC/  role network-admin

banner motd #Nexus 1000v Switch#

ssh key rsa 2048 
ip domain-lookup
ip host n1kdvs 172.31.82.36
hostname n1kdvs
errdisable recovery cause failed-port-state
snmp-server user admin network-admin auth md5 0x40562daed661c8ffaedf92fc5518bf73 priv 0x40562daed661c8ffaedf92fc5518bf73 localizedkey

vrf context management
  ip route 0.0.0.0/0 172.31.82.1
vlan 1-3
vlan 1-3

port-channel load-balance ethernet source-mac
port-profile default max-ports 32
port-profile type ethernet Unused_Or_Quarantine_Uplink
  vmware port-group
  shutdown
  description Port-group created for Nexus1000V internal usage. Do not use.
  state enabled
port-profile type vethernet Unused_Or_Quarantine_Veth
  vmware port-group
  shutdown
  description Port-group created for Nexus1000V internal usage. Do not use.
  state enabled

vdc n1kdvs id 1
  limit-resource vlan minimum 16 maximum 2049
  limit-resource monitor-session minimum 0 maximum 2
  limit-resource vrf minimum 16 maximum 8192
  limit-resource port-channel minimum 0 maximum 768
  limit-resource u4route-mem minimum 1 maximum 1
  limit-resource u6route-mem minimum 1 maximum 1
  limit-resource m4route-mem minimum 58 maximum 58
  limit-resource m6route-mem minimum 8 maximum 8

interface mgmt0
  ip address 172.31.82.36/24

interface control0
line console
boot kickstart bootflash:/nexus-1000v-kickstart.4.2.1.SV1.5.2b.bin sup-1
boot system bootflash:/nexus-1000v.4.2.1.SV1.5.2b.bin sup-1
boot kickstart bootflash:/nexus-1000v-kickstart.4.2.1.SV1.5.2b.bin sup-2
boot system bootflash:/nexus-1000v.4.2.1.SV1.5.2b.bin sup-2
svs-domain
 domain id 1
  control vlan 2
  packet vlan 3
  svs mode L2  
svs connection vcenter
  protocol vmware-vim
  remote ip address 172.31.82.35 port 80
  vmware dvs uuid "6a f9 39 50 46 1b 22 72-2a 1d 06 3c 34 ec ca 3f" datacenter-name klu.dc
  max-ports 8192
  connect
vservice global type vsg
  tcp state-checks
vnm-policy-agent
  registration-ip 0.0.0.0
  shared-secret **********
  log-level 
!!!!!!!

n1kdvs# show svs connections 

connection vcenter:
    ip address: 172.31.82.35
    remote port: 80
    protocol: vmware-vim https
    certificate: default
    datacenter name: klu.dc
    admin:   
    max-ports: 8192
    DVS uuid: 6a f9 39 50 46 1b 22 72-2a 1d 06 3c 34 ec ca 3f
    config status: Enabled
    operational status: Connected
    sync status: Complete
    version: VMware vCenter Server 5.1.0 build-947673
    vc-uuid: 2F3AC836-4076-4A67-B5FC-6EFB80A911D1
!!!!!!

n1kdvs# show svs neighbors 

Active Domain ID: 1

AIPC Interface MAC: 0050-56b9-7b5b
Inband Interface MAC: 0050-56b9-1771

Src MAC           Type   Domain-id    Node-id     Last learnt (Sec. ago)
------------------------------------------------------------------------
!!!!!!

n1kdvs# show module
Mod  Ports  Module-Type                       Model               Status
---  -----  --------------------------------  ------------------  ------------
1    0      Virtual Supervisor Module         Nexus1000V          active *

Mod  Sw                  Hw      
---  ------------------  ------------------------------------------------  
1    4.2(1)SV1(5.2b)     0.0                                              

Mod  MAC-Address(es)                         Serial-Num
---  --------------------------------------  ----------
1    00-19-07-6c-5a-a8 to 00-19-07-6c-62-a8  NA

Mod  Server-IP        Server-UUID                           Server-Name
---  ---------------  ------------------------------------  --------------------
1    172.31.82.36     NA                                    NA

* this terminal session